(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Open Pedalboard Mainboard")
		(date "2024-10-16")
		(rev "4.0.1-RC")
		(company "https://github.com/pedalboard")
		(comment 1 "Source Code: https://github.com/pedalboard/pedalboard-hw")
		(comment 2 "License: CERN Open Hardware Licence Version 2 - Permissive")
		(comment 3 "Git commit hash: ${GIT_HASH} ")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 18.005615 130.994385)
		(grid_origin 18 20)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(J25-Pin_2)")
	(net 3 "/LEDs/RGB_DATA")
	(net 4 "Net-(C30-Pad1)")
	(net 5 "Net-(C26-Pad1)")
	(net 6 "Net-(U9-XTALIN{slash}CLKIN)")
	(net 7 "+3V3")
	(net 8 "+1V1")
	(net 9 "/Audio/CM4_GPIO13")
	(net 10 "/Audio/CM4_GPIO16")
	(net 11 "/Audio/conf_i2c_sda")
	(net 12 "/Audio/conf_i2c_scl")
	(net 13 "/MIDI/EXT_MIDI_RX")
	(net 14 "/MIDI/EXT_MIDI_TX")
	(net 15 "/Audio/audio_pcm_clk")
	(net 16 "/Audio/audio_in_stereo")
	(net 17 "/MIDI/XIN")
	(net 18 "Net-(U9-XTALOUT)")
	(net 19 "/MIDI/A_EXP1")
	(net 20 "unconnected-(CM1A-Ethernet_Pair3_P-Pad3)")
	(net 21 "/MIDI/~{USB_BOOT}")
	(net 22 "unconnected-(CM1A-Ethernet_Pair1_P-Pad4)")
	(net 23 "/MIDI/SWCLK")
	(net 24 "/Power Supply/polarity_checked")
	(net 25 "/Audio/audio_pcm_fs")
	(net 26 "/Audio/audio_out_stereo")
	(net 27 "/Audio/audio_pcm_din")
	(net 28 "/Audio/audio_pcm_dout")
	(net 29 "unconnected-(CM1A-Ethernet_Pair3_N-Pad5)")
	(net 30 "unconnected-(CM1A-Ethernet_Pair1_N-Pad6)")
	(net 31 "unconnected-(CM1A-Ethernet_Pair2_N-Pad9)")
	(net 32 "unconnected-(CM1A-Ethernet_Pair0_N-Pad10)")
	(net 33 "unconnected-(CM1A-Ethernet_Pair2_P-Pad11)")
	(net 34 "unconnected-(CM1A-Ethernet_Pair0_P-Pad12)")
	(net 35 "unconnected-(CM1A-Ethernet_nLED3(3.3v)-Pad15)")
	(net 36 "unconnected-(CM1A-Ethernet_SYNC_IN(1.8v)-Pad16)")
	(net 37 "unconnected-(CM1A-Ethernet_nLED2(3.3v)-Pad17)")
	(net 38 "unconnected-(CM1A-Ethernet_SYNC_OUT(1.8v)-Pad18)")
	(net 39 "unconnected-(CM1A-Ethernet_nLED1(3.3v)-Pad19)")
	(net 40 "/MIDI/SW_D")
	(net 41 "/MIDI/SW_E")
	(net 42 "/MIDI/SW_F")
	(net 43 "/MIDI/SW_A")
	(net 44 "/MIDI/SW_B")
	(net 45 "/MIDI/SW_C")
	(net 46 "/MIDI/ROT_VOL_A")
	(net 47 "/MIDI/ROT_VOL_B")
	(net 48 "/MIDI/SW_VOL")
	(net 49 "/MIDI/ROT_GAIN_A")
	(net 50 "/MIDI/ROT_GAIN_B")
	(net 51 "/MIDI/SW_GAIN")
	(net 52 "Net-(C31-Pad1)")
	(net 53 "Net-(U6-COMP)")
	(net 54 "unconnected-(CM1A-EEPROM_nWP-Pad20)")
	(net 55 "unconnected-(CM1A-SD_CLK-Pad57)")
	(net 56 "unconnected-(CM1A-SD_DAT3-Pad61)")
	(net 57 "Net-(L3-Pad2)")
	(net 58 "Net-(U6-FB)")
	(net 59 "unconnected-(CM1A-SD_CMD-Pad62)")
	(net 60 "unconnected-(CM1A-SD_DAT0-Pad63)")
	(net 61 "unconnected-(CM1A-SD_DAT5-Pad64)")
	(net 62 "Net-(D6-A)")
	(net 63 "Net-(D7-K)")
	(net 64 "unconnected-(CM1A-SD_DAT1-Pad67)")
	(net 65 "/Audio/in_R-")
	(net 66 "/Audio/GND_in_R")
	(net 67 "/Audio/in_R+")
	(net 68 "/Audio/in_L-")
	(net 69 "/Audio/GND_in_L")
	(net 70 "/Audio/in_L+")
	(net 71 "/Audio/GND_out")
	(net 72 "unconnected-(CM1A-SD_DAT4-Pad68)")
	(net 73 "unconnected-(CM1A-SD_DAT2-Pad69)")
	(net 74 "/Power Supply/fused")
	(net 75 "+5VP")
	(net 76 "unconnected-(CM1A-SD_DAT7-Pad70)")
	(net 77 "unconnected-(CM1A-SD_DAT6-Pad72)")
	(net 78 "unconnected-(CM1A-SD_VDD_Override-Pad73)")
	(net 79 "/MIDI/SWD")
	(net 80 "/Power Supply/unfused")
	(net 81 "unconnected-(CM1A-SD_PWR_ON-Pad75)")
	(net 82 "unconnected-(CM1A-Reserved-Pad76)")
	(net 83 "unconnected-(CM1A-SCL0-Pad80)")
	(net 84 "unconnected-(CM1A-SDA0-Pad82)")
	(net 85 "unconnected-(CM1A-+1.8v_(Output)-Pad88)")
	(net 86 "unconnected-(CM1A-WiFi_nDisable-Pad89)")
	(net 87 "unconnected-(CM1A-+1.8v_(Output)-Pad90)")
	(net 88 "unconnected-(CM1A-BT_nDisable-Pad91)")
	(net 89 "unconnected-(CM1A-RUN_PG-Pad92)")
	(net 90 "unconnected-(CM1A-nRPIBOOT-Pad93)")
	(net 91 "Net-(D7-A)")
	(net 92 "unconnected-(CM1A-AnalogIP1-Pad94)")
	(net 93 "unconnected-(CM1A-AnalogIP0-Pad96)")
	(net 94 "unconnected-(CM1A-Camera_GPIO-Pad97)")
	(net 95 "/Audio/CM4_3V")
	(net 96 "/Audio/CM4_GPIO6")
	(net 97 "/Audio/CM4_GPIO12")
	(net 98 "/Audio/CM4_GPIO5")
	(net 99 "/Audio/CM4_ID_SC")
	(net 100 "/Audio/CM4_ID_SD")
	(net 101 "/Audio/CM4_GPIO7")
	(net 102 "/Audio/CM4_GPIO11")
	(net 103 "/Audio/CM4_GPIO8")
	(net 104 "/Audio/CM4_GPIO9")
	(net 105 "/Audio/CM4_GPIO25")
	(net 106 "/Audio/CM4_GPIO10")
	(net 107 "/Audio/CM4_GPIO24")
	(net 108 "/Audio/CM4_GPIO22")
	(net 109 "/Audio/CM4_GPIO23")
	(net 110 "/Audio/CM4_GPIO17")
	(net 111 "/Audio/INT_MIDI_RX")
	(net 112 "/Audio/CM4_GPIO4")
	(net 113 "/Audio/INT_MIDI_TX")
	(net 114 "unconnected-(CM1A-Global_EN-Pad99)")
	(net 115 "unconnected-(CM1B-PCIe_CLK_nREQ-Pad102)")
	(net 116 "unconnected-(CM1B-Reserved-Pad104)")
	(net 117 "unconnected-(CM1B-Reserved-Pad106)")
	(net 118 "unconnected-(CM1B-PCIe_nRST-Pad109)")
	(net 119 "unconnected-(CM1B-PCIe_CLK_P-Pad110)")
	(net 120 "unconnected-(CM1B-VDAC_COMP-Pad111)")
	(net 121 "unconnected-(CM1B-PCIe_CLK_N-Pad112)")
	(net 122 "unconnected-(CM1B-CAM1_D0_N-Pad115)")
	(net 123 "unconnected-(CM1B-PCIe_RX_P-Pad116)")
	(net 124 "unconnected-(CM1B-CAM1_D0_P-Pad117)")
	(net 125 "unconnected-(CM1B-PCIe_RX_N-Pad118)")
	(net 126 "unconnected-(CM1B-CAM1_D1_N-Pad121)")
	(net 127 "/Audio/CM4_LED_ACT")
	(net 128 "unconnected-(CM1B-PCIe_TX_P-Pad122)")
	(net 129 "unconnected-(CM1B-CAM1_D1_P-Pad123)")
	(net 130 "unconnected-(CM1B-PCIe_TX_N-Pad124)")
	(net 131 "unconnected-(CM1B-CAM1_C_N-Pad127)")
	(net 132 "unconnected-(CM1B-CAM0_D0_N-Pad128)")
	(net 133 "unconnected-(CM1B-CAM1_C_P-Pad129)")
	(net 134 "unconnected-(CM1B-CAM0_D0_P-Pad130)")
	(net 135 "unconnected-(CM1B-CAM1_D2_N-Pad133)")
	(net 136 "unconnected-(CM1B-CAM0_D1_N-Pad134)")
	(net 137 "unconnected-(CM1B-CAM1_D2_P-Pad135)")
	(net 138 "unconnected-(CM1B-CAM0_D1_P-Pad136)")
	(net 139 "unconnected-(CM1B-CAM1_D3_N-Pad139)")
	(net 140 "unconnected-(CM1B-CAM0_C_N-Pad140)")
	(net 141 "unconnected-(CM1B-CAM1_D3_P-Pad141)")
	(net 142 "unconnected-(CM1B-CAM0_C_P-Pad142)")
	(net 143 "unconnected-(CM1B-HDMI1_HOTPLUG-Pad143)")
	(net 144 "unconnected-(CM1B-HDMI1_SDA-Pad145)")
	(net 145 "unconnected-(CM1B-HDMI1_TX2_P-Pad146)")
	(net 146 "unconnected-(CM1B-HDMI1_SCL-Pad147)")
	(net 147 "unconnected-(CM1B-HDMI1_TX2_N-Pad148)")
	(net 148 "unconnected-(CM1B-HDMI1_CEC-Pad149)")
	(net 149 "unconnected-(CM1B-HDMI0_CEC-Pad151)")
	(net 150 "unconnected-(CM1B-HDMI1_TX1_P-Pad152)")
	(net 151 "unconnected-(CM1B-HDMI0_HOTPLUG-Pad153)")
	(net 152 "unconnected-(CM1B-HDMI1_TX1_N-Pad154)")
	(net 153 "unconnected-(CM1B-DSI0_D0_N-Pad157)")
	(net 154 "/MIDI/A_EXP2")
	(net 155 "unconnected-(CM1B-HDMI1_TX0_P-Pad158)")
	(net 156 "unconnected-(CM1B-DSI0_D0_P-Pad159)")
	(net 157 "unconnected-(CM1B-HDMI1_TX0_N-Pad160)")
	(net 158 "unconnected-(CM1B-DSI0_D1_N-Pad163)")
	(net 159 "unconnected-(CM1B-HDMI1_CLK_P-Pad164)")
	(net 160 "unconnected-(CM1B-DSI0_D1_P-Pad165)")
	(net 161 "unconnected-(CM1B-HDMI1_CLK_N-Pad166)")
	(net 162 "unconnected-(CM1B-DSI0_C_N-Pad169)")
	(net 163 "unconnected-(CM1B-HDMI0_TX2_P-Pad170)")
	(net 164 "unconnected-(CM1B-DSI0_C_P-Pad171)")
	(net 165 "unconnected-(CM1B-HDMI0_TX2_N-Pad172)")
	(net 166 "unconnected-(CM1B-DSI1_D0_N-Pad175)")
	(net 167 "unconnected-(CM1B-HDMI0_TX1_P-Pad176)")
	(net 168 "unconnected-(CM1B-DSI1_D0_P-Pad177)")
	(net 169 "unconnected-(CM1B-HDMI0_TX1_N-Pad178)")
	(net 170 "unconnected-(CM1B-DSI1_D1_N-Pad181)")
	(net 171 "unconnected-(CM1B-HDMI0_TX0_P-Pad182)")
	(net 172 "unconnected-(CM1B-DSI1_D1_P-Pad183)")
	(net 173 "unconnected-(CM1B-HDMI0_TX0_N-Pad184)")
	(net 174 "unconnected-(CM1B-DSI1_C_N-Pad187)")
	(net 175 "unconnected-(CM1B-HDMI0_CLK_P-Pad188)")
	(net 176 "unconnected-(CM1B-DSI1_C_P-Pad189)")
	(net 177 "unconnected-(CM1B-HDMI0_CLK_N-Pad190)")
	(net 178 "unconnected-(CM1B-DSI1_D2_N-Pad193)")
	(net 179 "unconnected-(CM1B-DSI1_D3_N-Pad194)")
	(net 180 "unconnected-(CM1B-DSI1_D2_P-Pad195)")
	(net 181 "unconnected-(CM1B-DSI1_D3_P-Pad196)")
	(net 182 "unconnected-(CM1B-HDMI0_SDA-Pad199)")
	(net 183 "unconnected-(CM1B-HDMI0_SCL-Pad200)")
	(net 184 "Net-(D1-K)")
	(net 185 "Net-(D1-A)")
	(net 186 "Net-(J25-Pin_1)")
	(net 187 "Net-(J25-Pin_3)")
	(net 188 "Net-(U6-BST)")
	(net 189 "Net-(J26-Pin_1)")
	(net 190 "Net-(U6-SS)")
	(net 191 "Net-(J26-Pin_3)")
	(net 192 "unconnected-(J8-PadSN)")
	(net 193 "unconnected-(J2-Pad1)")
	(net 194 "unconnected-(J2-Pad3)")
	(net 195 "Net-(J8-PadT)")
	(net 196 "unconnected-(J8-PadTN)")
	(net 197 "/Connectivity/VBUS")
	(net 198 "Net-(JP6-B)")
	(net 199 "unconnected-(J4-Pad1)")
	(net 200 "unconnected-(J19-PadRN)")
	(net 201 "Net-(J27-out_L)")
	(net 202 "unconnected-(J19-PadTN)")
	(net 203 "Net-(JP5-B)")
	(net 204 "Net-(JP3-A)")
	(net 205 "unconnected-(J20-PadRN)")
	(net 206 "unconnected-(J20-PadSN)")
	(net 207 "Net-(J27-out_R)")
	(net 208 "Net-(JP4-A)")
	(net 209 "unconnected-(J20-PadTN)")
	(net 210 "Net-(JP1-B)")
	(net 211 "Net-(JP2-B)")
	(net 212 "Net-(L2-Pad2)")
	(net 213 "/Audio/CM4_LED_PWR")
	(net 214 "Net-(JP6-A)")
	(net 215 "Net-(JP5-A)")
	(net 216 "Net-(L4-Pad2)")
	(net 217 "unconnected-(J4-Pad3)")
	(net 218 "Net-(U3-USB_DP)")
	(net 219 "Net-(U1-A)")
	(net 220 "/MIDI/XOUT")
	(net 221 "/MIDI/QSPI_SCLK")
	(net 222 "/MIDI/QSPI_SS")
	(net 223 "/MIDI/QSPI_SD1")
	(net 224 "/MIDI/QSPI_SD2")
	(net 225 "/MIDI/QSPI_SD0")
	(net 226 "/MIDI/QSPI_SD3")
	(net 227 "Net-(U3-USB_DM)")
	(net 228 "Net-(U3-RUN)")
	(net 229 "unconnected-(U2-NC-Pad2)")
	(net 230 "Net-(D2-A)")
	(net 231 "unconnected-(U3-GPIO12-Pad15)")
	(net 232 "unconnected-(U3-GPIO13-Pad16)")
	(net 233 "/MIDI/I2C_SCL")
	(net 234 "/MIDI/I2C_SDA")
	(net 235 "unconnected-(U3-GPIO14-Pad17)")
	(net 236 "unconnected-(U3-GPIO15-Pad18)")
	(net 237 "unconnected-(J5-PadSN)")
	(net 238 "Net-(J5-PadT)")
	(net 239 "unconnected-(J5-PadTN)")
	(net 240 "unconnected-(J7-Pad3)")
	(net 241 "unconnected-(J18-PadSN)")
	(net 242 "unconnected-(U3-GPIO22-Pad34)")
	(net 243 "/Power Supply/switch")
	(net 244 "unconnected-(U3-GPIO23-Pad35)")
	(net 245 "unconnected-(U3-GPIO26_ADC0-Pad38)")
	(net 246 "unconnected-(U3-GPIO29_ADC3-Pad41)")
	(net 247 "Net-(J28-Pin_3)")
	(net 248 "Net-(U1-Y)")
	(net 249 "Net-(U3-GPIO10)")
	(net 250 "Net-(CM1B-USB_OTG_ID)")
	(net 251 "Net-(J9-VBUS)")
	(net 252 "Net-(U9-RBIAS)")
	(net 253 "Net-(U9-SCL{slash}SMBCLK{slash}CFG_SEL0)")
	(net 254 "Net-(U9-SDA{slash}SMBDATA{slash}NON_REM1)")
	(net 255 "Net-(U9-SUSP_IND{slash}LOCAL_PWR{slash}NON_REM0)")
	(net 256 "Net-(U9-HS_IND{slash}CFG_SEL1)")
	(net 257 "Net-(U10-ILIM)")
	(net 258 "/Audio/nEXTRST")
	(net 259 "/Connectivity/nOCS1")
	(net 260 "unconnected-(U9-TEST-Pad11)")
	(net 261 "Net-(U10-EN)")
	(net 262 "unconnected-(U9-PLLFILT-Pad34)")
	(net 263 "unconnected-(U9-USBDM_DN3{slash}PRT_DIS_M3-Pad6)")
	(net 264 "unconnected-(U9-CRFILT-Pad14)")
	(net 265 "unconnected-(U9-PRTPWR2{slash}BC_EN2-Pad16)")
	(net 266 "unconnected-(U9-PRTPWR4{slash}BC_EN4-Pad20)")
	(net 267 "unconnected-(U9-USBDP_DN3{slash}PRT_DIS_P3-Pad7)")
	(net 268 "unconnected-(U9-USBDM_DN4{slash}PRT_DIS_M4-Pad8)")
	(net 269 "unconnected-(U9-PRTPWR3{slash}BC_EN3-Pad18)")
	(net 270 "unconnected-(J9-ID-Pad4)")
	(net 271 "unconnected-(U9-USBDP_DN4{slash}PRT_DIS_P4-Pad9)")
	(net 272 "/Connectivity/USB_CM_N")
	(net 273 "/Connectivity/USB_CM_P")
	(net 274 "Net-(J9-Shield)")
	(net 275 "Net-(J10-Shield)")
	(net 276 "/Connectivity/USB_OUT_N")
	(net 277 "/Connectivity/USB_OUT_P")
	(net 278 "/Connectivity/USB_RP_P")
	(net 279 "/Connectivity/USB_RP_N")
	(net 280 "/Connectivity/USB_UP_P")
	(net 281 "/Connectivity/USB_UP_N")
	(net 282 "/Connectivity/USB_D_P")
	(net 283 "/Connectivity/USB_D_N")
	(net 284 "unconnected-(U11-NC-Pad7)")
	(net 285 "unconnected-(U11-NC-Pad6)")
	(net 286 "unconnected-(U11-D1+-Pad1)")
	(net 287 "unconnected-(U11-NC-Pad10)")
	(net 288 "unconnected-(U11-NC-Pad9)")
	(net 289 "unconnected-(U11-D1--Pad2)")
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 164.76 56.86)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP3"
			(at 0.17 2.21 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 75 "+5VP")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 149.85 45.25 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at -3.06 0.41 180)
			(layer "F.SilkS")
		)
		(property "Value" "3K9"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT3K90/1760599"
			(at 297.48 89.62 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 233 "/MIDI/I2C_SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 111.89 54.81)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at -0.78 2.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2K2"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT2K20/1760345"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 249 "Net-(U3-GPIO10)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 230 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 115.75 44.27)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 -1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 47.01 42.96 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 3.16 -0.71 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965"
		(layer "F.Cu")
		(at 168 121.5)
		(descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
		(tags "mounting hole 2.7mm no annular m2.5 din965")
		(property "Reference" "H7"
			(at 0 -3.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Fiducial:Fiducial_1.5mm_Mask3mm"
		(layer "F.Cu")
		(at 20 28)
		(descr "Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening")
		(tags "fiducial")
		(property "Reference" "FID1"
			(at -0.16 2.41 0)
			(layer "F.SilkS")
		)
		(property "Value" "Fiducial"
			(at 0 2.6035 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Fiducial*")
		(sheetname "/")
		(sheetfile "pedalboard-hw.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.75)
			(clearance 0.75)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 99.4 44.46)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -1.8 -2.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "27R"
			(at 1.86 0.04 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT27R0/1712920"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 279 "/Connectivity/USB_RP_N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 227 "Net-(U3-USB_DM)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:Jack_3.5mm_CUI_SJ1-3525N_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 120 24.5 180)
		(descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
		(tags "TRS audio jack stereo horizontal")
		(property "Reference" "J3"
			(at -7 -1.7 270)
			(layer "F.SilkS")
		)
		(property "Value" "Jack 3.5mm"
			(at 0 2.5 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.cuidevices.com/product/resource/sj1-352xng.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/cui-devices/SJ1-3525NG/738690"
			(at 240 49 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(fp_text user "PCB edge"
			(at 0 3.65 180)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 180)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5 0 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu")
		)
		(pad "" np_thru_hole circle
			(at 0 -5 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu")
		)
		(pad "" np_thru_hole circle
			(at 5 0 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu")
		)
		(pad "R" thru_hole oval
			(at -5 -5 180)
			(size 1.2 2.2)
			(drill oval 0.45 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 189 "Net-(J26-Pin_1)")
			(pintype "passive")
		)
		(pad "RN" thru_hole oval
			(at -2.5 -5 180)
			(size 1.2 2.2)
			(drill oval 0.45 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 189 "Net-(J26-Pin_1)")
			(pintype "passive")
		)
		(pad "S" thru_hole oval
			(at 0 0 180)
			(size 2.2 1.2)
			(drill oval 1.4 0.45)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "T" thru_hole oval
			(at 5 -5)
			(size 1.2 2.2)
			(drill oval 0.45 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 191 "Net-(J26-Pin_3)")
			(pintype "passive")
		)
		(pad "TN" thru_hole oval
			(at 2.5 -5)
			(size 1.2 2.2)
			(drill oval 0.45 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 191 "Net-(J26-Pin_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3525N_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 99.44 39.85 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 -1.44 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 139.29 -59.59 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 139.29 -59.59 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 139.29 -59.59 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 139.29 -59.59 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 47.01 47.74 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C49"
			(at 1.66 1.71 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 155.84 47.16 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at -2.41 0.22 180)
			(layer "F.SilkS")
		)
		(property "Value" "1n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "1000 pF, 50 V"
			(at 203 -108.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B102KBANNNC/3886678"
			(at 203 -108.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Net-(U6-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1.5mm_Mask3mm"
		(layer "F.Cu")
		(at 190.005615 27.994385)
		(descr "Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening")
		(tags "fiducial")
		(property "Reference" "FID2"
			(at -0.047615 2.648215 180)
			(layer "F.SilkS")
		)
		(property "Value" "Fiducial"
			(at 0 2.6035 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Fiducial*")
		(sheetname "/")
		(sheetfile "pedalboard-hw.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.75)
			(clearance 0.75)
		)
		(embedded_fonts no)
	)
	(footprint "Symbol:OSHW-Logo_7.5x8mm_SilkScreen"
		(layer "F.Cu")
		(at 62.8 122.1)
		(descr "Open Source Hardware Logo")
		(tags "Logo OSHW")
		(property "Reference" "SYM1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Logo_Open_Hardware_Small"
			(at 0.75 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "pedalboard-hw.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 153.22 32.93)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP1"
			(at -1.03 2.91 90)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 24 "/Power Supply/polarity_checked")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 94.9375 55.85)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0.6625 1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "DNF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 222 "/MIDI/QSPI_SS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:Jack_6.35mm_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 34.4 50 180)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J8"
			(at -3 -2.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jack 6.35mm"
			(at 9.4 3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.schurter.com/en/datasheet/typ_4833.2320.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "EXP2"
			(at 68.8 100 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235"
			(at 68.8 100 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 0)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 154 "/MIDI/A_EXP2")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "S" thru_hole circle
			(at 12.7 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 192 "unconnected-(J8-PadSN)")
			(pintype "passive+no_connect")
		)
		(pad "T" thru_hole circle
			(at 0 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 195 "Net-(J8-PadT)")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 196 "unconnected-(J8-PadTN)")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
			(offset
				(xyz 16.5 -8 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Pedalboard Library:Jack_6.35mm_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 34.4 111.2 180)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J19"
			(at -3.3 -2 180)
			(layer "F.SilkS")
		)
		(property "Value" "Jack 6.35mm"
			(at 7.4 2.7 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.schurter.com/en/datasheet/typ_4833.2320.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Audio OUT Left"
			(at 68.8 222.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235"
			(at 68.8 222.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 180)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 198 "Net-(JP6-B)")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 200 "unconnected-(J19-PadRN)")
			(pintype "passive+no_connect")
		)
		(pad "S" thru_hole circle
			(at 12.7 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/Audio/GND_out")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 204 "Net-(JP3-A)")
			(pintype "passive")
		)
		(pad "T" thru_hole circle
			(at 0 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 201 "Net-(J27-out_L)")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 202 "unconnected-(J19-PadTN)")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
			(offset
				(xyz 16.5 -8 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 156.65 53.22 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at -0.18 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 209.87 -103.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 209.87 -103.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:BarrelJack_Wuerth_6941xx301002"
		(locked yes)
		(layer "F.Cu")
		(at 176.5372 30.3886 180)
		(descr "Wuerth electronics barrel jack connector (5.5mm outher diameter, inner diameter 2.05mm or 2.55mm depending on exact order number), See: http://katalog.we-online.de/em/datasheet/6941xx301002.pdf")
		(tags "connector barrel jack")
		(property "Reference" "J7"
			(at 5.36 8.46 270)
			(layer "F.SilkS")
		)
		(property "Value" "Barrel_Jack_MountingPin"
			(at 0 15.5 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/6941xx301002.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/694106301002/5047522"
			(at 358.8 60.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "BarrelJack*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 7.5 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 4.4 1.8)
			(drill oval 3.4 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 5.8 180)
			(size 4 1.8)
			(drill oval 3 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/Power Supply/unfused")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 4.8 3 270)
			(size 4 1.8)
			(drill oval 3 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 240 "unconnected-(J7-Pad3)")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/694106301002 (rev1).stp"
			(offset
				(xyz 0 -10 5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 122.89 54.05 180)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U5"
			(at 0 -4.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "NCP1117-3.3_SOT223"
			(at 0 4.5 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117I.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/diodes-incorporated/AZ1117IH-3-3TRG1/5699672"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3 180)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.15 0 180)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "2" smd roundrect
			(at 3.15 0 180)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3 180)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 139.7676 46.1366 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at -0.2824 -2.4134 270)
			(layer "F.SilkS")
		)
		(property "Value" "220R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT220R/1760238"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LEDs/")
		(sheetfile "leds.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 248 "Net-(U1-Y)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 247 "Net-(J28-Pin_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal"
		(layer "F.Cu")
		(at 175.6372 28.1986 90)
		(descr "Terminal Block Phoenix MKDS-1,5-2, 2 pins, pitch 5mm, size 10x9.8mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.farnell.com/datasheets/100425.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-2 pitch 5mm size 10x9.8mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J6"
			(at 5.5986 -6.8372 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 3.71 6.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.phoenixcontact.com/en-us/products/printed-circuit-board-terminal-mkds-15-2-1715022?type=pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/phoenix-contact/1715022/260626"
			(at 206.71 -150.29 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.096154)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/Power Supply/unfused")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 121.81 49.42 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 1.31 1.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 264.18 104.44 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 264.18 104.44 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 49.98 40.26 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 0.66 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
		(layer "F.Cu")
		(at 36.415 29.0424 180)
		(descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC-7352 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C43"
			(at -0.4318 -2.9972 0)
			(layer "F.SilkS")
		)
		(property "Value" "100u"
			(at 0 3.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://industrial.panasonic.com/cdbs/www-data/pdf/ABE0000/ABE0000C49.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Capacitor, SP-Cap, 100u, 6.3V, 15mR ESR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/panasonic-electronic-components/EEF-CX0J101R/816418"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.12 0 180)
			(size 2.07 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.120773)
			(net 197 "/Connectivity/VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.12 0 180)
			(size 2.07 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.120773)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_B3U-1000P"
		(layer "F.Cu")
		(at 124.01 44.86 90)
		(descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
		(tags "Tactile Switch")
		(property "Reference" "SW4"
			(at 0.22 -2.28 270)
			(layer "F.SilkS")
		)
		(property "Value" "Micro Button"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3u.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Reset"
			(at 168.87 -79.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/omron-electronics-inc-emc-div/B3U-1000P/1534338"
			(at 168.87 -79.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW*Omron*B3FS*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 90)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 90)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 228 "Net-(U3-RUN)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 99.4 46.36)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -2.7 0.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "27R"
			(at 1.86 0.14 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT27R0/1712920"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 278 "/Connectivity/USB_RP_P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 218 "Net-(U3-USB_DP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 58.24 43.99)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at -0.54 -1.59 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 94.8875 53.85 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 6.5875 0.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 189.775 107.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 189.775 107.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 189.775 107.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 189.775 107.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 72.991 48.1178 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "36K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 257 "Net-(U10-ILIM)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 49.549998 102.65)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP3"
			(at 0.55 -2.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "SJP"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 204 "Net-(JP3-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 26 "/Audio/audio_out_stereo")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 41.5246 24.9276 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 3.1276 0.0754 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "/Connectivity/VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_5032-2Pin_5.0x3.2mm"
		(layer "F.Cu")
		(at 66.84 48.12 -90)
		(descr "SMD Crystal SERIES SMD2520/2 http://www.icbase.com/File/PDF/HKC/HKC00061008.pdf, 5.0x3.2mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "Y1"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Crystal_Small"
			(at 0 2.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ctscorp.com/Files/DataSheets/Passives/FCP/Crystals/crystals-445-datasheet.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Two pin crystal, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/cts-frequency-controls/445C33D24M00000/3135787"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.85 0 270)
			(size 2 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U9-XTALIN{slash}CLKIN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.85 0 270)
			(size 2 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(U9-XTALOUT)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_5032-2Pin_5.0x3.2mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D"
		(layer "F.Cu")
		(at 154.779 57.4142 180)
		(descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC-7352 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
		(tags "capacitor tantalum")
		(property "Reference" "C33"
			(at 0 -3.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100u"
			(at 0 3.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://industrial.panasonic.com/cdbs/www-data/pdf/ABE0000/ABE0000C49.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Capacitor, SP-Cap, 100u, 6.3V, 15mR ESR"
			(at 208.4 -98.14 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/panasonic-electronic-components/EEF-CX0J101R/816418"
			(at 208.4 -98.14 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.12 0 180)
			(size 2.07 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.120773)
			(net 75 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.12 0 180)
			(size 2.07 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.120773)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 94.9375 51.85)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at -3.4375 -1.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 21 "/MIDI/~{USB_BOOT}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 222 "/MIDI/QSPI_SS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:Jack_6.35mm_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 34.4 91 180)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J20"
			(at -3.165 -1.9 180)
			(layer "F.SilkS")
		)
		(property "Value" "Jack 6.35mm"
			(at 9.4 3 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.schurter.com/en/datasheet/typ_4833.2320.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Audio OUT Right"
			(at 68.8 182 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235"
			(at 68.8 182 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 180)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 203 "Net-(JP5-B)")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 205 "unconnected-(J20-PadRN)")
			(pintype "passive+no_connect")
		)
		(pad "S" thru_hole circle
			(at 12.7 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/Audio/GND_out")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 206 "unconnected-(J20-PadSN)")
			(pintype "passive+no_connect")
		)
		(pad "T" thru_hole circle
			(at 0 0 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 207 "Net-(J27-out_R)")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23 180)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 209 "unconnected-(J20-PadTN)")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
			(offset
				(xyz 16.5 -8 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Pedalboard Library:Jack_6.35mm_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 175.6 94.995)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J22"
			(at -5.8 1.705 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jack 6.35mm"
			(at 5.4 13.505 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.schurter.com/en/datasheet/typ_4833.2320.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Audio IN Left"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 0)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/Audio/in_L-")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/Audio/GND_in_L")
			(pintype "passive")
		)
		(pad "S" thru_hole circle
			(at 12.7 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/Audio/GND_in_L")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 208 "Net-(JP4-A)")
			(pintype "passive")
		)
		(pad "T" thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/Audio/in_L+")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/Audio/GND_in_L")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
			(offset
				(xyz 16.5 -8 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 129.315 44.45 90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J12"
			(at 0.03 -2.57 90)
			(layer "F.SilkS")
		)
		(property "Value" "Debug"
			(at -2.7 2.64 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/MIDI/SWCLK")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/MIDI/SWD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 50.38 52.6644 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 3.2356 -0.22 270)
			(layer "F.SilkS")
		)
		(property "Value" "36K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 253 "Net-(U9-SCL{slash}SMBCLK{slash}CFG_SEL0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 159.64 47.11)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at -2.26 0.19 90)
			(layer "F.SilkS")
		)
		(property "Value" "1n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "1000 pF, 50 V"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B102KBANNNC/3886678"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "Net-(U6-COMP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 52.28 52.6744 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 3.1256 -0.12 270)
			(layer "F.SilkS")
		)
		(property "Value" "36K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 256 "Net-(U9-HS_IND{slash}CFG_SEL1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:ABM8-272-T3_ABR"
		(layer "F.Cu")
		(at 116 54.0877 90)
		(tags "ABM8-272-T3 ")
		(property "Reference" "Y2"
			(at 0.2877 2.8 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ABM8-272-T3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://abracon.com/datasheets/ABM8-272-T3.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/abracon-llc/ABM8-272-T3/22472366"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "ABM8-272-T3_ABR")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.800001 -1.1 90)
			(size 1.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/MIDI/XIN")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -0.800001 1.1 90)
			(size 1.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0.800001 1.1 90)
			(size 1.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(C26-Pad1)")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0.800001 -1.1 90)
			(size 1.1 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/ABM8-272-T3_ABR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965"
		(layer "F.Cu")
		(at 118.98 121.52)
		(descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
		(tags "mounting hole 2.7mm no annular m2.5 din965")
		(property "Reference" "H6"
			(at 3.52 -1.22 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 155.83 43.77 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "2K2"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Resistor 2.2K 1% 63mW"
			(at 199.6 -112.06 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT2K20/1760345"
			(at 199.6 -112.06 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 58 "Net-(U6-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:MIDI bites"
		(layer "F.Cu")
		(at 105.1 20.075)
		(property "Reference" "H2"
			(at 0.2 -2.175 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Midi Bites"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -25 1)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 2)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 3)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 4)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 5)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 6)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 10)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 11)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 12)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 13)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 14)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 15)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -25 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -24 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -23 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -22 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -21 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -20 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -19 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -18 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -17 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -16 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -15 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -14 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -13 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -12 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -11 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -10 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -9 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -8 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -7 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -6 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -5 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -4 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -3 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -2 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -1 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 1 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 3 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 4 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 6 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 7 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 8 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 9 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 10 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 11 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 12 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 13 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 14 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 15 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 16 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 17 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 18 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 19 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 20 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 21 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 22 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 23 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 24 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 1)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 2)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 3)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 4)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 5)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 6)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 7)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 8)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 9)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 10)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 11)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 12)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 13)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 14)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 15)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25 16)
			(size 0.6 0.6)
			(drill 0.5)
			(layers "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 116.7 57.68 180)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at -2.68 -0.01 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED Y"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/harvatek-corporation/B1701NG-20D000314U1930/16671738"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 230 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth"
		(locked yes)
		(layer "F.Cu")
		(at 105 67)
		(descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
		(tags "tact sw push 12mm")
		(property "Reference" "SW6"
			(at -4.9 -6.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "Tactile Button"
			(at 0 7.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/430172043816.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "E"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430162043826/9950802"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW*Omron*B3FS*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -3 -4 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/MIDI/SW_E")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/MIDI/SW_E")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/WE-tact-button.stp"
			(offset
				(xyz 0 0 1.75)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1.5mm_Mask3mm"
		(layer "F.Cu")
		(at 190.005615 122.994385)
		(descr "Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening")
		(tags "fiducial")
		(property "Reference" "FID4"
			(at 0.1524 -2.6416 0)
			(layer "F.SilkS")
		)
		(property "Value" "Fiducial"
			(at 0 2.6035 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Fiducial*")
		(sheetname "/")
		(sheetfile "pedalboard-hw.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.75)
			(clearance 0.75)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 154.42 29.67 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 184.09 -124.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 184.09 -124.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Supply/polarity_checked")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 169.13 53.73 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at -0.24 1.9 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 222.86 -115.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 222.86 -115.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 137.12 43.79 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at -2.41 -0.02 180)
			(layer "F.SilkS")
		)
		(property "Value" "220R"
			(at -2.675 0.15 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT220R/1760238"
			(at 144.54 -33.28 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LEDs/")
		(sheetfile "leds.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 3 "/LEDs/RGB_DATA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 219 "Net-(U1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_B3U-1000P"
		(layer "F.Cu")
		(at 91.51 53.65 90)
		(descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
		(tags "Tactile Switch")
		(property "Reference" "SW3"
			(at 0 -2.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Micro Button"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3u.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Boot"
			(at 145.16 -37.86 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/omron-electronics-inc-emc-div/B3U-1000P/1534338"
			(at 145.16 -37.86 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW*Omron*B3FS*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 90)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 90)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/MIDI/~{USB_BOOT}")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 163.21 44.13 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.36 1.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "10R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Resistor 10R 1% 63mW"
			(at 207.34 -119.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD10R0/2240197"
			(at 207.34 -119.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 243 "/Power Supply/switch")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 4 "Net-(C30-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 147.2 127.1 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP6"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "SJP"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 214 "Net-(JP6-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 198 "Net-(JP6-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965"
		(layer "F.Cu")
		(at 25 23)
		(descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
		(tags "mounting hole 2.7mm no annular m2.5 din965")
		(property "Reference" "H1"
			(at 3.5664 -1.857 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0.5 -2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "pedalboard-hw.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 160.62 53.22 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at -3.18 0.98 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 213.84 -107.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 213.84 -107.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:Jack_6.35mm_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 175.615 33.8)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J5"
			(at -5.515 1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jack 6.35mm"
			(at 3.885 13.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.schurter.com/en/datasheet/typ_4833.2320.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "EXP1"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 0)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/MIDI/A_EXP1")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "S" thru_hole circle
			(at 12.7 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 237 "unconnected-(J5-PadSN)")
			(pintype "passive+no_connect")
		)
		(pad "T" thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 238 "Net-(J5-PadT)")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 239 "unconnected-(J5-PadTN)")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
			(offset
				(xyz 16.5 -8 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 48.48 52.6644 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 3.2356 0.18 270)
			(layer "F.SilkS")
		)
		(property "Value" "36K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 254 "Net-(U9-SDA{slash}SMBDATA{slash}NON_REM1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 163.21 40.72 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0.7 1.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 203.93 -122.49 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 203.93 -122.49 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 203.93 -122.49 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(C30-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 188 "Net-(U6-BST)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 147.5 123 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP5"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "SJP"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 215 "Net-(JP5-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 203 "Net-(JP5-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 45.5082 60.132 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "2K2"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT2K20/1760345"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 250 "Net-(CM1B-USB_OTG_ID)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965"
		(layer "F.Cu")
		(at 168 63.5)
		(descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
		(tags "mounting hole 2.7mm no annular m2.5 din965")
		(property "Reference" "H4"
			(at -3.3 -1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Pedalboard Library:CP-2350"
		(locked yes)
		(layer "F.Cu")
		(at 120 22 180)
		(descr "Female <b>CONNECTOR</b><p>\n5 pins 90 deg. with shield, horizontal (DIN 41524)")
		(property "Reference" "J4"
			(at -12 -11.6 180)
			(layer "F.SilkS")
		)
		(property "Value" "DIN5"
			(at 0 5.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/18/40_c091_abd_e-75918.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5-pin DIN connector (5-pin DIN-5 stereo)"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "MIDI Out"
			(at 240 44 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/switchcraft-inc/57PC5F/275385"
			(at 240 44 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIN*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr dnp)
		(fp_text user "5"
			(at -7.9 -13.5 0)
			(layer "F.SilkS")
		)
		(fp_text user "4"
			(at 7.3 -13.5 0)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 8.4 -6.8 0)
			(layer "F.SilkS")
		)
		(fp_text user "3"
			(at -9.3 -6.9 0)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 0.5 -5.9 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole roundrect
			(at 7.5 -10 180)
			(size 2.5 2.5)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 199 "unconnected-(J4-Pad1)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 0 -10 270)
			(size 2.5 2.5)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at -7.5 -10 180)
			(size 2.5 2.5)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 217 "unconnected-(J4-Pad3)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 5 -12.5 180)
			(size 2.5 2.5)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 189 "Net-(J26-Pin_1)")
			(pintype "passive")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 45)
		)
		(pad "5" thru_hole roundrect
			(at -5 -12.5 180)
			(size 2.5 2.5)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 191 "Net-(J26-Pin_3)")
			(pintype "passive")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 45)
		)
		(pad "PE" thru_hole roundrect
			(at -2.5 0 180)
			(size 1.8 2)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.5)
			(chamfer bottom_right)
			(solder_mask_margin 0.0508)
		)
		(pad "PE1" thru_hole rect
			(at -5 0 180)
			(size 1.8 2)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0508)
		)
		(pad "PE2" thru_hole rect
			(at 5 0 180)
			(size 1.8 2)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0508)
		)
		(pad "PE@" thru_hole roundrect
			(at 2.5 0 180)
			(size 1.8 2)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.5)
			(chamfer bottom_left)
			(solder_mask_margin 0.0508)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965"
		(layer "F.Cu")
		(at 119 63.5)
		(descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
		(tags "mounting hole 2.7mm no annular m2.5 din965")
		(property "Reference" "H5"
			(at 0 -3.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 155.84 40.37 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at -0.31 1.62 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 115.47 196.21 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 115.47 196.21 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 115.47 196.21 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 190 "Net-(U6-SS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm_CircularMountingHoles"
		(locked yes)
		(layer "F.Cu")
		(at 60.25 31.5)
		(descr "Alps rotary encoder, EC12E... with switch, vertical shaft, mounting holes with circular drills, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC11/EC11E15204A3.html")
		(tags "rotary encoder")
		(property "Reference" "SW1"
			(at 2.8 -4.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "24P/R 24mm"
			(at 3.75 -4.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/PEC11R.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "VOL"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/bourns-inc/PEC11R-4225F-S0024/4499659"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RotaryEncoder*Switch*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 11.1 6.3 0)
			(layer "F.Fab")
		)
		(pad "A" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/MIDI/ROT_VOL_A")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "B" thru_hole circle
			(at 0 5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/MIDI/ROT_VOL_B")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "C" thru_hole circle
			(at 0 2.5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "MP" thru_hole circle
			(at 7.5 -3.1)
			(size 3.2 3.2)
			(drill 2.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "MP" thru_hole circle
			(at 7.5 8.1)
			(size 3.2 3.2)
			(drill 2.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "S1" thru_hole circle
			(at 14.5 5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/MIDI/SW_VOL")
			(pinfunction "S1")
			(pintype "passive")
		)
		(pad "S2" thru_hole circle
			(at 14.5 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "S2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/EC11E-05SW.STEP"
			(offset
				(xyz 7.4 -2.3 -12)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 157.8 35.69 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 2.4 0.02 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 315.6 71.38 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 315.6 71.38 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Supply/polarity_checked")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.95x4.9mm_Mask2.71x3.4mm_ThermalVias"
		(layer "F.Cu")
		(at 159.52 42.4 -90)
		(descr "SOIC, 8 Pin (http://www.ti.com/lit/ds/symlink/lm5017.pdf#page=31), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U6"
			(at -2 7.02 270)
			(layer "F.SilkS")
		)
		(property "Value" "AP64501SP-13"
			(at 0 3.4 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP64501.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/diodes-incorporated/AP64501SP-13/10419715"
			(at 117.12 201.92 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.68 -0.85 270)
			(size 1.13 1.42)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at -0.68 0.85 270)
			(size 1.13 1.42)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd rect
			(at 0 0 270)
			(size 2.71 3.4)
			(layers "F.Mask")
		)
		(pad "" smd roundrect
			(at 0.68 -0.85 270)
			(size 1.13 1.42)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "" smd roundrect
			(at 0.68 0.85 270)
			(size 1.13 1.42)
			(layers "F.Paste")
			(roundrect_rratio 0.221239)
		)
		(pad "1" smd roundrect
			(at -2.5625 -1.905 270)
			(size 1.775 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 188 "Net-(U6-BST)")
			(pinfunction "BST")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.5625 -0.635 270)
			(size 1.775 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Supply/polarity_checked")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.5625 0.635 270)
			(size 1.775 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Supply/polarity_checked")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.5625 1.905 270)
			(size 1.775 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 190 "Net-(U6-SS)")
			(pinfunction "SS")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.5625 1.905 270)
			(size 1.775 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Net-(U6-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.5625 0.635 270)
			(size 1.775 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "Net-(U6-COMP)")
			(pinfunction "COMP")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.5625 -0.635 270)
			(size 1.775 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 2.5625 -1.905 270)
			(size 1.775 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 243 "/Power Supply/switch")
			(pinfunction "SW")
			(pintype "output")
		)
		(pad "9" thru_hole circle
			(at -0.65 -1.95 270)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -0.65 -0.65 270)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -0.65 0.65 270)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -0.65 1.95 270)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0 0 270)
			(size 1.8 4.4)
			(layers "B.Cu")
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0 0 270)
			(size 2.95 4.9)
			(layers "F.Cu")
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0.65 -1.95 270)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0.65 -0.65 270)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0.65 0.65 270)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0.65 1.95 270)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/SO-8EP.STP"
			(offset
				(xyz 0 0 0.9)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 94.9112 49.8958 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0.2112 1.7958 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0.25 -1.64 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 138.39 -51.89 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 138.39 -51.89 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 138.39 -51.89 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 138.39 -51.89 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 39.5646 24.9276 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 3.1276 0.0354 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "/Connectivity/VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 42.8666 59.2176 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "2K2"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT2K20/1760345"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 250 "Net-(CM1B-USB_OTG_ID)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 251 "Net-(J9-VBUS)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 81.5466 40.9964 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 2.396 -0.0382 0)
			(layer "F.SilkS")
		)
		(property "Value" "220R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT220R/1760238"
			(at 170.58 79.96 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 216 "Net-(L4-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 184 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 103.35 52.7 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 3.31 -0.03 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 -1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 50.75 156.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 50.75 156.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 50.75 156.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 50.75 156.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 73.0926 51.877 90)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U10"
			(at 1.4478 -2.6162 90)
			(layer "F.SilkS")
		)
		(property "Value" "AP2553W6"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP255x.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field4" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" "AP2553W6-7DICT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/AP2553W6-7/AP2553W6-7DICT-ND/3882112"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 261 "Net-(U10-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "/Connectivity/nOCS1")
			(pinfunction "nFault")
			(pintype "open_collector")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 257 "Net-(U10-ILIM)")
			(pinfunction "ILIM")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "/Connectivity/VBUS")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965"
		(layer "F.Cu")
		(at 168 128)
		(descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
		(tags "mounting hole 2.7mm no annular m2.5 din965")
		(property "Reference" "H15"
			(at -4.013815 2.038415 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "pedalboard-hw.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 60.7 47.98)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0.1 2.02 0)
			(layer "F.SilkS")
		)
		(property "Value" "36K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 255 "Net-(U9-SUSP_IND{slash}LOCAL_PWR{slash}NON_REM0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 27.75 59.65)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at 1.4 -1.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "1n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "1000 pF, 50 V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B102KBANNNC/3886678"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 274 "Net-(J9-Shield)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:SO08-E3"
		(layer "F.Cu")
		(at 159.86 28.16)
		(descr "SMALL OUTLINE INTEGRATED CIRCUIT body 3.9 mm/JEDEC MS-012AA (combined pins variation)")
		(property "Reference" "Q1"
			(at -3.684205 -0.635205 180)
			(layer "F.SilkS")
		)
		(property "Value" "FDS4435BZ"
			(at 0.623003 -0.089 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/fds4435bz_f085-d.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/onsemi/FDS4435BZ/1305763"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(pad "1-3" smd rect
			(at -0.635 2.6 180)
			(size 3.15 2.2)
			(layers "F.Cu" "F.Paste")
			(net 24 "/Power Supply/polarity_checked")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.905 2.6)
			(size 0.6 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5-8" smd rect
			(at 0 -2.6 180)
			(size 4.4 2.2)
			(layers "F.Cu" "F.Paste")
			(net 74 "/Power Supply/fused")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 116.7 51.3877)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 2.4 -0.1877 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 220 "/MIDI/XOUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 5 "Net-(C26-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 57.7 32.75 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C51"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "1n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "1000 pF, 50 V"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B102KBANNNC/3886678"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 275 "Net-(J10-Shield)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 77.8 32.2 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 45.6 110 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 45.6 110 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 45.6 110 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 45.6 110 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(J25-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 161.23 33.73)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.21 -0.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Supply/polarity_checked")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 107.225 81.3 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J16"
			(at 0.61 -3.355 90)
			(layer "F.SilkS")
		)
		(property "Value" "Debug"
			(at 2.2 2.725 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "/Audio/INT_MIDI_TX")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "/Audio/INT_MIDI_RX")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 164.83 30.73 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.64 -0.02 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 329.66 61.46 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 329.66 61.46 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/Power Supply/fused")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:Jack_6.35mm_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 175.6 74.78)
		(descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
		(tags "neutrik jack m")
		(property "Reference" "J18"
			(at -5.5 -0.48 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jack 6.35mm"
			(at 4.9 14.22 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.schurter.com/en/datasheet/typ_4833.2320.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Audio IN Right"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.35 8.115 0)
			(layer "F.Fab")
		)
		(pad "R" thru_hole circle
			(at 6.35 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "/Audio/in_R-")
			(pintype "passive")
		)
		(pad "RN" thru_hole circle
			(at 6.35 16.23)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/Audio/GND_in_R")
			(pintype "passive")
		)
		(pad "S" thru_hole circle
			(at 12.7 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/Audio/GND_in_R")
			(pintype "passive")
		)
		(pad "SN" thru_hole circle
			(at 12.7 16.23)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 241 "unconnected-(J18-PadSN)")
			(pintype "passive+no_connect")
		)
		(pad "T" thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "/Audio/in_R+")
			(pintype "passive")
		)
		(pad "TN" thru_hole circle
			(at 0 16.23)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/Audio/GND_in_R")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
			(offset
				(xyz 16.5 -8 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 164.17 24.03 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 188.2 -140.14 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 188.2 -140.14 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/Power Supply/fused")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:USB_Micro-B_Amphenol_10103594-0001LF_Horizontal"
		(layer "F.Cu")
		(at 20.67 56.5 -90)
		(descr "Micro USB Type B 10103594-0001LF, http://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10103594.pdf")
		(tags "USB USB_B USB_micro USB_OTG")
		(property "Reference" "J9"
			(at -3.3 -3.98 0)
			(layer "F.SilkS")
		)
		(property "Value" "USB_OTG"
			(at -0.025 4.435 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/10103594.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB mini/micro connector"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/amphenol-cs-fci/10103594-0001LF/2350351"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "PCB edge"
			(at -0.025 2.235 270)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at -0.025 -0.015 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.325 -1.765)
			(size 1.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 251 "Net-(J9-VBUS)")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.675 -1.765)
			(size 1.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 283 "/Connectivity/USB_D_N")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -0.025 -1.765)
			(size 1.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 282 "/Connectivity/USB_D_P")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at 0.625 -1.765)
			(size 1.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 270 "unconnected-(J9-ID-Pad4)")
			(pinfunction "ID")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at 1.275 -1.765)
			(size 1.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.975 -0.565 270)
			(size 1.825 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.875 -1.865 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.755 0.185 270)
			(size 1.35 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -2.755 1.115)
			(size 1.7 1.35)
			(drill oval 1.2 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -2.445 -1.885)
			(size 1.5 1.1)
			(drill oval 1.05 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -0.985 1.385)
			(size 2.5 1.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.935 1.385)
			(size 2.5 1.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.395 -1.885)
			(size 1.5 1.1)
			(drill oval 1.05 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.705 1.115)
			(size 1.7 1.35)
			(drill oval 1.2 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.725 0.185 270)
			(size 1.35 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.875 -1.885 270)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.975 -0.565 270)
			(size 1.825 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "Net-(J9-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/10103594-0001LF--3DModel-STEP-269445.STEP"
			(offset
				(xyz 0 -1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 158.63 53.23 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at -3.17 1.47 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 211.86 -105.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 211.86 -105.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 54.35 36.25 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 3.3698 0.0448 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "/Connectivity/VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 168.9 115 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP4"
			(at 0 -2.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "SJP"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 208 "Net-(JP4-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 16 "/Audio/audio_in_stereo")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth"
		(locked yes)
		(layer "F.Cu")
		(at 30 67)
		(descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
		(tags "tact sw push 12mm")
		(property "Reference" "SW5"
			(at 4.5 -6.95 0)
			(layer "F.SilkS")
		)
		(property "Value" "Tactile Button"
			(at 0 7.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/430172043816.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430162043826/9950802"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW*Omron*B3FS*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.04 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "/MIDI/SW_D")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "/MIDI/SW_D")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/WE-tact-button.stp"
			(offset
				(xyz 0 0 1.75)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm"
		(layer "F.Cu")
		(at 52.19 45.96 -90)
		(descr "QFN, 36 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/36L_QFN_6x6_with_3_7x3_7_EP_Punch_Dimpled_4E_C04-0241A.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U9"
			(at 2.54 -4.61 180)
			(layer "F.SilkS")
		)
		(property "Value" "USB2514B_Bi"
			(at 0 4.3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00001692C.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB 2.0 Hi-Speed Hub Controller"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/microchip-technology/USB2514B-I-M2/5639468"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*6x6mm*P0.5mm*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -1.23 -1.23 270)
			(size 0.99 0.99)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1.23 0 270)
			(size 0.99 0.99)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -1.23 1.23 270)
			(size 0.99 0.99)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 -1.23 270)
			(size 0.99 0.99)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0 270)
			(size 0.99 0.99)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 1.23 270)
			(size 0.99 0.99)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.23 -1.23 270)
			(size 0.99 0.99)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.23 0 270)
			(size 0.99 0.99)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 1.23 1.23 270)
			(size 0.99 0.99)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -2.9375 -2 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 279 "/Connectivity/USB_RP_N")
			(pinfunction "USBDM_DN1/PRT_DIS_M1")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -2.9375 -1.5 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 278 "/Connectivity/USB_RP_P")
			(pinfunction "USBDP_DN1/PRT_DIS_P1")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.9375 -1 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 276 "/Connectivity/USB_OUT_N")
			(pinfunction "USBDM_DN2/PRT_DIS_M2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.9375 -0.5 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 277 "/Connectivity/USB_OUT_P")
			(pinfunction "USBDP_DN2/PRT_DIS_P2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.9375 0 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pinfunction "VDDA33")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -2.9375 0.5 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 263 "unconnected-(U9-USBDM_DN3{slash}PRT_DIS_M3-Pad6)")
			(pinfunction "USBDM_DN3/PRT_DIS_M3")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" smd roundrect
			(at -2.9375 1 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 267 "unconnected-(U9-USBDP_DN3{slash}PRT_DIS_P3-Pad7)")
			(pinfunction "USBDP_DN3/PRT_DIS_P3")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" smd roundrect
			(at -2.9375 1.5 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 268 "unconnected-(U9-USBDM_DN4{slash}PRT_DIS_M4-Pad8)")
			(pinfunction "USBDM_DN4/PRT_DIS_M4")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" smd roundrect
			(at -2.9375 2 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 271 "unconnected-(U9-USBDP_DN4{slash}PRT_DIS_P4-Pad9)")
			(pinfunction "USBDP_DN4/PRT_DIS_P4")
			(pintype "bidirectional+no_connect")
		)
		(pad "10" smd roundrect
			(at -2 2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pinfunction "VDDA33")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -1.5 2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 260 "unconnected-(U9-TEST-Pad11)")
			(pinfunction "TEST")
			(pintype "input+no_connect")
		)
		(pad "12" smd roundrect
			(at -1 2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 261 "Net-(U10-EN)")
			(pinfunction "PRTPWR1/BC_EN1")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -0.5 2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "/Connectivity/nOCS1")
			(pinfunction "OCS_N1")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 0 2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 264 "unconnected-(U9-CRFILT-Pad14)")
			(pinfunction "CRFILT")
			(pintype "input+no_connect")
		)
		(pad "15" smd roundrect
			(at 0.5 2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pinfunction "VDD33")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at 1 2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 265 "unconnected-(U9-PRTPWR2{slash}BC_EN2-Pad16)")
			(pinfunction "PRTPWR2/BC_EN2")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" smd roundrect
			(at 1.5 2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "/Connectivity/nOCS1")
			(pinfunction "OCS_N2")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 2 2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 269 "unconnected-(U9-PRTPWR3{slash}BC_EN3-Pad18)")
			(pinfunction "PRTPWR3/BC_EN3")
			(pintype "bidirectional+no_connect")
		)
		(pad "19" smd roundrect
			(at 2.9375 2 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "/Connectivity/nOCS1")
			(pinfunction "OCS_N3")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 2.9375 1.5 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 266 "unconnected-(U9-PRTPWR4{slash}BC_EN4-Pad20)")
			(pinfunction "PRTPWR4/BC_EN4")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" smd roundrect
			(at 2.9375 1 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "/Connectivity/nOCS1")
			(pinfunction "OCS_N4")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 2.9375 0.5 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 254 "Net-(U9-SDA{slash}SMBDATA{slash}NON_REM1)")
			(pinfunction "SDA/SMBDATA/NON_REM1")
			(pintype "bidirectional")
		)
		(pad "23" smd roundrect
			(at 2.9375 0 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pinfunction "VDD33")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 2.9375 -0.5 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 253 "Net-(U9-SCL{slash}SMBCLK{slash}CFG_SEL0)")
			(pinfunction "SCL/SMBCLK/CFG_SEL0")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at 2.9375 -1 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 256 "Net-(U9-HS_IND{slash}CFG_SEL1)")
			(pinfunction "HS_IND/CFG_SEL1")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at 2.9375 -1.5 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 258 "/Audio/nEXTRST")
			(pinfunction "RESET_N")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 2.9375 -2 270)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pinfunction "VBUS_DET")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 2 -2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 255 "Net-(U9-SUSP_IND{slash}LOCAL_PWR{slash}NON_REM0)")
			(pinfunction "SUSP_IND/LOCAL_PWR/NON_REM0")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at 1.5 -2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pinfunction "VDDA33")
			(pintype "power_in")
		)
		(pad "30" smd roundrect
			(at 1 -2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 281 "/Connectivity/USB_UP_N")
			(pinfunction "USBDM_UP")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at 0.5 -2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 280 "/Connectivity/USB_UP_P")
			(pinfunction "USBDP_UP")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at 0 -2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U9-XTALOUT)")
			(pinfunction "XTALOUT")
			(pintype "output")
		)
		(pad "33" smd roundrect
			(at -0.5 -2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U9-XTALIN{slash}CLKIN)")
			(pinfunction "XTALIN/CLKIN")
			(pintype "input")
		)
		(pad "34" smd roundrect
			(at -1 -2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 262 "unconnected-(U9-PLLFILT-Pad34)")
			(pinfunction "PLLFILT")
			(pintype "input+no_connect")
		)
		(pad "35" smd roundrect
			(at -1.5 -2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 252 "Net-(U9-RBIAS)")
			(pinfunction "RBIAS")
			(pintype "input")
		)
		(pad "36" smd roundrect
			(at -2 -2.9375 270)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pinfunction "VDDA33")
			(pintype "power_in")
		)
		(pad "37" smd rect
			(at 0 0 270)
			(size 3.7 3.7)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-6L_10x3.84mm_P1.27mm"
		(layer "F.Cu")
		(at 90.4616 39.2714)
		(descr "6-pin plasic small outline 7,5mm long https://toshiba.semicon-storage.com/info/docget.jsp?did=53548&prodName=TLP2770")
		(tags "SO-6L")
		(property "Reference" "U2"
			(at -4.7616 3.1286 90)
			(layer "F.SilkS")
		)
		(property "Value" "TLP2761"
			(at 0.1 3.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=28819&prodName=TLP2761"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "15-Mbps inverting photocouple,5 kVrms, 2.7 - 5.5 Vdd, push-pull output"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/toshiba-semiconductor-and-storage/TLP2761-TP-E/7809713"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SO*6L*10x3.84mm*P1.27mm*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.75 -1.27 90)
			(size 0.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 184 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.75 0 90)
			(size 0.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 229 "unconnected-(U2-NC-Pad2)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "3" smd rect
			(at -4.75 1.27 90)
			(size 0.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 185 "Net-(D1-A)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 4.75 1.27 90)
			(size 0.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 4.75 0 90)
			(size 0.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/MIDI/EXT_MIDI_RX")
			(pinfunction "VO")
			(pintype "output")
		)
		(pad "6" smd rect
			(at 4.75 -1.27 90)
			(size 0.8 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SO-6L_10x3.84mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-10_3x3mm_P0.5mm"
		(layer "F.Cu")
		(at 56.12 57.11 180)
		(descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
		(tags "SSOP 0.5")
		(property "Reference" "U8"
			(at 2.02 -2.49 180)
			(layer "F.SilkS")
		)
		(property "Value" "FSUSB42MUX"
			(at 0 2.55 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSUSB42-D.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low-Power, Two-Port, High-Speed, USB2.0 (480Mbps) or UART Switch, MSOP-10"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/onsemi/FSUSB42MUX/2036916"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MSOP*3x3mm*P0.5mm*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.15 -1 180)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "/Audio/CM4_3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -2.15 -0.5 180)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 250 "Net-(CM1B-USB_OTG_ID)")
			(pinfunction "SEL")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.15 0 180)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 273 "/Connectivity/USB_CM_P")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -2.15 0.5 180)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 272 "/Connectivity/USB_CM_N")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -2.15 1 180)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at 2.15 1 180)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 281 "/Connectivity/USB_UP_N")
			(pinfunction "HSD1-")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at 2.15 0.5 180)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 280 "/Connectivity/USB_UP_P")
			(pinfunction "HSD1+")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 2.15 0 180)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 283 "/Connectivity/USB_D_N")
			(pinfunction "HSD2-")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at 2.15 -0.5 180)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 282 "/Connectivity/USB_D_P")
			(pinfunction "HSD2+")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 2.15 -1 180)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 93.209 42.3914 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -2.591 -1.2086 0)
			(layer "F.SilkS")
		)
		(property "Value" "33R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT33R0/1760586"
			(at 135.47 -25.79 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 57 "Net-(L3-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 109.04 77.7025 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 2.9025 0.16 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at -2.55 0.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 62 "Net-(D6-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 95 "/Audio/CM4_3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 96.8 75.5 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP2"
			(at 2.97 0.03 90)
			(layer "F.SilkS")
		)
		(property "Value" "SJP"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 111 "/Audio/INT_MIDI_RX")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 211 "Net-(JP2-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 94.3 75.5 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 3.08 0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "SJP"
			(at 0 -1.3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 113 "/Audio/INT_MIDI_TX")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 210 "Net-(JP1-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 60.97 44.62 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at -1.38 -2.37 180)
			(layer "F.SilkS")
		)
		(property "Value" "12K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 252 "Net-(U9-RBIAS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:RP2040-QFN-56"
		(layer "F.Cu")
		(at 107.4 45.6 90)
		(descr "QFN, 56 Pin (http://www.cypress.com/file/416486/download#page=40), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
		(tags "QFN DFN_QFN")
		(property "Reference" "U3"
			(at -5.11 -1.24 180)
			(layer "F.SilkS")
		)
		(property "Value" "RP2040"
			(at 4.1 2.1 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/rp2040/rp2040-datasheet.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/raspberry-pi/SC0914-13/14306010"
			(at 153 -61.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(solder_paste_margin_ratio -0.1)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.6375 -0.6375 90)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "" smd roundrect
			(at -0.6375 0.6375 90)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "" smd roundrect
			(at 0.6375 -0.6375 90)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "" smd roundrect
			(at 0.6375 0.6375 90)
			(size 1.084435 1.084435)
			(layers "F.Paste")
			(roundrect_rratio 0.230535)
		)
		(pad "1" smd roundrect
			(at -3.4375 -2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.4375 -2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/MIDI/EXT_MIDI_TX")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -3.4375 -1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/MIDI/EXT_MIDI_RX")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -3.4375 -1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/MIDI/SW_C")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -3.4375 -1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/MIDI/SW_F")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -3.4375 -0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/MIDI/SW_E")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -3.4375 -0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/MIDI/SW_B")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -3.4375 0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/MIDI/SW_A")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -3.4375 0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/MIDI/SW_D")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -3.4375 1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -3.4375 1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 211 "Net-(JP2-B)")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -3.4375 1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 210 "Net-(JP1-B)")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -3.4375 2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 249 "Net-(U3-GPIO10)")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -3.4375 2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/LEDs/RGB_DATA")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -2.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 231 "unconnected-(U3-GPIO12-Pad15)")
			(pinfunction "GPIO12")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" smd roundrect
			(at -2.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 232 "unconnected-(U3-GPIO13-Pad16)")
			(pinfunction "GPIO13")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" smd roundrect
			(at -1.8 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 235 "unconnected-(U3-GPIO14-Pad17)")
			(pinfunction "GPIO14")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" smd roundrect
			(at -1.4 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 236 "unconnected-(U3-GPIO15-Pad18)")
			(pinfunction "GPIO15")
			(pintype "bidirectional+no_connect")
		)
		(pad "19" smd roundrect
			(at -1 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "TESTEN")
			(pintype "passive")
		)
		(pad "20" smd roundrect
			(at -0.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/MIDI/XIN")
			(pinfunction "XIN")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -0.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 220 "/MIDI/XOUT")
			(pinfunction "XOUT")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at 0.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "23" smd roundrect
			(at 0.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 1 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/MIDI/SWCLK")
			(pinfunction "SWCLK")
			(pintype "output")
		)
		(pad "25" smd roundrect
			(at 1.4 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "/MIDI/SWD")
			(pinfunction "SWD")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at 1.8 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 228 "Net-(U3-RUN)")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 2.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/MIDI/ROT_VOL_A")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "28" smd roundrect
			(at 2.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/MIDI/ROT_VOL_B")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at 3.4375 2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/MIDI/SW_VOL")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at 3.4375 2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/MIDI/ROT_GAIN_A")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at 3.4375 1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/MIDI/ROT_GAIN_B")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at 3.4375 1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/MIDI/SW_GAIN")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at 3.4375 1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "34" smd roundrect
			(at 3.4375 0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 242 "unconnected-(U3-GPIO22-Pad34)")
			(pinfunction "GPIO22")
			(pintype "bidirectional+no_connect")
		)
		(pad "35" smd roundrect
			(at 3.4375 0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 244 "unconnected-(U3-GPIO23-Pad35)")
			(pinfunction "GPIO23")
			(pintype "bidirectional+no_connect")
		)
		(pad "36" smd roundrect
			(at 3.4375 -0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 234 "/MIDI/I2C_SDA")
			(pinfunction "GPIO24")
			(pintype "bidirectional")
		)
		(pad "37" smd roundrect
			(at 3.4375 -0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 233 "/MIDI/I2C_SCL")
			(pinfunction "GPIO25")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at 3.4375 -1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 245 "unconnected-(U3-GPIO26_ADC0-Pad38)")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional+no_connect")
		)
		(pad "39" smd roundrect
			(at 3.4375 -1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "/MIDI/A_EXP2")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at 3.4375 -1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/MIDI/A_EXP1")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at 3.4375 -2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 246 "unconnected-(U3-GPIO29_ADC3-Pad41)")
			(pinfunction "GPIO29_ADC3")
			(pintype "bidirectional+no_connect")
		)
		(pad "42" smd roundrect
			(at 3.4375 -2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "43" smd roundrect
			(at 2.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "ADC_AVDD")
			(pintype "power_in")
		)
		(pad "44" smd roundrect
			(at 2.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "VREG_IN")
			(pintype "power_in")
		)
		(pad "45" smd roundrect
			(at 1.8 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pinfunction "VREG_VOUT")
			(pintype "power_out")
		)
		(pad "46" smd roundrect
			(at 1.4 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 227 "Net-(U3-USB_DM)")
			(pinfunction "USB_DM")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 1 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 218 "Net-(U3-USB_DP)")
			(pinfunction "USB_DP")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at 0.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "USB_VDD")
			(pintype "power_in")
		)
		(pad "49" smd roundrect
			(at 0.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "50" smd roundrect
			(at -0.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at -0.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 226 "/MIDI/QSPI_SD3")
			(pinfunction "QSPI_SD3")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at -1 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 221 "/MIDI/QSPI_SCLK")
			(pinfunction "QSPI_SCLK")
			(pintype "output")
		)
		(pad "53" smd roundrect
			(at -1.4 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 225 "/MIDI/QSPI_SD0")
			(pinfunction "QSPI_SD0")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at -1.8 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/MIDI/QSPI_SD2")
			(pinfunction "QSPI_SD2")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at -2.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/MIDI/QSPI_SD1")
			(pinfunction "QSPI_SD1")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at -2.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 222 "/MIDI/QSPI_SS")
			(pinfunction "QSPI_SS")
			(pintype "bidirectional")
		)
		(pad "57" thru_hole circle
			(at -1.275 -1.275 90)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at -1.275 0 90)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at -1.275 1.275 90)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 0 -1.275 90)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 0 0 90)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" smd roundrect
			(at 0 0 90)
			(size 3.2 3.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.045)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 0 1.275 90)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 1.275 -1.275 90)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 1.275 0 90)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" thru_hole circle
			(at 1.275 1.275 90)
			(size 0.6 0.6)
			(drill 0.35)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 51.52 60.3 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 0.42 -1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 105.09 77.7525 -90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D7"
			(at -2.6525 -0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED R"
			(at 3.5 2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/harvatek-corporation/B1701URO-20D000114U1930/16671739"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "Net-(D7-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "Net-(D7-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 69.6382 52.9438 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 125.23 49.45 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at -3.12 0.01 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 3 0.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 271.02 104.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 271.02 104.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 161.21 35.71)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 2.17 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Supply/polarity_checked")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 149.75 42.95 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at -3.12 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "3K9"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT3K90/1760599"
			(at 295.96 85.78 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 234 "/MIDI/I2C_SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 153.91 47.13 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at -2.44 -0.57 180)
			(layer "F.SilkS")
		)
		(property "Value" "12K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Resistor 12K 1% 63mW"
			(at 201.04 -106.78 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 75 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 58 "Net-(U6-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 108.74 39.46)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 3.39 -0.02 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at -0.95 -1.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 93.209 44.2914)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.591 0.9086 0)
			(layer "F.SilkS")
		)
		(property "Value" "10R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Resistor 10R 1% 63mW"
			(at 23.89 133.57 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD10R0/2240197"
			(at 23.89 133.57 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 212 "Net-(L2-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 14 "/MIDI/EXT_MIDI_TX")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 79.8216 41.1964 -90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L4"
			(at -2.6214 -0.0104 0)
			(layer "F.SilkS")
		)
		(property "Value" "120_100MHz"
			(at 2.5 1.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8796738650142/ENFA0003.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/murata-electronics/BLM18KG121TN1D/1982762"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 186 "Net-(J25-Pin_1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 216 "Net-(L4-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123F"
		(layer "F.Cu")
		(at 83.6616 41.9214 -90)
		(descr "D_SOD-123F")
		(tags "D_SOD-123F")
		(property "Reference" "D1"
			(at -3.0416 0.045 0)
			(layer "F.SilkS")
		)
		(property "Value" "SM4007"
			(at -0.9 -1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.mccsemi.com/pdf/Products/SM4001PL-SM4007PL(SOD-123FL).PDF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/micro-commercial-co/SM4007PL-TP/1793250"
			(at 167.5 87.08 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 1.4 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 270)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2272727273)
			(net 184 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 270)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2272727273)
			(net 185 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_A_Molex_67643_Horizontal"
		(layer "F.Cu")
		(at 53.08 31.75 180)
		(descr "USB type A, Horizontal, https://www.molex.com/pdm_docs/sd/676433910_sd.pdf")
		(tags "USB_A Female Connector receptacle")
		(property "Reference" "J10"
			(at 7.18 -3.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "USB_A"
			(at 3.5 14.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.molex.com/en-us/products/part-detail/676433910?display=pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB Type A connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/molex/0676433910/3598521"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.5 3.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.5)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 197 "/Connectivity/VBUS")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 276 "/Connectivity/USB_OUT_N")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at 4.5 0 180)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 277 "/Connectivity/USB_OUT_P")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at 7 0 180)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" thru_hole circle
			(at -3.07 2.71 180)
			(size 3 3)
			(drill 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 275 "Net-(J10-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 10.07 2.71 180)
			(size 3 3)
			(drill 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 275 "Net-(J10-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_Molex_67643_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 102.19 38.54 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at -3.35 0.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 204.38 77.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 204.38 77.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 204.38 77.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 204.38 77.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.19 0.04 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 151.1976 23.7338 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 -1.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 238 "Net-(J5-PadT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 81.0216 43.4214)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at -0.199 1.402 0)
			(layer "F.SilkS")
		)
		(property "Value" "120_100MHz"
			(at -5.75 -1.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8796738650142/ENFA0003.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/murata-electronics/BLM18KG121TN1D/1982762"
			(at 164.5 83.32 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 187 "Net-(J25-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 185 "Net-(D1-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 113.2 51.3877 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 1 -2.9 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "15p"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.seielect.com/Catalog/SEI-CML.PDF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "50V/5%"
			(at 226.4 105 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/CML0805C0G150JT50V/10660046"
			(at 226.4 105 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/MIDI/XIN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_1812_4532Metric"
		(layer "F.Cu")
		(at 166.07 27.71 180)
		(descr "Fuse SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.nikhef.nl/pub/departments/mt/projects/detectorR_D/dtddice/ERJ2G.pdf), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at -0.73 2.71 180)
			(layer "F.SilkS")
		)
		(property "Value" "Polyfuse 1.8A"
			(at -1.43 3.21 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/resettable_ptcs/littelfuse_ptc_1812l_datasheet.pdf.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/littelfuse-inc/1812L150-24MR/2023969"
			(at 332.14 55.42 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*polyfuse* *PTC*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1375 0 180)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 80 "/Power Supply/unfused")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1375 0 180)
			(size 1.125 3.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 74 "/Power Supply/fused")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1812_4532Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:JST_PH_B3B-PH-SM4-TB_1x03-1MP_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 137.3 52.8 90)
		(descr "JST PH series connector, B3B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH vertical")
		(property "Reference" "J28"
			(at 0 -5.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "JST PH 3"
			(at 0 4.45 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/jst-sales-america-inc/B3B-PH-SM4-TB/926832"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/LEDs/")
		(sheetfile "leds.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0.5 90)
			(size 1 5.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 0.5 90)
			(size 1 5.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 2 0.5 90)
			(size 1 5.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 247 "Net-(J28-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -4.4 -1.75 90)
			(size 1.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
		)
		(pad "MP" smd roundrect
			(at 4.4 -1.75 90)
			(size 1.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/B3B-PH-SM4-TB(LF)(SN)--3DModel-STEP-269445.STEP"
			(offset
				(xyz 0 1.75 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -180)
			)
		)
	)
	(footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth"
		(locked yes)
		(layer "F.Cu")
		(at 180 119)
		(descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
		(tags "tact sw push 12mm")
		(property "Reference" "SW10"
			(at -4.8 7.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "Tactile Button"
			(at 0 7.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/430172043816.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "C"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430162043826/9950802"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW*Omron*B3FS*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -4.5 -4.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/MIDI/SW_C")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/MIDI/SW_C")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/WE-tact-button.stp"
			(offset
				(xyz 0 0 1.75)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:SOIC-8_5.23x5.23mm_P1.27mm"
		(layer "F.Cu")
		(at 99.5 52.45 90)
		(descr "SOIC, 8 Pin (http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf#page=68), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U4"
			(at -5.53 1.31 180)
			(layer "F.SilkS")
		)
		(property "Value" "W25Q128JVS"
			(at -3.55 2.5 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25q128jv%20revf%2003272018%20plus.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/winbond-electronics/W25Q128JVSIQ-TR/5803944"
			(at 151.95 -47.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*5.23x5.23mm*P1.27mm*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.6 -1.905 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 222 "/MIDI/QSPI_SS")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.6 -0.635 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/MIDI/QSPI_SD1")
			(pinfunction "DO(IO1)")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -3.6 0.635 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/MIDI/QSPI_SD2")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -3.6 1.905 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 3.6 1.905 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 225 "/MIDI/QSPI_SD0")
			(pinfunction "DI(IO0)")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 3.6 0.635 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 221 "/MIDI/QSPI_SCLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 3.6 -0.635 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 226 "/MIDI/QSPI_SD3")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 3.6 -1.905 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/SOIC_128JVSIQ_WIN.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 55.03 51.44 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at -0.04 -1.77 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:Raspberry-Pi-4-Compute-Module"
		(layer "F.Cu")
		(at 89 63.5 180)
		(descr "Raspberry Pi 4 Compute Module")
		(tags "Raspberry Pi 4 Compute Module")
		(property "Reference" "CM1"
			(at 33 -53.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "CM4"
			(at 16.52 0.19 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.hirose.com/en/product/document?clcode=&productname=&series=DF40&documenttype=Catalog&lang=en&documentid=en_DF40_CAT"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "DF40C-100DS-0.4V(51)"
			(at 178 127 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/hirose-electric-co-ltd/DF40C-100DS-0-4V-51/1969476"
			(at 178 127 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(solder_paste_margin_ratio -0.1)
		(attr smd)
		(pad "" np_thru_hole circle
			(at 0 -48 180)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "" np_thru_hole circle
			(at 33 -48 180)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "" np_thru_hole circle
			(at 33 0 180)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "1" smd rect
			(at -2 -31.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at 1.08 -31.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -2 -30.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(CM1A-Ethernet_Pair3_P-Pad3)")
			(pinfunction "Ethernet_Pair3_P")
			(pintype "passive+no_connect")
		)
		(pad "4" smd rect
			(at 1.08 -30.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(CM1A-Ethernet_Pair1_P-Pad4)")
			(pinfunction "Ethernet_Pair1_P")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at -2 -30.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "unconnected-(CM1A-Ethernet_Pair3_N-Pad5)")
			(pinfunction "Ethernet_Pair3_N")
			(pintype "passive+no_connect")
		)
		(pad "6" smd rect
			(at 1.08 -30.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(CM1A-Ethernet_Pair1_N-Pad6)")
			(pinfunction "Ethernet_Pair1_N")
			(pintype "passive+no_connect")
		)
		(pad "7" smd rect
			(at -2 -30.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 1.08 -30.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at -2 -29.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(CM1A-Ethernet_Pair2_N-Pad9)")
			(pinfunction "Ethernet_Pair2_N")
			(pintype "passive+no_connect")
		)
		(pad "10" smd rect
			(at 1.08 -29.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "unconnected-(CM1A-Ethernet_Pair0_N-Pad10)")
			(pinfunction "Ethernet_Pair0_N")
			(pintype "passive+no_connect")
		)
		(pad "11" smd rect
			(at -2 -29.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "unconnected-(CM1A-Ethernet_Pair2_P-Pad11)")
			(pinfunction "Ethernet_Pair2_P")
			(pintype "passive+no_connect")
		)
		(pad "12" smd rect
			(at 1.08 -29.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "unconnected-(CM1A-Ethernet_Pair0_P-Pad12)")
			(pinfunction "Ethernet_Pair0_P")
			(pintype "passive+no_connect")
		)
		(pad "13" smd rect
			(at -2 -28.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 1.08 -28.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at -2 -28.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "unconnected-(CM1A-Ethernet_nLED3(3.3v)-Pad15)")
			(pinfunction "Ethernet_nLED3(3.3v)")
			(pintype "output+no_connect")
		)
		(pad "16" smd rect
			(at 1.08 -28.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "unconnected-(CM1A-Ethernet_SYNC_IN(1.8v)-Pad16)")
			(pinfunction "Ethernet_SYNC_IN(1.8v)")
			(pintype "input+no_connect")
		)
		(pad "17" smd rect
			(at -2 -28.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "unconnected-(CM1A-Ethernet_nLED2(3.3v)-Pad17)")
			(pinfunction "Ethernet_nLED2(3.3v)")
			(pintype "output+no_connect")
		)
		(pad "18" smd rect
			(at 1.08 -28.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(CM1A-Ethernet_SYNC_OUT(1.8v)-Pad18)")
			(pinfunction "Ethernet_SYNC_OUT(1.8v)")
			(pintype "input+no_connect")
		)
		(pad "19" smd rect
			(at -2 -27.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "unconnected-(CM1A-Ethernet_nLED1(3.3v)-Pad19)")
			(pinfunction "Ethernet_nLED1(3.3v)")
			(pintype "output+no_connect")
		)
		(pad "20" smd rect
			(at 1.08 -27.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "unconnected-(CM1A-EEPROM_nWP-Pad20)")
			(pinfunction "EEPROM_nWP")
			(pintype "passive+no_connect")
		)
		(pad "21" smd rect
			(at -2 -27.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "/Audio/CM4_LED_ACT")
			(pinfunction "PI_nLED_Activity")
			(pintype "open_collector")
		)
		(pad "22" smd rect
			(at 1.08 -27.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "23" smd rect
			(at -2 -26.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "24" smd rect
			(at 1.08 -26.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/Audio/audio_out_stereo")
			(pinfunction "GPIO26")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at -2 -26.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "/Audio/audio_pcm_dout")
			(pinfunction "GPIO21")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at 1.08 -26.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "/Audio/audio_pcm_fs")
			(pinfunction "GPIO19")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at -2 -26.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/Audio/audio_pcm_din")
			(pinfunction "GPIO20")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 1.08 -26.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/Audio/CM4_GPIO13")
			(pinfunction "GPIO13")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -2 -25.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/Audio/CM4_GPIO16")
			(pinfunction "GPIO16")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at 1.08 -25.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "/Audio/CM4_GPIO6")
			(pinfunction "GPIO6")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at -2 -25.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "/Audio/CM4_GPIO12")
			(pinfunction "GPIO12")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at 1.08 -25.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "33" smd rect
			(at -2 -24.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "34" smd rect
			(at 1.08 -24.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "/Audio/CM4_GPIO5")
			(pinfunction "GPIO5")
			(pintype "passive")
		)
		(pad "35" smd rect
			(at -2 -24.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "/Audio/CM4_ID_SC")
			(pinfunction "ID_SC")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at 1.08 -24.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "/Audio/CM4_ID_SD")
			(pinfunction "ID_SD")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at -2 -24.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "/Audio/CM4_GPIO7")
			(pinfunction "GPIO7")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at 1.08 -24.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "/Audio/CM4_GPIO11")
			(pinfunction "GPIO11")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at -2 -23.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "/Audio/CM4_GPIO8")
			(pinfunction "GPIO8")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at 1.08 -23.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "/Audio/CM4_GPIO9")
			(pinfunction "GPIO9")
			(pintype "passive")
		)
		(pad "41" smd rect
			(at -2 -23.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "/Audio/CM4_GPIO25")
			(pinfunction "GPIO25")
			(pintype "passive")
		)
		(pad "42" smd rect
			(at 1.08 -23.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "43" smd rect
			(at -2 -22.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "44" smd rect
			(at 1.08 -22.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "/Audio/CM4_GPIO10")
			(pinfunction "GPIO10")
			(pintype "passive")
		)
		(pad "45" smd rect
			(at -2 -22.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "/Audio/CM4_GPIO24")
			(pinfunction "GPIO24")
			(pintype "passive")
		)
		(pad "46" smd rect
			(at 1.08 -22.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "/Audio/CM4_GPIO22")
			(pinfunction "GPIO22")
			(pintype "passive")
		)
		(pad "47" smd rect
			(at -2 -22.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "/Audio/CM4_GPIO23")
			(pinfunction "GPIO23")
			(pintype "passive")
		)
		(pad "48" smd rect
			(at 1.08 -22.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/Audio/audio_in_stereo")
			(pinfunction "GPIO27")
			(pintype "passive")
		)
		(pad "49" smd rect
			(at -2 -21.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/Audio/audio_pcm_clk")
			(pinfunction "GPIO18")
			(pintype "passive")
		)
		(pad "50" smd rect
			(at 1.08 -21.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "/Audio/CM4_GPIO17")
			(pinfunction "GPIO17")
			(pintype "passive")
		)
		(pad "51" smd rect
			(at -2 -21.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "/Audio/INT_MIDI_RX")
			(pinfunction "GPIO15")
			(pintype "passive")
		)
		(pad "52" smd rect
			(at 1.08 -21.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at -2 -20.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "54" smd rect
			(at 1.08 -20.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "/Audio/CM4_GPIO4")
			(pinfunction "GPIO4")
			(pintype "passive")
		)
		(pad "55" smd rect
			(at -2 -20.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "/Audio/INT_MIDI_TX")
			(pinfunction "GPIO14")
			(pintype "passive")
		)
		(pad "56" smd rect
			(at 1.08 -20.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/Audio/conf_i2c_scl")
			(pinfunction "GPIO3")
			(pintype "passive")
		)
		(pad "57" smd rect
			(at -2 -20.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "unconnected-(CM1A-SD_CLK-Pad57)")
			(pinfunction "SD_CLK")
			(pintype "passive+no_connect")
		)
		(pad "58" smd rect
			(at 1.08 -20.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/Audio/conf_i2c_sda")
			(pinfunction "GPIO2")
			(pintype "passive")
		)
		(pad "59" smd rect
			(at -2 -19.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "60" smd rect
			(at 1.08 -19.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "61" smd rect
			(at -2 -19.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "unconnected-(CM1A-SD_DAT3-Pad61)")
			(pinfunction "SD_DAT3")
			(pintype "passive+no_connect")
		)
		(pad "62" smd rect
			(at 1.08 -19.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "unconnected-(CM1A-SD_CMD-Pad62)")
			(pinfunction "SD_CMD")
			(pintype "passive+no_connect")
		)
		(pad "63" smd rect
			(at -2 -18.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "unconnected-(CM1A-SD_DAT0-Pad63)")
			(pinfunction "SD_DAT0")
			(pintype "passive+no_connect")
		)
		(pad "64" smd rect
			(at 1.08 -18.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "unconnected-(CM1A-SD_DAT5-Pad64)")
			(pinfunction "SD_DAT5")
			(pintype "passive+no_connect")
		)
		(pad "65" smd rect
			(at -2 -18.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "66" smd rect
			(at 1.08 -18.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "67" smd rect
			(at -2 -18.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "unconnected-(CM1A-SD_DAT1-Pad67)")
			(pinfunction "SD_DAT1")
			(pintype "passive+no_connect")
		)
		(pad "68" smd rect
			(at 1.08 -18.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "unconnected-(CM1A-SD_DAT4-Pad68)")
			(pinfunction "SD_DAT4")
			(pintype "passive+no_connect")
		)
		(pad "69" smd rect
			(at -2 -17.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "unconnected-(CM1A-SD_DAT2-Pad69)")
			(pinfunction "SD_DAT2")
			(pintype "passive+no_connect")
		)
		(pad "70" smd rect
			(at 1.08 -17.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "unconnected-(CM1A-SD_DAT7-Pad70)")
			(pinfunction "SD_DAT7")
			(pintype "passive+no_connect")
		)
		(pad "71" smd rect
			(at -2 -17.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "72" smd rect
			(at 1.08 -17.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "unconnected-(CM1A-SD_DAT6-Pad72)")
			(pinfunction "SD_DAT6")
			(pintype "passive+no_connect")
		)
		(pad "73" smd rect
			(at -2 -16.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "unconnected-(CM1A-SD_VDD_Override-Pad73)")
			(pinfunction "SD_VDD_Override")
			(pintype "input+no_connect")
		)
		(pad "74" smd rect
			(at 1.08 -16.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "75" smd rect
			(at -2 -16.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "unconnected-(CM1A-SD_PWR_ON-Pad75)")
			(pinfunction "SD_PWR_ON")
			(pintype "output+no_connect")
		)
		(pad "76" smd rect
			(at 1.08 -16.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "unconnected-(CM1A-Reserved-Pad76)")
			(pinfunction "Reserved")
			(pintype "passive+no_connect")
		)
		(pad "77" smd rect
			(at -2 -16.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "+5VP")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
		)
		(pad "78" smd rect
			(at 1.08 -16.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "/Audio/CM4_3V")
			(pinfunction "GPIO_VREF(1.8v/3.3v_Input)")
			(pintype "power_in")
		)
		(pad "79" smd rect
			(at -2 -15.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "+5VP")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
		)
		(pad "80" smd rect
			(at 1.08 -15.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "unconnected-(CM1A-SCL0-Pad80)")
			(pinfunction "SCL0")
			(pintype "passive+no_connect")
		)
		(pad "81" smd rect
			(at -2 -15.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "+5VP")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
		)
		(pad "82" smd rect
			(at 1.08 -15.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "unconnected-(CM1A-SDA0-Pad82)")
			(pinfunction "SDA0")
			(pintype "passive+no_connect")
		)
		(pad "83" smd rect
			(at -2 -14.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "+5VP")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
		)
		(pad "84" smd rect
			(at 1.08 -14.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "/Audio/CM4_3V")
			(pinfunction "+3.3v_(Output)")
			(pintype "power_out")
		)
		(pad "85" smd rect
			(at -2 -14.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "+5VP")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
		)
		(pad "86" smd rect
			(at 1.08 -14.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "/Audio/CM4_3V")
			(pinfunction "+3.3v_(Output)")
			(pintype "power_out")
		)
		(pad "87" smd rect
			(at -2 -14.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "+5VP")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
		)
		(pad "88" smd rect
			(at 1.08 -14.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(CM1A-+1.8v_(Output)-Pad88)")
			(pinfunction "+1.8v_(Output)")
			(pintype "power_out+no_connect")
		)
		(pad "89" smd rect
			(at -2 -13.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "unconnected-(CM1A-WiFi_nDisable-Pad89)")
			(pinfunction "WiFi_nDisable")
			(pintype "power_in+no_connect")
		)
		(pad "90" smd rect
			(at 1.08 -13.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "unconnected-(CM1A-+1.8v_(Output)-Pad90)")
			(pinfunction "+1.8v_(Output)")
			(pintype "power_out+no_connect")
		)
		(pad "91" smd rect
			(at -2 -13.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "unconnected-(CM1A-BT_nDisable-Pad91)")
			(pinfunction "BT_nDisable")
			(pintype "power_in+no_connect")
		)
		(pad "92" smd rect
			(at 1.08 -13.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "unconnected-(CM1A-RUN_PG-Pad92)")
			(pinfunction "RUN_PG")
			(pintype "passive+no_connect")
		)
		(pad "93" smd rect
			(at -2 -12.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "unconnected-(CM1A-nRPIBOOT-Pad93)")
			(pinfunction "nRPIBOOT")
			(pintype "input+no_connect")
		)
		(pad "94" smd rect
			(at 1.08 -12.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "unconnected-(CM1A-AnalogIP1-Pad94)")
			(pinfunction "AnalogIP1")
			(pintype "passive+no_connect")
		)
		(pad "95" smd rect
			(at -2 -12.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 213 "/Audio/CM4_LED_PWR")
			(pinfunction "nPI_LED_PWR")
			(pintype "output")
		)
		(pad "96" smd rect
			(at 1.08 -12.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "unconnected-(CM1A-AnalogIP0-Pad96)")
			(pinfunction "AnalogIP0")
			(pintype "passive+no_connect")
		)
		(pad "97" smd rect
			(at -2 -12.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "unconnected-(CM1A-Camera_GPIO-Pad97)")
			(pinfunction "Camera_GPIO")
			(pintype "passive+no_connect")
		)
		(pad "98" smd rect
			(at 1.08 -12.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "99" smd rect
			(at -2 -11.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "unconnected-(CM1A-Global_EN-Pad99)")
			(pinfunction "Global_EN")
			(pintype "input+no_connect")
		)
		(pad "100" smd rect
			(at 1.08 -11.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 258 "/Audio/nEXTRST")
			(pinfunction "nEXTRST")
			(pintype "output")
		)
		(pad "101" smd rect
			(at 31.92 -31.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 250 "Net-(CM1B-USB_OTG_ID)")
			(pinfunction "USB_OTG_ID")
			(pintype "input")
		)
		(pad "102" smd rect
			(at 35 -31.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 115 "unconnected-(CM1B-PCIe_CLK_nREQ-Pad102)")
			(pinfunction "PCIe_CLK_nREQ")
			(pintype "input+no_connect")
		)
		(pad "103" smd rect
			(at 31.92 -30.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 272 "/Connectivity/USB_CM_N")
			(pinfunction "USB2_N")
			(pintype "passive")
		)
		(pad "104" smd rect
			(at 35 -30.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "unconnected-(CM1B-Reserved-Pad104)")
			(pinfunction "Reserved")
			(pintype "passive+no_connect")
		)
		(pad "105" smd rect
			(at 31.92 -30.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 273 "/Connectivity/USB_CM_P")
			(pinfunction "USB2_P")
			(pintype "passive")
		)
		(pad "106" smd rect
			(at 35 -30.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "unconnected-(CM1B-Reserved-Pad106)")
			(pinfunction "Reserved")
			(pintype "passive+no_connect")
		)
		(pad "107" smd rect
			(at 31.92 -30.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "108" smd rect
			(at 35 -30.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "109" smd rect
			(at 31.92 -29.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "unconnected-(CM1B-PCIe_nRST-Pad109)")
			(pinfunction "PCIe_nRST")
			(pintype "bidirectional+no_connect")
		)
		(pad "110" smd rect
			(at 35 -29.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "unconnected-(CM1B-PCIe_CLK_P-Pad110)")
			(pinfunction "PCIe_CLK_P")
			(pintype "output+no_connect")
		)
		(pad "111" smd rect
			(at 31.92 -29.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 120 "unconnected-(CM1B-VDAC_COMP-Pad111)")
			(pinfunction "VDAC_COMP")
			(pintype "passive+no_connect")
		)
		(pad "112" smd rect
			(at 35 -29.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 121 "unconnected-(CM1B-PCIe_CLK_N-Pad112)")
			(pinfunction "PCIe_CLK_N")
			(pintype "output+no_connect")
		)
		(pad "113" smd rect
			(at 31.92 -28.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "114" smd rect
			(at 35 -28.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "115" smd rect
			(at 31.92 -28.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 122 "unconnected-(CM1B-CAM1_D0_N-Pad115)")
			(pinfunction "CAM1_D0_N")
			(pintype "input+no_connect")
			(die_length 0.02)
		)
		(pad "116" smd rect
			(at 35 -28.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 123 "unconnected-(CM1B-PCIe_RX_P-Pad116)")
			(pinfunction "PCIe_RX_P")
			(pintype "input+no_connect")
		)
		(pad "117" smd rect
			(at 31.92 -28.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 124 "unconnected-(CM1B-CAM1_D0_P-Pad117)")
			(pinfunction "CAM1_D0_P")
			(pintype "input+no_connect")
			(die_length 0.01)
		)
		(pad "118" smd rect
			(at 35 -28.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "unconnected-(CM1B-PCIe_RX_N-Pad118)")
			(pinfunction "PCIe_RX_N")
			(pintype "input+no_connect")
		)
		(pad "119" smd rect
			(at 31.92 -27.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "120" smd rect
			(at 35 -27.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "121" smd rect
			(at 31.92 -27.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "unconnected-(CM1B-CAM1_D1_N-Pad121)")
			(pinfunction "CAM1_D1_N")
			(pintype "input+no_connect")
			(die_length 0.4)
		)
		(pad "122" smd rect
			(at 35 -27.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "unconnected-(CM1B-PCIe_TX_P-Pad122)")
			(pinfunction "PCIe_TX_P")
			(pintype "output+no_connect")
		)
		(pad "123" smd rect
			(at 31.92 -26.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "unconnected-(CM1B-CAM1_D1_P-Pad123)")
			(pinfunction "CAM1_D1_P")
			(pintype "input+no_connect")
			(die_length 0.4)
		)
		(pad "124" smd rect
			(at 35 -26.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 130 "unconnected-(CM1B-PCIe_TX_N-Pad124)")
			(pinfunction "PCIe_TX_N")
			(pintype "output+no_connect")
		)
		(pad "125" smd rect
			(at 31.92 -26.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "126" smd rect
			(at 35 -26.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "127" smd rect
			(at 31.92 -26.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "unconnected-(CM1B-CAM1_C_N-Pad127)")
			(pinfunction "CAM1_C_N")
			(pintype "input+no_connect")
			(die_length 0.78)
		)
		(pad "128" smd rect
			(at 35 -26.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 132 "unconnected-(CM1B-CAM0_D0_N-Pad128)")
			(pinfunction "CAM0_D0_N")
			(pintype "input+no_connect")
			(die_length 0.06)
		)
		(pad "129" smd rect
			(at 31.92 -25.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 133 "unconnected-(CM1B-CAM1_C_P-Pad129)")
			(pinfunction "CAM1_C_P")
			(pintype "input+no_connect")
			(die_length 0.78)
		)
		(pad "130" smd rect
			(at 35 -25.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 134 "unconnected-(CM1B-CAM0_D0_P-Pad130)")
			(pinfunction "CAM0_D0_P")
			(pintype "input+no_connect")
			(die_length 0.07)
		)
		(pad "131" smd rect
			(at 31.92 -25.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "132" smd rect
			(at 35 -25.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "133" smd rect
			(at 31.92 -24.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 135 "unconnected-(CM1B-CAM1_D2_N-Pad133)")
			(pinfunction "CAM1_D2_N")
			(pintype "input+no_connect")
			(die_length 0.05)
		)
		(pad "134" smd rect
			(at 35 -24.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 136 "unconnected-(CM1B-CAM0_D1_N-Pad134)")
			(pinfunction "CAM0_D1_N")
			(pintype "input+no_connect")
		)
		(pad "135" smd rect
			(at 31.92 -24.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "unconnected-(CM1B-CAM1_D2_P-Pad135)")
			(pinfunction "CAM1_D2_P")
			(pintype "input+no_connect")
			(die_length 0.04)
		)
		(pad "136" smd rect
			(at 35 -24.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "unconnected-(CM1B-CAM0_D1_P-Pad136)")
			(pinfunction "CAM0_D1_P")
			(pintype "input+no_connect")
		)
		(pad "137" smd rect
			(at 31.92 -24.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "138" smd rect
			(at 35 -24.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "139" smd rect
			(at 31.92 -23.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "unconnected-(CM1B-CAM1_D3_N-Pad139)")
			(pinfunction "CAM1_D3_N")
			(pintype "input+no_connect")
		)
		(pad "140" smd rect
			(at 35 -23.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "unconnected-(CM1B-CAM0_C_N-Pad140)")
			(pinfunction "CAM0_C_N")
			(pintype "input+no_connect")
			(die_length 0.02)
		)
		(pad "141" smd rect
			(at 31.92 -23.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "unconnected-(CM1B-CAM1_D3_P-Pad141)")
			(pinfunction "CAM1_D3_P")
			(pintype "input+no_connect")
		)
		(pad "142" smd rect
			(at 35 -23.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 142 "unconnected-(CM1B-CAM0_C_P-Pad142)")
			(pinfunction "CAM0_C_P")
			(pintype "input+no_connect")
			(die_length 0.02)
		)
		(pad "143" smd rect
			(at 31.92 -22.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "unconnected-(CM1B-HDMI1_HOTPLUG-Pad143)")
			(pinfunction "HDMI1_HOTPLUG")
			(pintype "input+no_connect")
		)
		(pad "144" smd rect
			(at 35 -22.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "145" smd rect
			(at 31.92 -22.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "unconnected-(CM1B-HDMI1_SDA-Pad145)")
			(pinfunction "HDMI1_SDA")
			(pintype "bidirectional+no_connect")
		)
		(pad "146" smd rect
			(at 35 -22.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "unconnected-(CM1B-HDMI1_TX2_P-Pad146)")
			(pinfunction "HDMI1_TX2_P")
			(pintype "output+no_connect")
		)
		(pad "147" smd rect
			(at 31.92 -22.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 146 "unconnected-(CM1B-HDMI1_SCL-Pad147)")
			(pinfunction "HDMI1_SCL")
			(pintype "open_collector+no_connect")
		)
		(pad "148" smd rect
			(at 35 -22.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "unconnected-(CM1B-HDMI1_TX2_N-Pad148)")
			(pinfunction "HDMI1_TX2_N")
			(pintype "output+no_connect")
		)
		(pad "149" smd rect
			(at 31.92 -21.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "unconnected-(CM1B-HDMI1_CEC-Pad149)")
			(pinfunction "HDMI1_CEC")
			(pintype "open_collector+no_connect")
		)
		(pad "150" smd rect
			(at 35 -21.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "151" smd rect
			(at 31.92 -21.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "unconnected-(CM1B-HDMI0_CEC-Pad151)")
			(pinfunction "HDMI0_CEC")
			(pintype "open_collector+no_connect")
		)
		(pad "152" smd rect
			(at 35 -21.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 150 "unconnected-(CM1B-HDMI1_TX1_P-Pad152)")
			(pinfunction "HDMI1_TX1_P")
			(pintype "output+no_connect")
			(die_length 1)
		)
		(pad "153" smd rect
			(at 31.92 -20.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 151 "unconnected-(CM1B-HDMI0_HOTPLUG-Pad153)")
			(pinfunction "HDMI0_HOTPLUG")
			(pintype "input+no_connect")
		)
		(pad "154" smd rect
			(at 35 -20.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 152 "unconnected-(CM1B-HDMI1_TX1_N-Pad154)")
			(pinfunction "HDMI1_TX1_N")
			(pintype "output+no_connect")
			(die_length 1)
		)
		(pad "155" smd rect
			(at 31.92 -20.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "156" smd rect
			(at 35 -20.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "157" smd rect
			(at 31.92 -20.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 153 "unconnected-(CM1B-DSI0_D0_N-Pad157)")
			(pinfunction "DSI0_D0_N")
			(pintype "output+no_connect")
		)
		(pad "158" smd rect
			(at 35 -20.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 155 "unconnected-(CM1B-HDMI1_TX0_P-Pad158)")
			(pinfunction "HDMI1_TX0_P")
			(pintype "output+no_connect")
			(die_length 1.51)
		)
		(pad "159" smd rect
			(at 31.92 -19.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 156 "unconnected-(CM1B-DSI0_D0_P-Pad159)")
			(pinfunction "DSI0_D0_P")
			(pintype "output+no_connect")
		)
		(pad "160" smd rect
			(at 35 -19.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "unconnected-(CM1B-HDMI1_TX0_N-Pad160)")
			(pinfunction "HDMI1_TX0_N")
			(pintype "output+no_connect")
			(die_length 1.51)
		)
		(pad "161" smd rect
			(at 31.92 -19.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "162" smd rect
			(at 35 -19.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "163" smd rect
			(at 31.92 -18.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 158 "unconnected-(CM1B-DSI0_D1_N-Pad163)")
			(pinfunction "DSI0_D1_N")
			(pintype "output+no_connect")
		)
		(pad "164" smd rect
			(at 35 -18.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 159 "unconnected-(CM1B-HDMI1_CLK_P-Pad164)")
			(pinfunction "HDMI1_CLK_P")
			(pintype "output+no_connect")
			(die_length 2.47)
		)
		(pad "165" smd rect
			(at 31.92 -18.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "unconnected-(CM1B-DSI0_D1_P-Pad165)")
			(pinfunction "DSI0_D1_P")
			(pintype "output+no_connect")
		)
		(pad "166" smd rect
			(at 35 -18.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "unconnected-(CM1B-HDMI1_CLK_N-Pad166)")
			(pinfunction "HDMI1_CLK_N")
			(pintype "output+no_connect")
			(die_length 2.47)
		)
		(pad "167" smd rect
			(at 31.92 -18.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "168" smd rect
			(at 35 -18.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "169" smd rect
			(at 31.92 -17.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 162 "unconnected-(CM1B-DSI0_C_N-Pad169)")
			(pinfunction "DSI0_C_N")
			(pintype "output+no_connect")
		)
		(pad "170" smd rect
			(at 35 -17.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 163 "unconnected-(CM1B-HDMI0_TX2_P-Pad170)")
			(pinfunction "HDMI0_TX2_P")
			(pintype "output+no_connect")
		)
		(pad "171" smd rect
			(at 31.92 -17.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 164 "unconnected-(CM1B-DSI0_C_P-Pad171)")
			(pinfunction "DSI0_C_P")
			(pintype "output+no_connect")
		)
		(pad "172" smd rect
			(at 35 -17.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "unconnected-(CM1B-HDMI0_TX2_N-Pad172)")
			(pinfunction "HDMI0_TX2_N")
			(pintype "output+no_connect")
		)
		(pad "173" smd rect
			(at 31.92 -16.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "174" smd rect
			(at 35 -16.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "175" smd rect
			(at 31.92 -16.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 166 "unconnected-(CM1B-DSI1_D0_N-Pad175)")
			(pinfunction "DSI1_D0_N")
			(pintype "output+no_connect")
		)
		(pad "176" smd rect
			(at 35 -16.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 167 "unconnected-(CM1B-HDMI0_TX1_P-Pad176)")
			(pinfunction "HDMI0_TX1_P")
			(pintype "output+no_connect")
			(die_length 0.62)
		)
		(pad "177" smd rect
			(at 31.92 -16.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 168 "unconnected-(CM1B-DSI1_D0_P-Pad177)")
			(pinfunction "DSI1_D0_P")
			(pintype "output+no_connect")
			(die_length 0.01)
		)
		(pad "178" smd rect
			(at 35 -16.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 169 "unconnected-(CM1B-HDMI0_TX1_N-Pad178)")
			(pinfunction "HDMI0_TX1_N")
			(pintype "output+no_connect")
			(die_length 0.62)
		)
		(pad "179" smd rect
			(at 31.92 -15.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "180" smd rect
			(at 35 -15.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "181" smd rect
			(at 31.92 -15.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "unconnected-(CM1B-DSI1_D1_N-Pad181)")
			(pinfunction "DSI1_D1_N")
			(pintype "output+no_connect")
			(die_length 1.06)
		)
		(pad "182" smd rect
			(at 35 -15.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 171 "unconnected-(CM1B-HDMI0_TX0_P-Pad182)")
			(pinfunction "HDMI0_TX0_P")
			(pintype "output+no_connect")
			(die_length 1.76)
		)
		(pad "183" smd rect
			(at 31.92 -14.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 172 "unconnected-(CM1B-DSI1_D1_P-Pad183)")
			(pinfunction "DSI1_D1_P")
			(pintype "output+no_connect")
			(die_length 1.06)
		)
		(pad "184" smd rect
			(at 35 -14.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 173 "unconnected-(CM1B-HDMI0_TX0_N-Pad184)")
			(pinfunction "HDMI0_TX0_N")
			(pintype "output+no_connect")
			(die_length 1.76)
		)
		(pad "185" smd rect
			(at 31.92 -14.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "186" smd rect
			(at 35 -14.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "187" smd rect
			(at 31.92 -14.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 174 "unconnected-(CM1B-DSI1_C_N-Pad187)")
			(pinfunction "DSI1_C_N")
			(pintype "output+no_connect")
		)
		(pad "188" smd rect
			(at 35 -14.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 175 "unconnected-(CM1B-HDMI0_CLK_P-Pad188)")
			(pinfunction "HDMI0_CLK_P")
			(pintype "output+no_connect")
			(die_length 3.24)
		)
		(pad "189" smd rect
			(at 31.92 -13.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 176 "unconnected-(CM1B-DSI1_C_P-Pad189)")
			(pinfunction "DSI1_C_P")
			(pintype "output+no_connect")
			(die_length 1.28)
		)
		(pad "190" smd rect
			(at 35 -13.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 177 "unconnected-(CM1B-HDMI0_CLK_N-Pad190)")
			(pinfunction "HDMI0_CLK_N")
			(pintype "output+no_connect")
			(die_length 3.25)
		)
		(pad "191" smd rect
			(at 31.92 -13.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(die_length 1.28)
		)
		(pad "192" smd rect
			(at 35 -13.3 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "193" smd rect
			(at 31.92 -12.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 178 "unconnected-(CM1B-DSI1_D2_N-Pad193)")
			(pinfunction "DSI1_D2_N")
			(pintype "output+no_connect")
			(die_length 0.83)
		)
		(pad "194" smd rect
			(at 35 -12.9 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 179 "unconnected-(CM1B-DSI1_D3_N-Pad194)")
			(pinfunction "DSI1_D3_N")
			(pintype "output+no_connect")
			(die_length 3.78)
		)
		(pad "195" smd rect
			(at 31.92 -12.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 180 "unconnected-(CM1B-DSI1_D2_P-Pad195)")
			(pinfunction "DSI1_D2_P")
			(pintype "output+no_connect")
			(die_length 0.84)
		)
		(pad "196" smd rect
			(at 35 -12.5 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 181 "unconnected-(CM1B-DSI1_D3_P-Pad196)")
			(pinfunction "DSI1_D3_P")
			(pintype "output+no_connect")
			(die_length 3.78)
		)
		(pad "197" smd rect
			(at 31.92 -12.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "198" smd rect
			(at 35 -12.1 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "199" smd rect
			(at 31.92 -11.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 182 "unconnected-(CM1B-HDMI0_SDA-Pad199)")
			(pinfunction "HDMI0_SDA")
			(pintype "bidirectional+no_connect")
		)
		(pad "200" smd rect
			(at 35 -11.7 90)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 183 "unconnected-(CM1B-HDMI0_SCL-Pad200)")
			(pinfunction "HDMI0_SCL")
			(pintype "open_collector+no_connect")
		)
		(embedded_fonts no)
		(model "./3d-models/DF40C-100DS.stp"
			(offset
				(xyz -0.46 15.38 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "./3d-models/DF40C-100DS.stp"
			(offset
				(xyz 33.46 15.38 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/3d-models/cm-min.step"
			(offset
				(xyz 52.5 -3.5 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "Fiducial:Fiducial_1.5mm_Mask3mm"
		(layer "F.Cu")
		(at 20.005615 122.994385)
		(descr "Circular Fiducial, 1.5mm bare copper, 3mm soldermask opening")
		(tags "fiducial")
		(property "Reference" "FID3"
			(at -0.405615 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "Fiducial"
			(at 0 2.6035 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Fiducial*")
		(sheetname "/")
		(sheetfile "pedalboard-hw.kicad_sch")
		(attr smd exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.75)
			(clearance 0.75)
		)
		(embedded_fonts no)
	)
	(footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth"
		(locked yes)
		(layer "F.Cu")
		(at 180 67)
		(descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
		(tags "tact sw push 12mm")
		(property "Reference" "SW7"
			(at -4.8 -7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Tactile Button"
			(at 0 7.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/430172043816.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "F"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430162043826/9950802"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW*Omron*B3FS*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -4 -4 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/MIDI/SW_F")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/MIDI/SW_F")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/WE-tact-button.stp"
			(offset
				(xyz 0 0 1.75)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 157.79 37.67 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.36 0.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 315.58 75.34 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 315.58 75.34 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Supply/polarity_checked")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965"
		(layer "F.Cu")
		(at 42 128)
		(descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
		(tags "mounting hole 2.7mm no annular m2.5 din965")
		(property "Reference" "H14"
			(at 3.992585 2.089215 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "pedalboard-hw.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 157.82 33.73 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.37 0.24 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 315.64 67.46 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 315.64 67.46 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Supply/polarity_checked")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth"
		(locked yes)
		(layer "F.Cu")
		(at 30 119)
		(descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
		(tags "tact sw push 12mm")
		(property "Reference" "SW8"
			(at 3.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Tactile Button"
			(at 0 7.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/430172043816.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430162043826/9950802"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW*Omron*B3FS*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -4 -5 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/MIDI/SW_A")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/MIDI/SW_A")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/WE-tact-button.stp"
			(offset
				(xyz 0 0 1.75)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 161.2 37.68)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 2.25 0.32 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Supply/polarity_checked")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 103.19 77.7525 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 2.9525 -0.09 90)
			(layer "F.SilkS")
		)
		(property "Value" "2K2"
			(at -2.5 3.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Resistor 2.2K 1% 63mW"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT2K20/1760345"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 91 "Net-(D7-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 95 "/Audio/CM4_3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 113.2 47.7 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at -1.6 -2.4 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 65.35 160.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 65.35 160.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 65.35 160.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 65.35 160.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 158.67 49.8 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 1 4.37 180)
			(layer "F.SilkS")
		)
		(property "Value" "20K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "Resistor 20K 1% 63mW"
			(at 108.87 208.47 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RMCF0805FT20K0/1760314"
			(at 108.87 208.47 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 53 "Net-(U6-COMP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 52 "Net-(C31-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965"
		(layer "F.Cu")
		(at 185.005615 22.994385)
		(descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
		(tags "mounting hole 2.7mm no annular m2.5 din965")
		(property "Reference" "H3"
			(at -0.005615 3.905615 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at -0.5 -3.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "pedalboard-hw.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 107.09 77.7525 -90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D6"
			(at -2.6525 -0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED Y"
			(at 3.5 2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/harvatek-corporation/B1701NG-20D000314U1930/16671738"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "/Audio/CM4_LED_ACT")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 102.2 40.5 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at -2.3 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "25V/10%"
			(at 204.4 81 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B105KAFNNNE/3886724"
			(at 204.4 81 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 90.009 43.6474)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at -2.48 -0.06 0)
			(layer "F.SilkS")
		)
		(property "Value" "120_100MHz"
			(at -5.7 -0.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8796738650142/ENFA0003.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/murata-electronics/BLM18KG121TN1D/1982762"
			(at 27.29 130.57 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 191 "Net-(J26-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 212 "Net-(L2-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SON:USON-10_2.5x1.0mm_P0.5mm"
		(layer "F.Cu")
		(at 25.05 56.95 180)
		(descr "USON-10 2.5x1.0mm_ Pitch 0.5mm http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf")
		(tags "USON-10 2.5x1.0mm Pitch 0.5mm")
		(property "Reference" "U11"
			(at 0.2 -2.7 180)
			(layer "F.SilkS")
		)
		(property "Value" "TPD4EUSB30"
			(at 0.01829 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd2eusb30a.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4-Channel ESD Protection for Super-Speed USB 3.0 Interface, USON-10"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/texas-instruments/TPD4EUSB30DQAR/2503665"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USON*2.5x1.0mm*P0.5mm*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.385 -1 90)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "unconnected-(U11-D1+-Pad1)")
			(pinfunction "D1+")
			(pintype "passive+no_connect")
		)
		(pad "2" smd roundrect
			(at -0.385 -0.5 90)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 289 "unconnected-(U11-D1--Pad2)")
			(pinfunction "D1-")
			(pintype "passive+no_connect")
		)
		(pad "3" smd roundrect
			(at -0.385 0 90)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -0.385 0.5 90)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 282 "/Connectivity/USB_D_P")
			(pinfunction "D2+")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -0.385 1 90)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 283 "/Connectivity/USB_D_N")
			(pinfunction "D2-")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 0.385 1 90)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 285 "unconnected-(U11-NC-Pad6)")
			(pinfunction "NC")
			(pintype "free")
		)
		(pad "7" smd roundrect
			(at 0.385 0.5 90)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 284 "unconnected-(U11-NC-Pad7)")
			(pinfunction "NC")
			(pintype "free")
		)
		(pad "8" smd roundrect
			(at 0.385 0 90)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 0.385 -0.5 90)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 288 "unconnected-(U11-NC-Pad9)")
			(pinfunction "NC")
			(pintype "free")
		)
		(pad "10" smd roundrect
			(at 0.385 -1 90)
			(size 0.3 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "unconnected-(U11-NC-Pad10)")
			(pinfunction "NC")
			(pintype "free")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_SON.3dshapes/USON-10_2.5x1.0mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 154.23 25.94)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP2"
			(at 0 -1.998 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 63.96 46.36 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 3.16 0.04 90)
			(layer "F.SilkS")
		)
		(property "Value" "18p"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.seielect.com/Catalog/SEI-CML.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "50V/5%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/CML0805C0G180JT50V/10659995"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U9-XTALIN{slash}CLKIN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 42.7 47.46 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 2.71 -0.19 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 -1.64 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/RNCP0805FTD1K00/2240229"
			(at -4.76 90.16 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 195 "Net-(J8-PadT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 139.75 43.5)
		(descr "SOT-353, SC-70-5")
		(tags "SOT-353 SC-70-5")
		(property "Reference" "U1"
			(at -0.85 -2.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "74AHCT1G32SE-7"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/74AHCT1G32.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/diodes-incorporated/74AHCT1G32SE-7/2711987"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LEDs/")
		(sheetfile "leds.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 219 "Net-(U1-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.95 0)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 248 "Net-(U1-Y)")
			(pinfunction "Y")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "+5VP")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm_CircularMountingHoles"
		(locked yes)
		(layer "F.Cu")
		(at 135.25 31.5)
		(descr "Alps rotary encoder, EC12E... with switch, vertical shaft, mounting holes with circular drills, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC11/EC11E15204A3.html")
		(tags "rotary encoder")
		(property "Reference" "SW2"
			(at 2.8 -4.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "24P/R 24mm"
			(at 7.5 10.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/PEC11R.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "GAIN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/bourns-inc/PEC11R-4225F-S0024/4499659"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RotaryEncoder*Switch*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 11.1 6.3 0)
			(layer "F.Fab")
		)
		(pad "A" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/MIDI/ROT_GAIN_A")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "B" thru_hole circle
			(at 0 5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/MIDI/ROT_GAIN_B")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "C" thru_hole circle
			(at 0 2.5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "MP" thru_hole circle
			(at 7.5 -3.1)
			(size 3.2 3.2)
			(drill 2.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "MP" thru_hole circle
			(at 7.5 8.1)
			(size 3.2 3.2)
			(drill 2.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "S1" thru_hole circle
			(at 14.5 5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/MIDI/SW_GAIN")
			(pinfunction "S1")
			(pintype "passive")
		)
		(pad "S2" thru_hole circle
			(at 14.5 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "S2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/EC11E-05SW.STEP"
			(offset
				(xyz 7.4 -2.3 -12)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965"
		(layer "F.Cu")
		(at 105 98)
		(descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
		(tags "mounting hole 2.7mm no annular m2.5 din965")
		(property "Reference" "H16"
			(at -4.7 1 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "pedalboard-hw.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth"
		(locked yes)
		(layer "F.Cu")
		(at 105 119)
		(descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
		(tags "tact sw push 12mm")
		(property "Reference" "SW9"
			(at -4.4 7.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "Tactile Button"
			(at 0 7.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/430172043816.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "B"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430162043826/9950802"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW*Omron*B3FS*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -4 -5 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "/MIDI/SW_B")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 7 -2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "/MIDI/SW_B")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 7 2.5)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/WE-tact-button.stp"
			(offset
				(xyz 0 0 1.75)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 100.5906 77.8525)
		(descr "SOT-353, SC-70-5")
		(tags "SOT-353 SC-70-5")
		(property "Reference" "U7"
			(at 0 -2.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "74AHCT1G32SE-7"
			(at 0 2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/74AHCT1G32.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/diodes-incorporated/74AHCT1G32SE-7/2711987"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 213 "/Audio/CM4_LED_PWR")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.95 0)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "Net-(D7-K)")
			(pinfunction "Y")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 0.95 -0.65)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/Audio/CM4_3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 108.64 52.8 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 3.08 -0.08 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 -1.36 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 55.84 161.44 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 55.84 161.44 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 55.84 161.44 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 55.84 161.44 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 117.4 48.7 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0.21 -1.89 90)
			(layer "F.SilkS")
		)
		(property "Value" "15p"
			(at 2.4 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.seielect.com/Catalog/SEI-CML.PDF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "50V/5%"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/CML0805C0G150JT50V/10660046"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(C26-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 160.67 49.82 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at -1.08 -3.97 180)
			(layer "F.SilkS")
		)
		(property "Value" "1.2n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM2165C2A122JA01-01.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 10V Ceramic Capacitor X5R"
			(at 210.49 -110.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/murata-electronics/GRM2165C2A122JA01D/2544699"
			(at 210.49 -110.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(C31-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.0x2.0mm"
		(layer "F.Cu")
		(at 113.49 57.66)
		(descr "SMD rectangular pad as test Point, square 2.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP4"
			(at 0.27 2.08 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 230 "Net-(D2-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Pedalboard Library:CP-2350"
		(locked yes)
		(layer "F.Cu")
		(at 90 22 180)
		(descr "Female <b>CONNECTOR</b><p>\n5 pins 90 deg. with shield, horizontal (DIN 41524)")
		(property "Reference" "J2"
			(at -11.6945 -12 180)
			(layer "F.SilkS")
		)
		(property "Value" "DIN5"
			(at 0 5.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.switchcraft.com/assets/1/24/57PC5F_CD.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "MIDI In"
			(at 180 44 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/switchcraft-inc/57PC5F/275385"
			(at 180 44 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIN*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr dnp)
		(fp_text user "4"
			(at 7.1055 -13.6 0)
			(layer "F.SilkS")
		)
		(fp_text user "3"
			(at -9.3945 -6.9 0)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 0.5 -5.9 0)
			(layer "F.SilkS")
		)
		(fp_text user "5"
			(at -8.2945 -13.6 0)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 8.4055 -6.8 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole roundrect
			(at 7.5 -10 180)
			(size 2.5 2.5)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 193 "unconnected-(J2-Pad1)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole roundrect
			(at 0 -10 270)
			(size 2.5 2.5)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 2 "Net-(J25-Pin_2)")
			(pintype "passive")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 45)
		)
		(pad "3" thru_hole roundrect
			(at -7.5 -10 180)
			(size 2.5 2.5)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 194 "unconnected-(J2-Pad3)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 45)
		)
		(pad "4" thru_hole roundrect
			(at 5 -12.5 180)
			(size 2.5 2.5)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 186 "Net-(J25-Pin_1)")
			(pintype "passive")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 45)
		)
		(pad "5" thru_hole roundrect
			(at -5 -12.5 180)
			(size 2.5 2.5)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 187 "Net-(J25-Pin_3)")
			(pintype "passive")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 45)
		)
		(pad "PE" thru_hole roundrect
			(at -2.5 0 180)
			(size 1.8 2)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.5)
			(chamfer bottom_right)
			(solder_mask_margin 0.0508)
		)
		(pad "PE1" thru_hole rect
			(at -5 0 180)
			(size 1.8 2)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0508)
		)
		(pad "PE2" thru_hole rect
			(at 5 0 180)
			(size 1.8 2)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0508)
		)
		(pad "PE@" thru_hole roundrect
			(at 2.5 0 180)
			(size 1.8 2)
			(drill 1.3208)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0)
			(chamfer_ratio 0.5)
			(chamfer bottom_left)
			(solder_mask_margin 0.0508)
		)
		(embedded_fonts no)
	)
	(footprint "Inductor_SMD:L_Bourns_SRN6045TA"
		(layer "F.Cu")
		(at 164.9 50.14 -90)
		(descr "http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf")
		(tags "Semi-shielded Power Inductor")
		(property "Reference" "L5"
			(at 3.58 -4.14 90)
			(layer "F.SilkS")
		)
		(property "Value" "SRN6045TA-3R3Y"
			(at 0 4.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.bourns.com/docs/Product-Datasheets/SRN6045TA.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "3.3µH Semi-Shielded Wirewound Inductor 7.8A 21mOhm Nonstandard"
			(at 114.76 215.04 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/bourns-inc/SRN6045TA-3R3Y/6155103"
			(at 114.76 215.04 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power Supply/")
		(sheetfile "psu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.075 0 270)
			(size 2.35 5.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 243 "/Power Supply/switch")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.075 0 270)
			(size 2.35 5.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "+5VP")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 146 44.5 180)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U12"
			(at -0.15 2.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "AT24CS01-STUM"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "I2C Serial EEPROM, 1Kb (128x8) with Unique Serial Number, SOT-23-5"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/microchip-technology/AT24CS01-STUM-T/3973063"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 233 "/MIDI/I2C_SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 234 "/MIDI/I2C_SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "WP")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 63.96 49.76 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 3.34 -0.14 90)
			(layer "F.SilkS")
		)
		(property "Value" "18p"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.seielect.com/Catalog/SEI-CML.PDF"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "50V/5%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/stackpole-electronics-inc/CML0805C0G180JT50V/10659995"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U9-XTALOUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 100.73 42.53 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at -1.37 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at -2.27 0.03 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "25V/10%"
			(at 201.46 85.06 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B105KAFNNNE/3886724"
			(at 201.46 85.06 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 142.9 44.5 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C52"
			(at -2.2 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "1276-1180-1-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser" "581-08055C104K"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% 16V Ceramic Capacitor X7R"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21B104KBCNNNC/3886661"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:JST_PH_B4B-PH-SM4-TB_1x04-1MP_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 146.2366 52.9692 90)
		(descr "JST PH series connector, B4B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH side entry")
		(property "Reference" "J14"
			(at 0 -5.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "JST PH 4"
			(at 0 4.45 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/jst-sales-america-inc./B4B-PH-SM4-TB/926833"
			(at 199.68 -92.06 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3 0.5 90)
			(size 1 5.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 233 "/MIDI/I2C_SCL")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1 0.5 90)
			(size 1 5.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 234 "/MIDI/I2C_SDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1 0.5 90)
			(size 1 5.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+3V3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 3 0.5 90)
			(size 1 5.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -5.4 -1.75 90)
			(size 1.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
		)
		(pad "MP" smd roundrect
			(at 5.4 -1.75 90)
			(size 1.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/B4B-PH-SM4-TB (LF)(SN).STEP"
			(offset
				(xyz 0 1.75 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 90.009 42.1742)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L3"
			(at -2.52 -0.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "120_100MHz"
			(at -5.7 1.3375 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8796738650142/ENFA0003.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/murata-electronics/BLM18KG121TN1D/1982762"
			(at 28.75 132.03 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 189 "Net-(J26-Pin_1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "Net-(L3-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:Jack_3.5mm_CUI_SJ1-3525N_Horizontal"
		(locked yes)
		(layer "F.Cu")
		(at 89.9945 24.5 180)
		(descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
		(tags "TRS audio jack stereo horizontal")
		(property "Reference" "J1"
			(at -7 -1.7 270)
			(layer "F.SilkS")
		)
		(property "Value" "Jack 3.5mm"
			(at 0 2 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.cuidevices.com/product/resource/sj1-352xng.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "MIDI Out"
			(at 179.989 49 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/cui-devices/SJ1-3525NG/738690"
			(at 179.989 49 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(fp_text user "PCB edge"
			(at 0 3.65 180)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 180)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5 0 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu")
		)
		(pad "" np_thru_hole circle
			(at 0 -5 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu")
		)
		(pad "" np_thru_hole circle
			(at 5 0 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu")
		)
		(pad "R" thru_hole oval
			(at -5 -5 180)
			(size 1.2 2.2)
			(drill oval 0.45 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 186 "Net-(J25-Pin_1)")
			(pintype "passive")
		)
		(pad "RN" thru_hole oval
			(at -2.5 -5 180)
			(size 1.2 2.2)
			(drill oval 0.45 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 186 "Net-(J25-Pin_1)")
			(pintype "passive")
		)
		(pad "S" thru_hole oval
			(at 0 0 180)
			(size 2.2 1.2)
			(drill oval 1.4 0.45)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J25-Pin_2)")
			(pintype "passive")
		)
		(pad "T" thru_hole oval
			(at 5 -5)
			(size 1.2 2.2)
			(drill oval 0.45 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 187 "Net-(J25-Pin_3)")
			(pintype "passive")
		)
		(pad "TN" thru_hole oval
			(at 2.5 -5)
			(size 1.2 2.2)
			(drill oval 0.45 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 187 "Net-(J25-Pin_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3525N_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 56.31 36.25 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 3.2698 0.0048 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.samsungsem.com/resources/file/global/support/product_catalog/MLCC.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "10% or 20% 35V Ceramic Capacitor X6S 0805 (2012 Metric)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/samsung-electro-mechanics/CL21X106KAYNNNE/5961182"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectivity/")
		(sheetfile "connect.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "/Connectivity/VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:WA-SMSI_M2.5"
		(locked yes)
		(layer "B.Cu")
		(at 30 119 180)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H13"
			(at -0.01 -3.36 0)
			(layer "B.SilkS")
		)
		(property "Value" "Spacer"
			(at 0 -3.7 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/9774027151R.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "MIDI In"
			(at 60 238 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/9774027151R/5320625"
			(at 60 238 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 6 6)
			(drill 3.7)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(solder_paste_margin -0.2)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/spacer.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:WA-SMSI_M2.5"
		(locked yes)
		(layer "B.Cu")
		(at 105 67 180)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H9"
			(at 0.08 -2.98 0)
			(layer "B.SilkS")
		)
		(property "Value" "Spacer"
			(at 0 -3.7 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/9774027151R.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "MIDI In"
			(at 210 134 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/9774027151R/5320625"
			(at 210 134 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 6 6)
			(drill 3.7)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(solder_paste_margin -0.2)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/spacer.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:WA-SMSI_M2.5"
		(locked yes)
		(layer "B.Cu")
		(at 30 67 180)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H10"
			(at -0.04 -3.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "Spacer"
			(at 0 -3.7 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/9774027151R.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "MIDI In"
			(at 60 134 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/9774027151R/5320625"
			(at 60 134 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 6 6)
			(drill 3.7)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(solder_paste_margin -0.2)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/spacer.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:WA-SMSI_M2.5"
		(locked yes)
		(layer "B.Cu")
		(at 180 67 180)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H8"
			(at 0.16 -3.09 0)
			(layer "B.SilkS")
		)
		(property "Value" "Spacer"
			(at 0 -3.7 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/9774027151R.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "MIDI In"
			(at 360 134 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/9774027151R/5320625"
			(at 360 134 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 6 6)
			(drill 3.7)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(solder_paste_margin -0.2)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/spacer.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:WA-SMSI_M2.5"
		(locked yes)
		(layer "B.Cu")
		(at 105 119 180)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H12"
			(at 0.03 -2.95 0)
			(layer "B.SilkS")
		)
		(property "Value" "Spacer"
			(at 0 -3.7 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/9774027151R.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "MIDI In"
			(at 210 238 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/9774027151R/5320625"
			(at 210 238 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 6 6)
			(drill 3.7)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(solder_paste_margin -0.2)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/spacer.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical"
		(layer "B.Cu")
		(at 72.96 23.49)
		(descr "JST PH series connector, B3B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH side entry")
		(property "Reference" "J25"
			(at 0.14 2.86 180)
			(layer "B.SilkS")
		)
		(property "Value" "JST PH 3"
			(at 2 -4 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/jst-sales-america-inc/B3B-PH-K-S/926612"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Notes" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 2 -1.5 180)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 186 "Net-(J25-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J25-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 4 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 187 "Net-(J25-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:WA-SMSI_M2.5"
		(locked yes)
		(layer "B.Cu")
		(at 180 119 180)
		(descr "Mounting Hole 2.7mm, no annular, M2.5")
		(tags "mounting hole 2.7mm no annular m2.5")
		(property "Reference" "H11"
			(at -0.04 -3.06 0)
			(layer "B.SilkS")
		)
		(property "Value" "Spacer"
			(at 0 -3.7 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/9774027151R.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Notes" "MIDI In"
			(at 360 238 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/9774027151R/5320625"
			(at 360 238 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 6 6)
			(drill 3.7)
			(layers "*.Cu" "*.Mask" "B.Paste")
			(solder_paste_margin -0.2)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/spacer.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Pedalboard Library:Pedalboard_Soundcard"
		(layer "B.Cu")
		(at 120.25 68.3756 180)
		(descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 2x20 2.54mm double row")
		(property "Reference" "J27"
			(at -0.1096 -47.581238 0)
			(layer "B.SilkS")
		)
		(property "Value" "Pedalboard Soundcard"
			(at -3.45 -25.4 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader*2x20*P2.54mm*Vertical* PinSocket*2x20*P2.54mm*Vertical*")
		(sheetname "/Audio/")
		(sheetfile "audio.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 -24.13 90)
			(layer "F.Fab")
		)
		(dimension
			(type aligned)
			(layer "Dwgs.User")
			(pts
				(xy 118.98 63.5056) (xy 167.98 63.5056)
			)
			(height -7)
			(format
				(prefix "")
				(suffix "")
				(units 3)
				(units_format 1)
				(precision 4)
				(suppress_zeroes yes)
			)
			(style
				(thickness 0.1)
				(arrow_length 1.27)
				(text_position_mode 0)
				(arrow_direction outward)
				(extension_height 0.58642)
				(extension_offset 0.5)
				(keep_text_aligned yes)
			)
			(gr_text "49 mm"
				(at 143.48 55.3556 0)
				(layer "Dwgs.User")
			)
		)
		(dimension
			(type aligned)
			(layer "Dwgs.User")
			(pts
				(xy 118.98 63.5056) (xy 118.98 121.5056)
			)
			(height 11.5)
			(format
				(prefix "")
				(suffix "")
				(units 3)
				(units_format 1)
				(precision 4)
				(suppress_zeroes yes)
			)
			(style
				(thickness 0.1)
				(arrow_length 1.27)
				(text_position_mode 0)
				(arrow_direction outward)
				(extension_height 0.58642)
				(extension_offset 0.5)
				(keep_text_aligned yes)
			)
			(gr_text "58 mm"
				(at 106.33 92.5056 90)
				(layer "Dwgs.User")
			)
		)
		(dimension
			(type aligned)
			(layer "Dwgs.User")
			(pts
				(xy 118.98 125.0056) (xy 118.98 60.0056)
			)
			(height -16)
			(format
				(prefix "")
				(suffix "")
				(units 3)
				(units_format 1)
				(precision 4)
				(suppress_zeroes yes)
			)
			(style
				(thickness 0.1)
				(arrow_length 1.27)
				(text_position_mode 0)
				(arrow_direction outward)
				(extension_height 0.58642)
				(extension_offset 0.5)
				(keep_text_aligned yes)
			)
			(gr_text "65 mm"
				(at 101.83 92.5056 90)
				(layer "Dwgs.User")
			)
		)
		(dimension
			(type aligned)
			(layer "Dwgs.User")
			(pts
				(xy 118.98 92.5056) (xy 118.98 63.5056)
			)
			(height -7.5)
			(format
				(prefix "")
				(suffix "")
				(units 3)
				(units_format 1)
				(precision 4)
				(suppress_zeroes yes)
			)
			(style
				(thickness 0.1)
				(arrow_length 1.27)
				(text_position_mode 0)
				(arrow_direction outward)
				(extension_height 0.58642)
				(extension_offset 0.5)
				(keep_text_aligned yes)
			)
			(gr_text "29 mm"
				(at 110.33 78.0056 90)
				(layer "Dwgs.User")
			)
		)
		(dimension
			(type aligned)
			(layer "Dwgs.User")
			(pts
				(xy 167.98 63.5056) (xy 171.48 63.5056)
			)
			(height -7)
			(format
				(prefix "")
				(suffix "")
				(units 3)
				(units_format 1)
				(precision 4)
				(suppress_zeroes yes)
			)
			(style
				(thickness 0.1)
				(arrow_length 1.27)
				(text_position_mode 2)
				(arrow_direction outward)
				(extension_height 0.58642)
				(extension_offset 0.5)
				(keep_text_aligned yes)
			)
			(gr_text "3.5 mm"
				(at 170.98 54.5056 0)
				(layer "Dwgs.User")
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "/Audio/CM4_3V")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "+5VP")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 0 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/Audio/conf_i2c_sda")
			(pinfunction "SDA/GPIO2")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole oval
			(at 2.54 -2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "+5VP")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 0 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/Audio/conf_i2c_scl")
			(pinfunction "SCL/GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at 2.54 -5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" thru_hole oval
			(at 0 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "/Audio/CM4_GPIO4")
			(pinfunction "GCLK0/GPIO4")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at 2.54 -7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "/Audio/INT_MIDI_TX")
			(pinfunction "GPIO14/TXD")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at 0 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" thru_hole oval
			(at 2.54 -10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "/Audio/INT_MIDI_RX")
			(pinfunction "GPIO15/RXD")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at 0 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/Audio/CM4_GPIO17")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole oval
			(at 2.54 -12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/Audio/audio_pcm_clk")
			(pinfunction "GPIO18/PWM0")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole oval
			(at 0 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/Audio/audio_in_stereo")
			(pinfunction "GPIO27")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole oval
			(at 2.54 -15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" thru_hole oval
			(at 0 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "/Audio/CM4_GPIO22")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole oval
			(at 2.54 -17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "/Audio/CM4_GPIO23")
			(pinfunction "GPIO23")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole oval
			(at 0 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "/Audio/CM4_3V")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "18" thru_hole oval
			(at 2.54 -20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/Audio/CM4_GPIO24")
			(pinfunction "GPIO24")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole oval
			(at 0 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "/Audio/CM4_GPIO10")
			(pinfunction "MOSI0/GPIO10")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole oval
			(at 2.54 -22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "21" thru_hole oval
			(at 0 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "/Audio/CM4_GPIO9")
			(pinfunction "MISO0/GPIO9")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 2.54 -25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "/Audio/CM4_GPIO25")
			(pinfunction "GPIO25")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole oval
			(at 0 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "/Audio/CM4_GPIO11")
			(pinfunction "SCLK0/GPIO11")
			(pintype "bidirectional")
		)
		(pad "24" thru_hole oval
			(at 2.54 -27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "/Audio/CM4_GPIO8")
			(pinfunction "~{CE0}/GPIO8")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole oval
			(at 0 -30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "26" thru_hole oval
			(at 2.54 -30.48 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "/Audio/CM4_GPIO7")
			(pinfunction "~{CE1}/GPIO7")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole oval
			(at 0 -33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "/Audio/CM4_ID_SD")
			(pinfunction "ID_SD/GPIO0")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole oval
			(at 2.54 -33.02 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "/Audio/CM4_ID_SC")
			(pinfunction "ID_SC/GPIO1")
			(pintype "bidirectional")
		)
		(pad "29" thru_hole oval
			(at 0 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "/Audio/CM4_GPIO5")
			(pinfunction "GCLK1/GPIO5")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole oval
			(at 2.54 -35.56 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "31" thru_hole oval
			(at 0 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "/Audio/CM4_GPIO6")
			(pinfunction "GCLK2/GPIO6")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole oval
			(at 2.54 -38.1 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "/Audio/CM4_GPIO12")
			(pinfunction "PWM0/GPIO12")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole oval
			(at 0 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/Audio/CM4_GPIO13")
			(pinfunction "PWM1/GPIO13")
			(pintype "bidirectional")
		)
		(pad "34" thru_hole oval
			(at 2.54 -40.64 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "35" thru_hole oval
			(at 0 -43.18 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/Audio/audio_pcm_fs")
			(pinfunction "GPIO19/MISO1")
			(pintype "bidirectional")
		)
		(pad "36" thru_hole oval
			(at 2.54 -43.18 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/Audio/CM4_GPIO16")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "37" thru_hole oval
			(at 0 -45.72 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/Audio/audio_out_stereo")
			(pinfunction "GPIO26")
			(pintype "bidirectional")
		)
		(pad "38" thru_hole oval
			(at 2.54 -45.72 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/Audio/audio_pcm_din")
			(pinfunction "GPIO20/MOSI1")
			(pintype "bidirectional")
		)
		(pad "39" thru_hole oval
			(at 0 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" thru_hole oval
			(at 2.54 -48.26 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/Audio/audio_pcm_dout")
			(pinfunction "GPIO21/SCLK1")
			(pintype "bidirectional")
		)
		(pad "41" thru_hole rect
			(at -36.305 -6.47 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "/Audio/in_R-")
			(pinfunction "in_R-")
			(pintype "input")
		)
		(pad "42" thru_hole oval
			(at -33.765 -6.47 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "/Audio/in_R+")
			(pinfunction "in_R+")
			(pintype "input")
		)
		(pad "43" thru_hole oval
			(at -36.305 -9.01 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/Audio/GND_in_R")
			(pinfunction "in_GND")
			(pintype "input")
		)
		(pad "44" thru_hole oval
			(at -33.765 -9.01 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/Audio/GND_in_L")
			(pinfunction "in_GND")
			(pintype "input")
		)
		(pad "45" thru_hole oval
			(at -36.305 -11.55 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/Audio/in_L+")
			(pinfunction "in_L+")
			(pintype "input")
		)
		(pad "46" thru_hole oval
			(at -33.765 -11.55 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/Audio/in_L-")
			(pinfunction "in_L-")
			(pintype "input")
		)
		(pad "47" thru_hole rect
			(at -32.13 -50.775 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 215 "Net-(JP5-A)")
			(pinfunction "out_5V")
			(pintype "power_out")
		)
		(pad "48" thru_hole oval
			(at -32.13 -53.315 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 207 "Net-(J27-out_R)")
			(pinfunction "out_R")
			(pintype "output")
		)
		(pad "49" thru_hole oval
			(at -34.67 -50.775 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/Audio/GND_out")
			(pinfunction "out_GND")
			(pintype "input")
		)
		(pad "50" thru_hole oval
			(at -34.67 -53.315 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/Audio/GND_out")
			(pinfunction "out_GND")
			(pintype "input")
		)
		(pad "51" thru_hole oval
			(at -37.21 -50.775 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 214 "Net-(JP6-A)")
			(pinfunction "out_5V")
			(pintype "power_out")
		)
		(pad "52" thru_hole oval
			(at -37.21 -53.315 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 201 "Net-(J27-out_L)")
			(pinfunction "out_L")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d-models/pedalboard-soundcard-3D.step"
			(offset
				(xyz 57.25 57 7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical"
		(layer "B.Cu")
		(at 64.03 23.5)
		(descr "JST PH series connector, B3B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH side entry")
		(property "Reference" "J26"
			(at -4.055 1.6 180)
			(layer "B.SilkS")
		)
		(property "Value" "JST PH 3"
			(at 2 -4 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.jst-mfg.com/product/pdf/eng/ePH.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Supplier" "https://www.digikey.ch/en/products/detail/jst-sales-america-inc/B3B-PH-K-S/926612"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Notes" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/MIDI/")
		(sheetfile "pico.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 2 -1.5 180)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 189 "Net-(J26-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 4 0)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 191 "Net-(J26-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 122.2 20)
		(end 187 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 18 124)
		(end 18 27)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 23 131)
		(mid 22.292893 130.707107)
		(end 22 130)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 100 131)
		(mid 105 126)
		(end 110 131)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 23 131)
		(end 100 131)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 118.2 21.4)
		(mid 117.917157 21.282843)
		(end 117.8 21)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 110 20)
		(mid 105 25)
		(end 100 20)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 88.2 21.4)
		(mid 87.917158 21.282843)
		(end 87.8 21)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 188 130)
		(mid 187.707107 130.707107)
		(end 187 131)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.2 21.4)
		(end 121.799998 21.400002)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 191 26)
		(mid 188.87868 25.12132)
		(end 188 23)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 19 125)
		(mid 18.292893 124.707107)
		(end 18 124)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 18 27)
		(mid 18.292893 26.292893)
		(end 19 26)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 191 26)
		(mid 191.707107 26.292893)
		(end 192 27)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 110 20)
		(end 117.8 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 192 27)
		(end 192 124)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 19 125)
		(mid 21.12132 125.87868)
		(end 22 128)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188 128)
		(end 188 130)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 117.8 20)
		(end 117.8 21)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.2 21)
		(end 92.2 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188 21)
		(end 188 23)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.2 20)
		(end 100 20)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 92.2 21)
		(mid 92.082843 21.282842)
		(end 91.8 21.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.8 20)
		(end 87.8 21)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 22 23)
		(mid 21.12132 25.12132)
		(end 19 26)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.2 21.4)
		(end 91.8 21.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 22 21)
		(mid 22.292893 20.292893)
		(end 23 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.8 20)
		(end 23 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 22 21)
		(end 22 23)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 122.2 21)
		(mid 122.082842 21.282843)
		(end 121.799998 21.400002)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 192 124)
		(mid 191.707107 124.707107)
		(end 191 125)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 122.2 21)
		(end 122.2 20)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 110 131)
		(end 187 131)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 22 128)
		(end 22 130)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 188 128)
		(mid 188.87868 125.87868)
		(end 191 125)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 187 20)
		(mid 187.707107 20.292893)
		(end 188 21)
		(layer "Edge.Cuts")
	)
	(gr_text "IN L"
		(at 165.06 99.49 -90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GAIN"
		(at 133.6 25.1 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "A"
		(at 18.6858 116.774 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "EXP 2"
		(at 44.78 46.17 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "B"
		(at 94.0222 115.4278 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "C"
		(at 188.815 116.9772 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "RX TX GND"
		(at 101.19 84.14 0)
		(layer "F.SilkS")
	)
	(gr_text "MIDI\nOUT"
		(at 106.28 30.48 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "DATA\n+5V\nGND\n"
		(at 134.586 68.26 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "${TITLE}\n${COMPANY}\nPCB: ${REVISION} ${GIT_HASH}"
		(at 67.67 122.5 0)
		(layer "F.SilkS")
	)
	(gr_text "reset"
		(at 121.86 42.31 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "D"
		(at 18.7366 64.7802 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "bootsel"
		(at 88.57 59.08 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "IN R"
		(at 164.97 79.59 -90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "EXP 1"
		(at 165.3 36.85 -90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "SWCLK GND SWD"
		(at 126.76 43.07 0)
		(layer "F.SilkS")
	)
	(gr_text "OUT L"
		(at 44.79 107.88 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "OLED OUT"
		(at 142.079 62.799 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "LED OUT"
		(at 133.4684 62.8244 -0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "F\n"
		(at 189.196 63.6626 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "OUT R"
		(at 44.76 87.68 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "MIDI\n IN\n"
		(at 100.68 30.48 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "E"
		(at 113.0722 63.561 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "VOL"
		(at 58.52 24.81 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND\n+3V3\nSDA\nSCL\n"
		(at 143.5268 69.4284 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 22.37 44.27 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "IN"
		(at 79.02 27.08 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 188.99 36.29 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "${TITLE}\n${COMPANY}\nPCB: ${REVISION} ${GIT_HASH}"
		(at 90.5 123.2 0)
		(layer "B.SilkS")
	)
	(gr_text "VREF"
		(at 35.12 43.84 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "MIDI"
		(at 60.88 23.3 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "in"
		(at 134.4408 56.8516 90)
		(layer "B.SilkS")
	)
	(gr_text "IN"
		(at 182.55 36.09 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "OUT"
		(at 64.59 27.32 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "IN"
		(at 28.69 45.85 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "VREF"
		(at 176.1 36.09 90)
		(layer "B.SilkS" knockout)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 30 119) (xy 105 119)
		)
		(height 22.999999)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "75.0000 mm"
			(at 67.5 140.849999 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 185.005615 22.994385) (xy 192 23)
		)
		(height -8.4)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 1)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "7 mm"
			(at 188.510474 13.447196 359.9539955)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 142.5 34) (xy 142.5 67)
		)
		(height -56.5)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "33 mm"
			(at 197.85 50.5 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 179.66 119) (xy 179.66 131)
		)
		(height -19.34)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "12 mm"
			(at 198 124.1 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 24.4874 22.9972) (xy 24.4874 19.9972)
		)
		(height 7)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3 mm"
			(at 33.618014 22.4972 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 67.5 48) (xy 92.5 48)
		)
		(height 3.999999)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "25.0000 mm"
			(at 80 50.849999 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 80 19.994385) (xy 130 19.994385)
		)
		(height -2.494385)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "50 mm"
			(at 105 16.35 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 195.42 105.61) (xy 14.58 105.61)
		)
		(height -42.19)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "180.84 mm"
			(at 105 146.65 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 180 67) (xy 180 119)
		)
		(height -19)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "52 mm"
			(at 197.85 93 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 187 20) (xy 187 131)
		)
		(height -14.2)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "111 mm"
			(at 200.05 75.5 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 18 125) (xy 192 125)
		)
		(height 20.05)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "174 mm"
			(at 105 143.9 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 25 23) (xy 185.005615 22.994385)
		)
		(height -8.5)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 1)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "160 mm"
			(at 105.00247 13.347192 0.002011011274)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 75)
		(net_name "+5VP")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.1)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 89.5 73.5) (xy 92.5 73.5) (xy 92.5 80.15) (xy 89.5 80.15)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52.5 73.5) (xy 52.5 96.5) (xy 59 96.5) (xy 59 73.5)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 86 73.5) (xy 86 96.5) (xy 92.5 96.5) (xy 92.5 80.5) (xy 89.5 80.5) (xy 89.5 73.5)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "power-in-gnd")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.5 22) (xy 153.75 22.25) (xy 152.2204 23.546) (xy 151.9 53.92) (xy 170.15 53.67) (xy 170.1 32.3)
				(xy 184.5 32.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 58.005615 20) (xy 18 20) (xy 18.005615 130.994385) (xy 192.005615 130.994385) (xy 192.005615 19.994385)
				(xy 130 19.994385) (xy 130 36) (xy 80 36) (xy 80 19.994385)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Audio/GND_out")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.35)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52 129) (xy 42 115) (xy 21 115) (xy 21 72) (xy 42 72) (xy 42 104) (xy 53 115) (xy 88 115) (xy 97 122)
				(xy 125 122) (xy 131 115) (xy 163 115) (xy 163 129)
			)
		)
	)
	(zone
		(net 66)
		(net_name "/Audio/GND_in_R")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 155.152834 76) (xy 149.274311 76) (xy 149.2 71.7) (xy 152.7 68.1) (xy 169 68) (xy 173 72) (xy 190 72)
				(xy 190 93.1) (xy 171.5 93.1) (xy 157.8 78.85) (xy 156 78)
			)
		)
	)
	(zone
		(net 69)
		(net_name "/Audio/GND_in_L")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 157.8 78.85) (xy 155.152834 76) (xy 149.274311 76) (xy 149.25 91) (xy 171 113) (xy 190 113)
				(xy 190 93.1) (xy 171.5 93.1)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 58 20) (xy 18 20) (xy 18 131) (xy 192 131) (xy 192 20) (xy 130 20) (xy 130 36) (xy 130 36.00225)
				(xy 80 36) (xy 80 20)
			)
		)
	)
	(embedded_fonts no)
)
