(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Open Pedalboard")
    (date "2023-03-12")
    (rev "2.0.0")
    (company "https://github.com/pedalboard")
    (comment 1 "Source Code: https://github.com/pedalboard/pedalboard-hw")
    (comment 2 "License: CERN Open Hardware Licence Version 2 - Permissive")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 20 125)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+3.3V")
  (net 3 "Net-(D1-DOUT)")
  (net 4 "/MIDI/RGB_DATA")
  (net 5 "Net-(D2-DOUT)")
  (net 6 "Net-(D3-DOUT)")
  (net 7 "Net-(D4-DOUT)")
  (net 8 "Net-(D5-DOUT)")
  (net 9 "Net-(D6-DOUT)")
  (net 10 "Net-(D7-DOUT)")
  (net 11 "Net-(D8-DOUT)")
  (net 12 "Net-(D10-DIN)")
  (net 13 "Net-(D10-DOUT)")
  (net 14 "Net-(D11-K)")
  (net 15 "Net-(D11-A)")
  (net 16 "Net-(U1-GPIO28_ADC2)")
  (net 17 "Net-(U1-AGND)")
  (net 18 "unconnected-(J3-PadSN)")
  (net 19 "Net-(U1-ADC_VREF)")
  (net 20 "unconnected-(J3-PadTN)")
  (net 21 "/Audio/INT_MIDI_TX")
  (net 22 "/Audio/INT_MIDI_RX")
  (net 23 "Net-(J7-3V3-Pad1)")
  (net 24 "/Audio/conf_i2c_sda")
  (net 25 "/Audio/conf_i2c_scl")
  (net 26 "Net-(J7-GCLK0{slash}GPIO4)")
  (net 27 "/MIDI/EXT_MIDI_RX")
  (net 28 "/MIDI/EXT_MIDI_TX")
  (net 29 "Net-(J7-GPIO17)")
  (net 30 "/Audio/audio_pcm_clk")
  (net 31 "/Audio/audio_in_stereo")
  (net 32 "Net-(J7-GPIO22)")
  (net 33 "unconnected-(U1-GPIO10-Pad14)")
  (net 34 "unconnected-(U1-GPIO12-Pad16)")
  (net 35 "unconnected-(U1-GPIO13-Pad17)")
  (net 36 "unconnected-(U1-GPIO14-Pad19)")
  (net 37 "unconnected-(U1-GPIO15-Pad20)")
  (net 38 "unconnected-(U1-GPIO22-Pad29)")
  (net 39 "unconnected-(U1-RUN-Pad30)")
  (net 40 "unconnected-(U1-GPIO26_ADC0-Pad31)")
  (net 41 "unconnected-(U1-GPIO27_ADC1-Pad32)")
  (net 42 "unconnected-(U1-3V3_EN-Pad37)")
  (net 43 "+5VD")
  (net 44 "/Audio/USB_DN")
  (net 45 "unconnected-(U2-Pad3)")
  (net 46 "Net-(J7-GPIO23)")
  (net 47 "Net-(J7-3V3-Pad17)")
  (net 48 "Net-(J7-GPIO24)")
  (net 49 "Net-(J7-MOSI0{slash}GPIO10)")
  (net 50 "Net-(J7-MISO0{slash}GPIO9)")
  (net 51 "Net-(J7-GPIO25)")
  (net 52 "Net-(J7-SCLK0{slash}GPIO11)")
  (net 53 "Net-(J7-~{CE0}{slash}GPIO8)")
  (net 54 "Net-(J7-~{CE1}{slash}GPIO7)")
  (net 55 "Net-(J7-ID_SD{slash}GPIO0)")
  (net 56 "Net-(J7-ID_SC{slash}GPIO1)")
  (net 57 "Net-(J7-GCLK1{slash}GPIO5)")
  (net 58 "Net-(J7-GCLK2{slash}GPIO6)")
  (net 59 "Net-(J7-PWM0{slash}GPIO12)")
  (net 60 "Net-(J7-PWM1{slash}GPIO13)")
  (net 61 "/Audio/audio_pcm_fs")
  (net 62 "Net-(J7-GPIO16)")
  (net 63 "/Audio/audio_out_stereo")
  (net 64 "/Audio/audio_pcm_din")
  (net 65 "/Audio/audio_pcm_dout")
  (net 66 "unconnected-(J9-PadSN)")
  (net 67 "unconnected-(J11-PadR)")
  (net 68 "unconnected-(J11-PadRN)")
  (net 69 "unconnected-(J11-PadSN)")
  (net 70 "unconnected-(J8-out_5V-Pad47)")
  (net 71 "unconnected-(J11-PadTN)")
  (net 72 "unconnected-(J12-PadR)")
  (net 73 "unconnected-(J12-PadRN)")
  (net 74 "Net-(J8-out_R)")
  (net 75 "unconnected-(J12-PadTN)")
  (net 76 "unconnected-(J8-out_5V-Pad51)")
  (net 77 "Net-(J8-out_L)")
  (net 78 "/MIDI/SW_D")
  (net 79 "/MIDI/SW_E")
  (net 80 "/MIDI/SW_F")
  (net 81 "/MIDI/SW_A")
  (net 82 "/MIDI/SW_B")
  (net 83 "/MIDI/SW_C")
  (net 84 "/MIDI/ROT_VOL_A")
  (net 85 "/MIDI/ROT_VOL_B")
  (net 86 "/MIDI/SW_VOL")
  (net 87 "/MIDI/ROT_GAIN_A")
  (net 88 "/MIDI/ROT_GAIN_B")
  (net 89 "/MIDI/SW_GAIN")
  (net 90 "unconnected-(J1-Pad1)")
  (net 91 "unconnected-(J1-Pad3)")
  (net 92 "unconnected-(J2-Pad1)")
  (net 93 "unconnected-(J2-Pad3)")
  (net 94 "Net-(L1-Pad2)")
  (net 95 "Net-(L3-Pad2)")
  (net 96 "Net-(L4-Pad2)")
  (net 97 "Net-(J15-Pin_2)")
  (net 98 "Net-(J15-Pin_6)")
  (net 99 "Net-(J15-Pin_4)")
  (net 100 "Net-(J15-Pin_3)")
  (net 101 "Net-(J15-Pin_1)")
  (net 102 "/Audio/USB_DP")
  (net 103 "Net-(D1-DIN)")
  (net 104 "/Audio/in_R-")
  (net 105 "/Audio/GND_in_R")
  (net 106 "/Audio/in_R+")
  (net 107 "/Audio/in_L-")
  (net 108 "/Audio/GND_in_L")
  (net 109 "/Audio/in_L+")
  (net 110 "/Audio/GND_out")
  (net 111 "unconnected-(PS1-CTRL-Pad1)")
  (net 112 "unconnected-(PS1-TRIM-Pad5)")
  (net 113 "/Power Supply/fused")
  (net 114 "+5VP")
  (net 115 "/Power Supply/power_input_gnd")
  (net 116 "Net-(J7-5V-Pad4)")
  (net 117 "/VBUS")
  (net 118 "unconnected-(J13-Pad3)")
  (net 119 "/Power Supply/vin")
  (net 120 "/MIDI/VSYS")
  (net 121 "/Power Supply/unfused")
  (net 122 "/MIDI/VBUS_FILTERED")
  (net 123 "Net-(U1-GPIO8)")
  (net 124 "Net-(U1-GPIO9)")
  (net 125 "Net-(F4-Pad1)")
  (net 126 "Net-(F5-Pad1)")
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 168.02 121.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at -2.76 -0.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (at 146.8 46.7 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 1.46 -2.445 -180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.35 -0.1 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:Jack_3.5mm_CUI_SJ1-3525N_Horizontal" locked (layer "F.Cu")
    (at 116 24.5 180)
    (descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
    (tags "TRS audio jack stereo horizontal")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/cui-devices/SJ1-3525NG/738690")
    (property "ki_description" "Audio Jack, 3 Poles (Stereo / TRS), Switched TR Poles (Normalling)")
    (property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "J16" (at -7 -1.7 270) (layer "F.SilkS"))
    (fp_text value "MIDI OUT J" (at 0 -10 180) (layer "F.Fab"))
    (fp_text user "PCB edge" (at 0 3.65 180 unlocked) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 180) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5 0 180) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "" np_thru_hole circle locked (at 0 -5 180) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "" np_thru_hole circle locked (at 5 0 180) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "R" thru_hole oval locked (at -5 -5 180) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask")
      (net 98 "Net-(J15-Pin_6)") (pintype "passive"))
    (pad "RN" thru_hole oval locked (at -2.5 -5 180) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask")
      (net 98 "Net-(J15-Pin_6)") (pintype "passive"))
    (pad "S" thru_hole oval locked (at 0 0 180) (size 2.2 1.2) (drill oval 1.4 0.4) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "T" thru_hole oval locked (at 5 -5) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask")
      (net 99 "Net-(J15-Pin_4)") (pintype "passive"))
    (pad "TN" thru_hole oval locked (at 2.5 -5) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask")
      (net 99 "Net-(J15-Pin_4)") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/jack3.5mm.x3d"
      (offset (xyz 0 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 133 23)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Sheetfile" "pedalboard-hw.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 3.245 0) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Pedalboard Library:Jack_6.35mm_Horizontal" locked (layer "F.Cu")
    (at 34.4 111.2 180)
    (descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
    (tags "neutrik jack m")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235")
    (property "ki_description" "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins")
    (property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik")
    (attr through_hole)
    (fp_text reference "J12" (at 6.35 -3 180) (layer "F.SilkS"))
    (fp_text value "Audio OUT Left" (at 6.35 19 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 8.115 180) (layer "F.Fab"))
    (pad "R" thru_hole circle locked (at 6.35 0 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 72 "unconnected-(J12-PadR)") (pintype "passive+no_connect"))
    (pad "RN" thru_hole circle locked (at 6.35 16.23 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 73 "unconnected-(J12-PadRN)") (pintype "passive+no_connect"))
    (pad "S" thru_hole circle locked (at 12.7 0 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 110 "/Audio/GND_out") (pintype "passive"))
    (pad "SN" thru_hole circle locked (at 12.7 16.23 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 125 "Net-(F4-Pad1)") (pintype "passive"))
    (pad "T" thru_hole circle locked (at 0 0 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 77 "Net-(J8-out_L)") (pintype "passive"))
    (pad "TN" thru_hole circle locked (at 0 16.23 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 75 "unconnected-(J12-PadTN)") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
      (offset (xyz 16.5 -8 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 158.6376 44.6)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/kemet/C322C475K5R5TA/3726055")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C16" (at -2.9 0.1 180) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 2.5 2.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 113 "/Power Supply/fused") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 115 "/Power Supply/power_input_gnd") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:BarrelJack_Wuerth_6941xx301002" (layer "F.Cu")
    (at 179.4 30.4 180)
    (descr "Wuerth electronics barrel jack connector (5.5mm outher diameter, inner diameter 2.05mm or 2.55mm depending on exact order number), See: http://katalog.we-online.de/em/datasheet/6941xx301002.pdf")
    (tags "connector barrel jack")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/694106301002/5047522")
    (property "ki_description" "DC Barrel Jack with an internal switch")
    (property "ki_keywords" "DC power barrel jack connector")
    (attr through_hole)
    (fp_text reference "J13" (at -6.5 -0.8 180) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack_MountingPin" (at 0 15.5 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 7.5 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 4.4 1.8) (drill oval 3.4 0.8) (layers "*.Cu" "*.Mask")
      (net 115 "/Power Supply/power_input_gnd") (pintype "power_out"))
    (pad "2" thru_hole oval (at 0 5.8 180) (size 4 1.8) (drill oval 3 0.8) (layers "*.Cu" "*.Mask")
      (net 121 "/Power Supply/unfused") (pintype "power_out"))
    (pad "3" thru_hole oval (at 4.8 3 270) (size 4 1.8) (drill oval 3 0.8) (layers "*.Cu" "*.Mask")
      (net 118 "unconnected-(J13-Pad3)") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/3d-models/694106301002 (rev1).stp"
      (offset (xyz 0 -10 5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2" (layer "F.Cu")
    (at 130.7 46.82 -90)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=6.6*2.7mm^2, Vishay, IM-2, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 10.16mm  length 6.6mm diameter 2.7mm Vishay IM-2")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/fair-rite-products-corp/2743005111/8599429")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L5" (at 0.68 -2.3 -180) (layer "F.SilkS"))
    (fp_text value "103_100MHz" (at 5.08 2.47 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 122 "/MIDI/VBUS_FILTERED") (pinfunction "1") (pintype "power_out"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 117 "/VBUS") (pinfunction "2") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:LED_D5.0mm-NeoPixel" locked (layer "F.Cu")
    (at 115.6 48)
    (descr "LED, diameter 5.0mm, 4 pins, WP154A4,https://www.adafruit.com/product/1938")
    (tags "LED diameter 5.0mm neopixel adafruit")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/sparkfun-electronics/COM-12999/5673800")
    (property "ki_description" "RGB LED with integrated controller, 5mm/8mm LED package")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr through_hole)
    (fp_text reference "D3" (at 1.905 -3.96) (layer "F.SilkS"))
    (fp_text value "NEOPIX" (at 1.905 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.905 -3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D2-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D3-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:Jack_6.35mm_Horizontal" locked (layer "F.Cu")
    (at 34.435 91 180)
    (descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
    (tags "neutrik jack m")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235")
    (property "ki_description" "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins")
    (property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik")
    (attr through_hole)
    (fp_text reference "J11" (at 6.35 -3 180) (layer "F.SilkS"))
    (fp_text value "Audio OUT Right" (at 6.35 19 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 8.115 180) (layer "F.Fab"))
    (pad "R" thru_hole circle locked (at 6.35 0 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 67 "unconnected-(J11-PadR)") (pintype "passive+no_connect"))
    (pad "RN" thru_hole circle locked (at 6.35 16.23 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 68 "unconnected-(J11-PadRN)") (pintype "passive+no_connect"))
    (pad "S" thru_hole circle locked (at 12.7 0 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 110 "/Audio/GND_out") (pintype "passive"))
    (pad "SN" thru_hole circle locked (at 12.7 16.23 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 69 "unconnected-(J11-PadSN)") (pintype "passive+no_connect"))
    (pad "T" thru_hole circle locked (at 0 0 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(J8-out_R)") (pintype "passive"))
    (pad "TN" thru_hole circle locked (at 0 16.23 180) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 71 "unconnected-(J11-PadTN)") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
      (offset (xyz 16.5 -8 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Pedalboard Library:CONV_PDQE15-Q24-S5-D" (layer "F.Cu")
    (at 134.8 81.68 -90)
    (descr "DC-DC Converter 24V/5V 15W")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/cui-inc/PDQE15-Q24-S5-D/10230147")
    (attr through_hole)
    (fp_text reference "PS1" (at -8.89 -13.97 -90) (layer "F.SilkS"))
    (fp_text value "PDQE15-Q24-S5-D" (at 0.635 13.97 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -10.16 -10.16 270) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 111 "unconnected-(PS1-CTRL-Pad1)") (pinfunction "CTRL") (pintype "input+no_connect"))
    (pad "2" thru_hole circle (at -10.16 -2.54 270) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 115 "/Power Supply/power_input_gnd") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at -10.16 2.54 270) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 119 "/Power Supply/vin") (pinfunction "VIN") (pintype "input"))
    (pad "4" thru_hole circle (at 10.16 10.16 270) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 43 "+5VD") (pinfunction "+VO") (pintype "power_out"))
    (pad "5" thru_hole circle (at 10.16 0 270) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 112 "unconnected-(PS1-TRIM-Pad5)") (pinfunction "TRIM") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 10.16 -10.16 270) (size 2.25 2.25) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "0V") (pintype "power_out"))
    (model "${KIPRJMOD}/3d-models/PDQE15-Q24-S5-D.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Pedalboard Library:Jack_6.35mm_Horizontal" locked (layer "F.Cu")
    (at 175.6 94.995)
    (descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
    (tags "neutrik jack m")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235")
    (property "ki_description" "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins")
    (property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik")
    (attr through_hole)
    (fp_text reference "J10" (at -5.8 1.705) (layer "F.SilkS"))
    (fp_text value "Audio IN Left" (at 6.35 19) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 8.115) (layer "F.Fab"))
    (pad "R" thru_hole circle locked (at 6.35 0) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 107 "/Audio/in_L-") (pintype "passive"))
    (pad "RN" thru_hole circle locked (at 6.35 16.23) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 108 "/Audio/GND_in_L") (pintype "passive"))
    (pad "S" thru_hole circle locked (at 12.7 0) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 108 "/Audio/GND_in_L") (pintype "passive"))
    (pad "SN" thru_hole circle locked (at 12.7 16.23) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 126 "Net-(F5-Pad1)") (pintype "passive"))
    (pad "T" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 109 "/Audio/in_L+") (pintype "passive"))
    (pad "TN" thru_hole circle locked (at 0 16.23) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 108 "/Audio/GND_in_L") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
      (offset (xyz 16.5 -8 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Pedalboard Library:Trace_Fuse" (layer "F.Cu")
    (at 95.97 113.2)
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Fuse, small symbol")
    (property "ki_keywords" "fuse")
    (attr smd)
    (fp_text reference "F4" (at 0 -2.9 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0.1 3.6 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1 5.1 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.3 0) (size 2.286 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(F4-Pad1)") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 1.3 0) (size 2.286 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/Audio/audio_out_stereo") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 42 63.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Sheetfile" "pedalboard-hw.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 2 2.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Pedalboard Library:LED_D5.0mm-NeoPixel" locked (layer "F.Cu")
    (at 140.6 48)
    (descr "LED, diameter 5.0mm, 4 pins, WP154A4,https://www.adafruit.com/product/1938")
    (tags "LED diameter 5.0mm neopixel adafruit")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/sparkfun-electronics/COM-12999/5673800")
    (property "ki_description" "RGB LED with integrated controller, 5mm/8mm LED package")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr through_hole)
    (fp_text reference "D4" (at 1.905 -3.96) (layer "F.SilkS"))
    (fp_text value "NEOPIX" (at 1.905 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.905 -3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D3-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D4-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (at 109.31 104.93 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C10" (at -1.63 -1.49 -180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:LED_D5.0mm-NeoPixel" locked (layer "F.Cu")
    (at 103.1 106)
    (descr "LED, diameter 5.0mm, 4 pins, WP154A4,https://www.adafruit.com/product/1938")
    (tags "LED diameter 5.0mm neopixel adafruit")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/sparkfun-electronics/COM-12999/5673800")
    (property "ki_description" "RGB LED with integrated controller, 5mm/8mm LED package")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr through_hole)
    (fp_text reference "D7" (at -0.3 -3.6) (layer "F.SilkS"))
    (fp_text value "NEOPIX" (at 1.905 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.905 -3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D6-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D7-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 118.98 121.52)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 3.52 -1.22) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Pedalboard Library:Raspberry PI Compute Module CM4 Nano A" (layer "F.Cu")
    (at 49.59 106.32 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/61304021121/4846886")
    (property "ki_description" "expansion header for Raspberry Pi 2 & 3")
    (property "ki_keywords" "raspberrypi gpio")
    (attr through_hole)
    (fp_text reference "J7" (at -3.28 0.11 180) (layer "B.SilkS"))
    (fp_text value "Raspberry_pi" (at 1.27 50.59 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 24.13) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(J7-3V3-Pad1)") (pinfunction "3V3") (pintype "power_out"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 114 "+5VP") (pinfunction "5V") (pintype "power_in"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/Audio/conf_i2c_sda") (pinfunction "SDA/GPIO2") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 116 "Net-(J7-5V-Pad4)") (pinfunction "5V") (pintype "power_out"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "/Audio/conf_i2c_scl") (pinfunction "SCL/GPIO3") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(J7-GCLK0{slash}GPIO4)") (pinfunction "GCLK0/GPIO4") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/Audio/INT_MIDI_TX") (pinfunction "GPIO14/TXD") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "10" thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/Audio/INT_MIDI_RX") (pinfunction "GPIO15/RXD") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(J7-GPIO17)") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "/Audio/audio_pcm_clk") (pinfunction "GPIO18/PWM0") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "/Audio/audio_in_stereo") (pinfunction "GPIO27") (pintype "bidirectional"))
    (pad "14" thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "15" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(J7-GPIO22)") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(J7-GPIO23)") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "17" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(J7-3V3-Pad17)") (pinfunction "3V3") (pintype "power_out"))
    (pad "18" thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(J7-GPIO24)") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "19" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(J7-MOSI0{slash}GPIO10)") (pinfunction "MOSI0/GPIO10") (pintype "bidirectional"))
    (pad "20" thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "21" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(J7-MISO0{slash}GPIO9)") (pinfunction "MISO0/GPIO9") (pintype "bidirectional"))
    (pad "22" thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(J7-GPIO25)") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "23" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(J7-SCLK0{slash}GPIO11)") (pinfunction "SCLK0/GPIO11") (pintype "bidirectional"))
    (pad "24" thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "Net-(J7-~{CE0}{slash}GPIO8)") (pinfunction "~{CE0}/GPIO8") (pintype "bidirectional"))
    (pad "25" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "26" thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(J7-~{CE1}{slash}GPIO7)") (pinfunction "~{CE1}/GPIO7") (pintype "bidirectional"))
    (pad "27" thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(J7-ID_SD{slash}GPIO0)") (pinfunction "ID_SD/GPIO0") (pintype "bidirectional"))
    (pad "28" thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(J7-ID_SC{slash}GPIO1)") (pinfunction "ID_SC/GPIO1") (pintype "bidirectional"))
    (pad "29" thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(J7-GCLK1{slash}GPIO5)") (pinfunction "GCLK1/GPIO5") (pintype "bidirectional"))
    (pad "30" thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "31" thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(J7-GCLK2{slash}GPIO6)") (pinfunction "GCLK2/GPIO6") (pintype "bidirectional"))
    (pad "32" thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 59 "Net-(J7-PWM0{slash}GPIO12)") (pinfunction "PWM0/GPIO12") (pintype "bidirectional"))
    (pad "33" thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(J7-PWM1{slash}GPIO13)") (pinfunction "PWM1/GPIO13") (pintype "bidirectional"))
    (pad "34" thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "/Audio/audio_pcm_fs") (pinfunction "GPIO19/MISO1") (pintype "bidirectional"))
    (pad "36" thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(J7-GPIO16)") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "37" thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "/Audio/audio_out_stereo") (pinfunction "GPIO26") (pintype "bidirectional"))
    (pad "38" thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/Audio/audio_pcm_din") (pinfunction "GPIO20/MOSI1") (pintype "bidirectional"))
    (pad "39" thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "40" thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "/Audio/audio_pcm_dout") (pinfunction "GPIO21/SCLK1") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3d-models/CM4-NANO-A.step"
      (offset (xyz -278.638 165.1 -7.62))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${KIPRJMOD}/3d-models/cm-min.step"
      (offset (xyz 37.5 4 -11))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 90))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (at 161.62 107.3 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C11" (at 1.26 -2.01 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.2 0.1 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:MIDI bites" (layer "F.Cu")
    (at 105.1 20.075)
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (fp_text reference "H10" (at -23.4 15.225 unlocked) (layer "F.SilkS"))
    (fp_text value "Midi Bites" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -25 1) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 2) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 3) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 4) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 5) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 6) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 10) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 11) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 12) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 13) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 14) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 15) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -25 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -24 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -23 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -22 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -21 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -20 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -19 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -18 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -17 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -15 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -14 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -13 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -12 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -11 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -10 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -9 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -8 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -7 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -5 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -4 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -3 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -2 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at -1 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 0 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 1 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 2 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 3 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 4 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 5 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 7 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 8 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 9 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 10 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 11 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 12 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 13 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 14 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 15 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 17 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 18 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 19 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 20 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 21 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 22 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 23 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 24 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 1) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 2) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 3) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 4) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 5) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 6) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 7) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 8) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 9) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 10) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 11) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 12) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 13) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 14) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 15) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
    (pad "" np_thru_hole circle (at 25 16) (size 0.6 0.6) (drill 0.5) (layers "*.Mask"))
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (at 44.155 101.7 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C9" (at 1.2 2.595 180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth-430476085716" locked (layer "F.Cu")
    (at 98.75 64.5)
    (descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430466043726/5209037")
    (property "ki_description" "Omron B3FS 6x6mm single pole normally-open tactile switch")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW2" (at 6.35 -4.66) (layer "F.SilkS"))
    (fp_text value "E" (at 6.35 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 79 "/MIDI/SW_E") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole oval locked (at 12.5 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 79 "/MIDI/SW_E") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.5 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/430476085716_Download_STP_430476085716_rev1.stp"
      (offset (xyz 6 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:LED_D5.0mm-NeoPixel" locked (layer "F.Cu")
    (at 42.1 79)
    (descr "LED, diameter 5.0mm, 4 pins, WP154A4,https://www.adafruit.com/product/1938")
    (tags "LED diameter 5.0mm neopixel adafruit")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/sparkfun-electronics/COM-12999/5673800")
    (property "ki_description" "RGB LED with integrated controller, 5mm/8mm LED package")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr through_hole)
    (fp_text reference "D9" (at -0.1 -3.5) (layer "F.SilkS"))
    (fp_text value "NEOPIX" (at 1.905 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.905 -3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D8-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D10-DIN)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" placed (layer "F.Cu")
    (at 74.575 53.105 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/koa-speer-electronics-inc/CF1-4C471J/13537235")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 2.515 2.565 180) (layer "F.SilkS"))
    (fp_text value "470" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/MIDI/RGB_DATA") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 103 "Net-(D1-DIN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-6_W7.62mm_LongPads" placed (layer "F.Cu")
    (at 69.475 65.8 180)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/onsemi/H11L1M/284866")
    (property "ki_description" "Schmitt Trigger Output Optocoupler, High Speed, DIP-6, 1.6mA turn on threshold")
    (property "ki_keywords" "High Speed Schmitt Optocoupler")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "H11L1" (at 3.81 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D11-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D11-A)") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(U2-Pad3)") (pintype "no_connect"))
    (pad "4" thru_hole oval (at 7.62 5.08 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "/MIDI/EXT_MIDI_RX") (pintype "output"))
    (pad "5" thru_hole oval (at 7.62 2.54 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "power_in"))
    (pad "6" thru_hole oval (at 7.62 0 180) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 77 23)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Sheetfile" "pedalboard-hw.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 1.5 3) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Inductor_THT:L_Radial_D12.0mm_P5.00mm_Fastron_11P" (layer "F.Cu")
    (at 161.9 50.3 -90)
    (descr "Inductor, Radial series, Radial, pin pitch=5.00mm, , diameter=12.0mm, Fastron, 11P, http://cdn-reichelt.de/documents/datenblatt/B400/DS_11P.pdf")
    (tags "Inductor Radial series Radial pin pitch 5.00mm  diameter 12.0mm Fastron 11P")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/7447471022/2794428")
    (property "ki_description" "Inductor")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L6" (at 9.9 0.4 -180) (layer "F.SilkS"))
    (fp_text value "2.2uH" (at 2.5 7.25 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 113 "/Power Supply/fused") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 2.6 2.6) (drill 1.3) (layers "*.Cu" "*.Mask")
      (net 119 "/Power Supply/vin") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Radial_D12.0mm_P5.00mm_Fastron_11P.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:Jack_6.35mm_Horizontal" locked (layer "F.Cu")
    (at 175.615 33.8)
    (descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
    (tags "neutrik jack m")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235")
    (property "ki_description" "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins")
    (property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik")
    (attr through_hole)
    (fp_text reference "J3" (at -5.515 1.9) (layer "F.SilkS"))
    (fp_text value "EXP" (at 6.35 19) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 8.115) (layer "F.Fab"))
    (pad "R" thru_hole circle locked (at 6.35 0) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(U1-GPIO28_ADC2)") (pintype "passive"))
    (pad "RN" thru_hole circle locked (at 6.35 16.23) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(U1-AGND)") (pintype "passive"))
    (pad "S" thru_hole circle locked (at 12.7 0) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(U1-AGND)") (pintype "passive"))
    (pad "SN" thru_hole circle locked (at 12.7 16.23) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(J3-PadSN)") (pintype "passive+no_connect"))
    (pad "T" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(U1-ADC_VREF)") (pintype "passive"))
    (pad "TN" thru_hole circle locked (at 0 16.23) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(J3-PadTN)") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
      (offset (xyz 16.5 -8 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" placed (layer "F.Cu")
    (at 63.475 43.7)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 1.225 -2.13 180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 97 "Net-(J15-Pin_2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:CP-2350" locked (layer "F.Cu")
    (at 116 22 180)
    (descr "Female <b>CONNECTOR</b><p>\n5 pins 90 deg. with shield, horizontal (DIN 41524)")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/switchcraft-inc/57PC5F/275385")
    (property "ki_description" "5-pin DIN connector (5-pin DIN-5 stereo)")
    (property "ki_keywords" "circular DIN connector stereo audio")
    (fp_text reference "J1" (at -12 -11.6 180) (layer "F.SilkS"))
    (fp_text value "MIDI_OUT" (at -5.6 4.8) (layer "F.Fab"))
    (fp_text user "5" (at -7.9 -13.5) (layer "F.SilkS"))
    (fp_text user "4" (at 7.3 -13.5) (layer "F.SilkS"))
    (fp_text user "1" (at 8.4 -6.8) (layer "F.SilkS"))
    (fp_text user "3" (at -9.3 -6.9) (layer "F.SilkS"))
    (fp_text user "2" (at 0.5 -5.9) (layer "F.SilkS"))
    (pad "1" thru_hole roundrect locked (at 7.5 -10 180) (size 2.5 2.5) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 90 "unconnected-(J1-Pad1)") (pintype "passive+no_connect") (solder_mask_margin 0.0508) (thermal_bridge_angle 45))
    (pad "2" thru_hole roundrect locked (at 0 -10 270) (size 2.5 2.5) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "GND") (pintype "passive") (solder_mask_margin 0.0508) (thermal_bridge_angle 45))
    (pad "3" thru_hole roundrect locked (at -7.5 -10 180) (size 2.5 2.5) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 91 "unconnected-(J1-Pad3)") (pintype "passive+no_connect") (solder_mask_margin 0.0508) (thermal_bridge_angle 45))
    (pad "4" thru_hole roundrect locked (at 5 -12.5 180) (size 2.5 2.5) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 98 "Net-(J15-Pin_6)") (pintype "passive") (solder_mask_margin 0.0508) (thermal_bridge_angle 45))
    (pad "5" thru_hole roundrect locked (at -5 -12.5 180) (size 2.5 2.5) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 99 "Net-(J15-Pin_4)") (pintype "passive") (solder_mask_margin 0.0508) (thermal_bridge_angle 45))
    (pad "PE" thru_hole roundrect locked (at -2.5 0 180) (size 1.8 2) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.5) (chamfer bottom_right)
      (solder_mask_margin 0.0508))
    (pad "PE1" thru_hole rect locked (at -5 0 180) (size 1.8 2) (drill 1.3208) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.0508))
    (pad "PE2" thru_hole rect locked (at 5 0 180) (size 1.8 2) (drill 1.3208) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.0508))
    (pad "PE@" thru_hole roundrect locked (at 2.5 0 180) (size 1.8 2) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.5) (chamfer bottom_left)
      (solder_mask_margin 0.0508))
  )
  (footprint "Pedalboard Library:LED_D5.0mm-NeoPixel" locked (layer "F.Cu")
    (at 90.6 48)
    (descr "LED, diameter 5.0mm, 4 pins, WP154A4,https://www.adafruit.com/product/1938")
    (tags "LED diameter 5.0mm neopixel adafruit")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/sparkfun-electronics/COM-12999/5673800")
    (property "ki_description" "RGB LED with integrated controller, 5mm/8mm LED package")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr through_hole)
    (fp_text reference "D2" (at 1.905 -3.96) (layer "F.SilkS"))
    (fp_text value "NEOPIX" (at 1.905 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.905 -3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D2-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm_CircularMountingHoles" locked (layer "F.Cu")
    (at 60.25 31.5)
    (descr "Alps rotary encoder, EC12E... with switch, vertical shaft, mounting holes with circular drills, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC11/EC11E15204A3.html")
    (tags "rotary encoder")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/482016514001/10056402")
    (property "ki_description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch")
    (property "ki_keywords" "rotary switch encoder switch push button")
    (attr through_hole)
    (fp_text reference "SW7" (at 2.8 -4.3) (layer "F.SilkS"))
    (fp_text value "VOL Rotary" (at 7.5 10.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.1 6.3) (layer "F.Fab"))
    (pad "A" thru_hole rect locked (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 84 "/MIDI/ROT_VOL_A") (pinfunction "A") (pintype "passive"))
    (pad "B" thru_hole circle locked (at 0 5) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 85 "/MIDI/ROT_VOL_B") (pinfunction "B") (pintype "passive"))
    (pad "C" thru_hole circle locked (at 0 2.5) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive"))
    (pad "MP" thru_hole circle locked (at 7.5 -3.1) (size 3.2 3.2) (drill 2.6) (layers "*.Cu" "*.Mask"))
    (pad "MP" thru_hole circle locked (at 7.5 8.1) (size 3.2 3.2) (drill 2.6) (layers "*.Cu" "*.Mask"))
    (pad "S1" thru_hole circle locked (at 14.5 5) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 86 "/MIDI/SW_VOL") (pinfunction "S1") (pintype "passive"))
    (pad "S2" thru_hole circle locked (at 14.5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "S2") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/EC11E-05SW.STEP"
      (offset (xyz 7.4 -2.3 -12))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (at 68.75 43.675)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 1.49 -1.975) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (at 164.57 83.3)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C8" (at -2.2976 -0.088) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm" (layer "F.Cu")
    (at 144.1 60.932323 -90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/cornell-dubilier-illinois-capacitor/227AVG050MGBJ/5411698")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C14" (at 6.867677 -5.4 -180) (layer "F.SilkS"))
    (fp_text value "220uF" (at 2.5 6.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 119 "/Power Supply/vin") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 115 "/Power Supply/power_input_gnd") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" placed (layer "F.Cu")
    (at 78.28 68.98 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/koa-speer-electronics-inc/CF1-4C221J/13537314")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 10.18 -1.92) (layer "F.SilkS"))
    (fp_text value "220" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 94 "Net-(L1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D11-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 167.9 63.45)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0.1 -3.15) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm" (layer "F.Cu")
    (at 135.6 63.4 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/cornell-dubilier-illinois-capacitor/227AVG050MGBJ/5411698")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C15" (at 8 -3.9) (layer "F.SilkS"))
    (fp_text value "220uF" (at 2.5 6.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "+5VD") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:LED_D5.0mm-NeoPixel" locked (layer "F.Cu")
    (at 65.6 48)
    (descr "LED, diameter 5.0mm, 4 pins, WP154A4,https://www.adafruit.com/product/1938")
    (tags "LED diameter 5.0mm neopixel adafruit")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/sparkfun-electronics/COM-12999/5673800")
    (property "ki_description" "RGB LED with integrated controller, 5mm/8mm LED package")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr through_hole)
    (fp_text reference "D1" (at -2.1 -1.8736) (layer "F.SilkS"))
    (fp_text value "NEOPIX" (at 1.905 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.905 -3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 103 "Net-(D1-DIN)") (pinfunction "DIN") (pintype "input"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" locked (layer "F.Cu")
    (at 91.25 52.4)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 1.25 2.1) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.5 -0.05) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 42 121.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Sheetfile" "pedalboard-hw.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H9" (at 0 -3.35) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Pedalboard Library:Jack_6.35mm_Horizontal" locked (layer "F.Cu")
    (at 175.6 74.78)
    (descr "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins, https://www.neutrik.com/en/product/nmj6hcd2")
    (tags "neutrik jack m")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/schurter-inc/4833-2320/2644235")
    (property "ki_description" "M Series, 6.35mm (1/4in) stereo jack, switched, with chrome ferrule and straight PCB pins")
    (property "ki_keywords" "audio jack receptacle stereo headphones connector neutrik")
    (attr through_hole)
    (fp_text reference "J9" (at -5.5 -0.48) (layer "F.SilkS"))
    (fp_text value "Audio IN Right" (at 6.35 19) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 8.115) (layer "F.Fab"))
    (pad "R" thru_hole circle locked (at 6.35 0) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 104 "/Audio/in_R-") (pintype "passive"))
    (pad "RN" thru_hole circle locked (at 6.35 16.23) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 105 "/Audio/GND_in_R") (pintype "passive"))
    (pad "S" thru_hole circle locked (at 12.7 0) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 105 "/Audio/GND_in_R") (pintype "passive"))
    (pad "SN" thru_hole circle locked (at 12.7 16.23) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 66 "unconnected-(J9-PadSN)") (pintype "passive+no_connect"))
    (pad "T" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 106 "/Audio/in_R+") (pintype "passive"))
    (pad "TN" thru_hole circle locked (at 0 16.23) (size 3 3) (drill 1.4) (layers "*.Cu" "*.Mask")
      (net 105 "/Audio/GND_in_R") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/3-D NMJ6HCD2.stp"
      (offset (xyz 16.5 -8 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth-430476085716" locked (layer "F.Cu")
    (at 23.75 64.5)
    (descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430466043726/5209037")
    (property "ki_description" "Omron B3FS 6x6mm single pole normally-open tactile switch")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW1" (at 6.35 -4.66) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 78 "/MIDI/SW_D") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole oval locked (at 12.5 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 78 "/MIDI/SW_D") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.5 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/430476085716_Download_STP_430476085716_rev1.stp"
      (offset (xyz 6 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (at 129.65 43.47)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C12" (at 1.25 -2.05) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 122 "/MIDI/VBUS_FILTERED") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" placed (layer "F.Cu")
    (at 47.695 63.05)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/koa-speer-electronics-inc/CF1-4C330J/13537493")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 0.305 -1.55) (layer "F.SilkS"))
    (fp_text value "33" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 95 "Net-(L3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm" (layer "F.Cu")
    (at 160.532323 37.5)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/cornell-dubilier-illinois-capacitor/227AVG050MGBJ/5411698")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C13" (at -2.632323 -4.7) (layer "F.SilkS"))
    (fp_text value "220uF" (at 2.5 6.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 113 "/Power Supply/fused") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 115 "/Power Supply/power_input_gnd") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:LED_D5.0mm-NeoPixel" (layer "F.Cu")
    (at 164.1 79)
    (descr "LED, diameter 5.0mm, 4 pins, WP154A4,https://www.adafruit.com/product/1938")
    (tags "LED diameter 5.0mm neopixel adafruit")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/sparkfun-electronics/COM-12999/5673800")
    (property "ki_description" "RGB LED with integrated controller, 5mm/8mm LED package")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr through_hole)
    (fp_text reference "D5" (at 1.905 -3.96) (layer "F.SilkS"))
    (fp_text value "NEOPIX" (at 1.905 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.905 -3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D4-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D5-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" placed (layer "F.Cu")
    (at 81.19 69.34)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/koa-speer-electronics-inc/CF1-4C100J/13537327")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 12.51 0.16) (layer "F.SilkS"))
    (fp_text value "10" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 96 "Net-(L4-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "/MIDI/EXT_MIDI_TX") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:LED_D5.0mm-NeoPixel" locked (layer "F.Cu")
    (at 42.1 106)
    (descr "LED, diameter 5.0mm, 4 pins, WP154A4,https://www.adafruit.com/product/1938")
    (tags "LED diameter 5.0mm neopixel adafruit")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/sparkfun-electronics/COM-12999/5673800")
    (property "ki_description" "RGB LED with integrated controller, 5mm/8mm LED package")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr through_hole)
    (fp_text reference "D10" (at 6.3632 2.5088) (layer "F.SilkS"))
    (fp_text value "NEOPIX" (at 1.905 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.905 -3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D10-DIN)") (pinfunction "DIN") (pintype "input"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D10-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2" (layer "F.Cu")
    (at 76.6 55.27 -90)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=6.6*2.7mm^2, Vishay, IM-2, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 10.16mm  length 6.6mm diameter 2.7mm Vishay IM-2")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/fair-rite-products-corp/2743005111/8599429")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L1" (at 0.13 -2.2 -180) (layer "F.SilkS"))
    (fp_text value "103_100MHz" (at 5.08 2.47 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 100 "Net-(J15-Pin_3)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 94 "Net-(L1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D7.5mm_W4.4mm_P5.00mm" (layer "F.Cu")
    (at 146.5 55.7 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*4.4mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 4.4mm Capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/kemet/C330C102JHR5TA/1465599")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C18" (at 5.4 3.1 180) (layer "F.SilkS"))
    (fp_text value "1nF" (at 2.5 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 119 "/Power Supply/vin") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 43 "+5VD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W4.4mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" placed (layer "F.Cu")
    (at 73.7 65.775 90)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/onsemi/1N4148/458603")
    (property "ki_description" "100V 0.15A standard switching diode, DO-35")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D11" (at 8.975 -0.3 180) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 3.81 2.12 90) (layer "F.Fab"))
    (fp_text user "K" (at 1.125 -0.59 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D11-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D11-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" locked (layer "F.Cu")
    (at 116.15 52.3)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 1.245 2.115) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-201AD_P15.24mm_Horizontal" (layer "F.Cu")
    (at 154.7 45.9 90)
    (descr "Diode, DO-201AD series, Axial, Horizontal, pin pitch=15.24mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
    (tags "Diode DO-201AD series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 5.2mm")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/onsemi/1N5401G/1485525")
    (property "ki_description" "100V 3A General Purpose Rectifier Diode, DO-201AD")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D12" (at 7.62 -3.72 90) (layer "F.SilkS"))
    (fp_text value "1N5401" (at 7.62 3.72 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.6 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 8.3325 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.6 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 3.2 3.2) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 113 "/Power Supply/fused") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 15.24 0 90) (size 3.2 3.2) (drill 1.6) (layers "*.Cu" "*.Mask")
      (net 115 "/Power Supply/power_input_gnd") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-201AD_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2" (layer "F.Cu")
    (at 91.28 62.575 180)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=6.6*2.7mm^2, Vishay, IM-2, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 10.16mm  length 6.6mm diameter 2.7mm Vishay IM-2")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/fair-rite-products-corp/2743005111/8599429")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L2" (at -2.22 -0.025) (layer "F.SilkS"))
    (fp_text value "103_100MHz" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 101 "Net-(J15-Pin_1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D11-A)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (at 171.9 29.8 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/bel-fuse-inc/0ZRP0090FF1E/9468255")
    (property "ki_description" "Resettable fuse, polymeric positive temperature coefficient")
    (property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch")
    (attr through_hole)
    (fp_text reference "F1" (at -0.2 2.7) (layer "F.SilkS"))
    (fp_text value "Polyfuse 1.8A" (at 2.5 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 121 "/Power Supply/unfused") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 113 "/Power Supply/fused") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 118.9 63.5656)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.35) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Capacitor_THT:C_Disc_D5.1mm_W3.2mm_P5.00mm" (layer "F.Cu")
    (at 151.7 57.2 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5.1*3.2mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5.1mm width 3.2mm Capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/kemet/C322C475K5R5TA/3726055")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C17" (at -1.1676 0.7224 -180) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 2.5 2.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 119 "/Power Supply/vin") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 115 "/Power Supply/power_input_gnd") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.1mm_W3.2mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:LED_D5.0mm-NeoPixel" locked (layer "F.Cu")
    (at 164.1 106)
    (descr "LED, diameter 5.0mm, 4 pins, WP154A4,https://www.adafruit.com/product/1938")
    (tags "LED diameter 5.0mm neopixel adafruit")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/sparkfun-electronics/COM-12999/5673800")
    (property "ki_description" "RGB LED with integrated controller, 5mm/8mm LED package")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr through_hole)
    (fp_text reference "D6" (at 1.905 -3.96) (layer "F.SilkS"))
    (fp_text value "NEOPIX" (at 1.905 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.905 -3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D5-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D6-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth-430476085716" locked (layer "F.Cu")
    (at 173.75 116.5)
    (descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430466043726/5209037")
    (property "ki_description" "Omron B3FS 6x6mm single pole normally-open tactile switch")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW6" (at -2.45 -2.3) (layer "F.SilkS"))
    (fp_text value "C" (at 6.35 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 83 "/MIDI/SW_C") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole oval locked (at 12.5 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 83 "/MIDI/SW_C") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.5 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/430476085716_Download_STP_430476085716_rev1.stp"
      (offset (xyz 6 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth-430476085716" locked (layer "F.Cu")
    (at 173.75 64.5)
    (descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430466043726/5209037")
    (property "ki_description" "Omron B3FS 6x6mm single pole normally-open tactile switch")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW3" (at 6.35 -4.66) (layer "F.SilkS"))
    (fp_text value "F" (at 6.35 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 80 "/MIDI/SW_F") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole oval locked (at 12.5 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 80 "/MIDI/SW_F") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.5 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/430476085716_Download_STP_430476085716_rev1.stp"
      (offset (xyz 6 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (at 100.67 79.05 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at -2.55 0.35) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth-430476085716" locked (layer "F.Cu")
    (at 23.75 116.5)
    (descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430466043726/5209037")
    (property "ki_description" "Omron B3FS 6x6mm single pole normally-open tactile switch")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW4" (at 6.35 -4.66) (layer "F.SilkS"))
    (fp_text value "A" (at 6.35 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 81 "/MIDI/SW_A") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole oval locked (at 12.5 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 81 "/MIDI/SW_A") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.5 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/430476085716_Download_STP_430476085716_rev1.stp"
      (offset (xyz 6 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965" (layer "F.Cu")
    (at 168 23)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, DIN965")
    (tags "mounting hole 2.7mm no annular m2.5 din965")
    (property "Sheetfile" "pedalboard-hw.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H8" (at -3 0.1) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Inductor_THT:L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2" (layer "F.Cu")
    (at 91.35 65.98 180)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=6.6*2.7mm^2, Vishay, IM-2, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 10.16mm  length 6.6mm diameter 2.7mm Vishay IM-2")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/fair-rite-products-corp/2743005111/8599429")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L4" (at -2.25 -0.12) (layer "F.SilkS"))
    (fp_text value "103_100MHz" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 99 "Net-(J15-Pin_4)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 96 "Net-(L4-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm_CircularMountingHoles" locked (layer "F.Cu")
    (at 135.25 31.5)
    (descr "Alps rotary encoder, EC12E... with switch, vertical shaft, mounting holes with circular drills, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC11/EC11E15204A3.html")
    (tags "rotary encoder")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/482016514001/10056402")
    (property "ki_description" "Rotary encoder, dual channel, incremental quadrate outputs, with switch")
    (property "ki_keywords" "rotary switch encoder switch push button")
    (attr through_hole)
    (fp_text reference "SW8" (at 2.8 -4.7) (layer "F.SilkS"))
    (fp_text value "GAIN Rotary" (at 7.5 10.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.1 6.3) (layer "F.Fab"))
    (pad "A" thru_hole rect locked (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 87 "/MIDI/ROT_GAIN_A") (pinfunction "A") (pintype "passive"))
    (pad "B" thru_hole circle locked (at 0 5) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 88 "/MIDI/ROT_GAIN_B") (pinfunction "B") (pintype "passive"))
    (pad "C" thru_hole circle locked (at 0 2.5) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "C") (pintype "passive"))
    (pad "MP" thru_hole circle locked (at 7.5 -3.1) (size 3.2 3.2) (drill 2.6) (layers "*.Cu" "*.Mask"))
    (pad "MP" thru_hole circle locked (at 7.5 8.1) (size 3.2 3.2) (drill 2.6) (layers "*.Cu" "*.Mask"))
    (pad "S1" thru_hole circle locked (at 14.5 5) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 89 "/MIDI/SW_GAIN") (pinfunction "S1") (pintype "passive"))
    (pad "S2" thru_hole circle locked (at 14.5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "S2") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/EC11E-05SW.STEP"
      (offset (xyz 7.4 -2.3 -12))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" placed (layer "F.Cu")
    (at 47.695 66.05)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/koa-speer-electronics-inc/CF1-4C471J/13537235")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 0.305 2.45) (layer "F.SilkS"))
    (fp_text value "470" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "/MIDI/EXT_MIDI_RX") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:SW_PUSH-12mm_Wuerth-430476085716" locked (layer "F.Cu")
    (at 98.75 116.5)
    (descr "SW PUSH 12mm http://katalog.we-online.de/em/datasheet/430476085716.pdf")
    (tags "tact sw push 12mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/430466043726/5209037")
    (property "ki_description" "Omron B3FS 6x6mm single pole normally-open tactile switch")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW5" (at 6.35 -4.66) (layer "F.SilkS"))
    (fp_text value "B" (at 6.35 9.93) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval locked (at 0 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 82 "/MIDI/SW_B") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole oval locked (at 12.5 0) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 82 "/MIDI/SW_B") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.5 5) (size 3 2.5) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/430476085716_Download_STP_430476085716_rev1.stp"
      (offset (xyz 6 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D7.5mm_W4.4mm_P5.00mm" (layer "F.Cu")
    (at 156.2 64.7 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7.5*4.4mm^2, Capacitor")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7.5mm width 4.4mm Capacitor")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/kemet/C330C102JHR5TA/1465599")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C19" (at 7.3468 -1.0568 180) (layer "F.SilkS"))
    (fp_text value "1nF" (at 2.5 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 115 "/Power Supply/power_input_gnd") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.5mm_W4.4mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:CP-2350" locked (layer "F.Cu")
    (at 94.0055 22 180)
    (descr "Female <b>CONNECTOR</b><p>\n5 pins 90 deg. with shield, horizontal (DIN 41524)")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/switchcraft-inc/57PC5F/275385")
    (property "ki_description" "5-pin DIN connector (5-pin DIN-5 stereo)")
    (property "ki_keywords" "circular DIN connector stereo audio")
    (fp_text reference "J2" (at -11.6945 -12 180) (layer "F.SilkS"))
    (fp_text value "MIDI_IN" (at -5.6 4.8) (layer "F.Fab"))
    (fp_text user "4" (at 7.1055 -13.6) (layer "F.SilkS"))
    (fp_text user "3" (at -9.3945 -6.9) (layer "F.SilkS"))
    (fp_text user "2" (at 0.5 -5.9) (layer "F.SilkS"))
    (fp_text user "5" (at -8.2945 -13.6) (layer "F.SilkS"))
    (fp_text user "1" (at 8.4055 -6.8) (layer "F.SilkS"))
    (pad "1" thru_hole roundrect locked (at 7.5 -10 180) (size 2.5 2.5) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 92 "unconnected-(J2-Pad1)") (pintype "passive+no_connect") (solder_mask_margin 0.0508) (thermal_bridge_angle 45))
    (pad "2" thru_hole roundrect locked (at 0 -10 270) (size 2.5 2.5) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 97 "Net-(J15-Pin_2)") (pintype "passive") (solder_mask_margin 0.0508) (thermal_bridge_angle 45))
    (pad "3" thru_hole roundrect locked (at -7.5 -10 180) (size 2.5 2.5) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 93 "unconnected-(J2-Pad3)") (pintype "passive+no_connect") (solder_mask_margin 0.0508) (thermal_bridge_angle 45))
    (pad "4" thru_hole roundrect locked (at 5 -12.5 180) (size 2.5 2.5) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 100 "Net-(J15-Pin_3)") (pintype "passive") (solder_mask_margin 0.0508) (thermal_bridge_angle 45))
    (pad "5" thru_hole roundrect locked (at -5 -12.5 180) (size 2.5 2.5) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (chamfer_ratio 0.2928932188) (chamfer top_left top_right bottom_left bottom_right)
      (net 101 "Net-(J15-Pin_1)") (pintype "passive") (solder_mask_margin 0.0508) (thermal_bridge_angle 45))
    (pad "PE" thru_hole roundrect locked (at -2.5 0 180) (size 1.8 2) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.5) (chamfer bottom_right)
      (solder_mask_margin 0.0508))
    (pad "PE1" thru_hole rect locked (at -5 0 180) (size 1.8 2) (drill 1.3208) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.0508))
    (pad "PE2" thru_hole rect locked (at 5 0 180) (size 1.8 2) (drill 1.3208) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.0508))
    (pad "PE@" thru_hole roundrect locked (at 2.5 0 180) (size 1.8 2) (drill 1.3208) (layers "*.Cu" "*.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.5) (chamfer bottom_left)
      (solder_mask_margin 0.0508))
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (at 44.355 72.2 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/vishay-beyschlag-draloric-bc-components/K104K20X7RH5TL2/286568")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 1.46 -2.645 -180) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.25 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:Trace_Fuse" (layer "F.Cu")
    (at 188.93 119.106 -90)
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "ki_description" "Fuse, small symbol")
    (property "ki_keywords" "fuse")
    (attr smd)
    (fp_text reference "F5" (at 0 -2.9 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "~" (at 0.1 3.6 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1 5.1 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.3 0 270) (size 2.286 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(F5-Pad1)") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 1.3 0 270) (size 2.286 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/Audio/audio_in_stereo") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 149.606 43.0784 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/onsemi/1N5817RLG/807254")
    (property "ki_description" "20V 1A Schottky Barrier Rectifier Diode, DO-41")
    (property "ki_keywords" "diode Schottky")
    (attr through_hole)
    (fp_text reference "D13" (at 5.08 -2.47 90) (layer "F.SilkS"))
    (fp_text value "1N5817" (at 5.08 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 120 "/MIDI/VSYS") (pinfunction "K") (pintype "power_out"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 43 "+5VD") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:LED_D5.0mm-NeoPixel" locked (layer "F.Cu")
    (at 103.1 79)
    (descr "LED, diameter 5.0mm, 4 pins, WP154A4,https://www.adafruit.com/product/1938")
    (tags "LED diameter 5.0mm neopixel adafruit")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/sparkfun-electronics/COM-12999/5673800")
    (property "ki_description" "RGB LED with integrated controller, 5mm/8mm LED package")
    (property "ki_keywords" "RGB LED NeoPixel addressable")
    (attr through_hole)
    (fp_text reference "D8" (at 1.905 -3.96) (layer "F.SilkS"))
    (fp_text value "NEOPIX" (at 1.905 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.905 -3.96) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D7-DOUT)") (pinfunction "DIN") (pintype "input"))
    (pad "2" thru_hole oval locked (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D8-DOUT)") (pinfunction "DOUT") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2" (layer "F.Cu")
    (at 59.5 40.445 -90)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=6.6*2.7mm^2, Vishay, IM-2, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 10.16mm  length 6.6mm diameter 2.7mm Vishay IM-2")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/en/products/detail/fair-rite-products-corp/2743005111/8599429")
    (property "ki_description" "Inductor with ferrite core")
    (property "ki_keywords" "inductor choke coil reactor magnetic")
    (attr through_hole)
    (fp_text reference "L3" (at 9.755 -2.1 -90) (layer "F.SilkS"))
    (fp_text value "103_100MHz" (at 5.08 2.47 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 98 "Net-(J15-Pin_6)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 95 "Net-(L3-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:Jack_3.5mm_CUI_SJ1-3525N_Horizontal" locked (layer "F.Cu")
    (at 94 24.5 180)
    (descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
    (tags "TRS audio jack stereo horizontal")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/cui-devices/SJ1-3525NG/738690")
    (property "ki_description" "Audio Jack, 3 Poles (Stereo / TRS), Switched TR Poles (Normalling)")
    (property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "J17" (at -7 -1.7 270) (layer "F.SilkS"))
    (fp_text value "MIDI IN J" (at 0 -10 180) (layer "F.Fab"))
    (fp_text user "PCB edge" (at 0 3.65 180 unlocked) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 180) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5 0 180) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "" np_thru_hole circle locked (at 0 -5 180) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "" np_thru_hole circle locked (at 5 0 180) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "R" thru_hole oval locked (at -5 -5 180) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask")
      (net 100 "Net-(J15-Pin_3)") (pintype "passive"))
    (pad "RN" thru_hole oval locked (at -2.5 -5 180) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask")
      (net 100 "Net-(J15-Pin_3)") (pintype "passive"))
    (pad "S" thru_hole oval locked (at 0 0 180) (size 2.2 1.2) (drill oval 1.4 0.4) (layers "*.Cu" "*.Mask")
      (net 97 "Net-(J15-Pin_2)") (pintype "passive"))
    (pad "T" thru_hole oval locked (at 5 -5) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask")
      (net 101 "Net-(J15-Pin_1)") (pintype "passive"))
    (pad "TN" thru_hole oval locked (at 2.5 -5) (size 1.2 2.2) (drill oval 0.4 1.4) (layers "*.Cu" "*.Mask")
      (net 101 "Net-(J15-Pin_1)") (pintype "passive"))
    (model "${KIPRJMOD}/3d-models/jack3.5mm.x3d"
      (offset (xyz 0 1.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Pedalboard Library:USB A BCB Male Plug" (layer "B.Cu")
    (at 113.625 97.78)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/gct/USB1061-GF-L-A/10649776")
    (property "ki_description" "USB Type A connector")
    (property "ki_keywords" "connector USB")
    (attr through_hole)
    (fp_text reference "J6" (at 0 2.33) (layer "B.SilkS"))
    (fp_text value "USB_A" (at 0 -9.95) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 117 "/VBUS") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 44 "/Audio/USB_DN") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 102 "/Audio/USB_DP") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (model "${KIPRJMOD}/3d-models/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3d-models/USB1061-GF-L-A.stp"
      (offset (xyz -21.6 -3.9 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 -90))
    )
  )
  (footprint "Pedalboard Library:Trace_Fuse" (layer "B.Cu")
    (at 94.31 74.7 90)
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "ki_description" "Fuse, small symbol")
    (property "ki_keywords" "fuse")
    (attr smd)
    (fp_text reference "F3" (at 0.06 -2.06 270 unlocked) (layer "B.SilkS"))
    (fp_text value "~" (at 0.1 -3.6 270 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1 -5.1 270 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.3 0 90) (size 2.286 1.524) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/Audio/INT_MIDI_TX") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 1.3 0 90) (size 2.286 1.524) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(U1-GPIO9)") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal" (layer "B.Cu")
    (at 138 57.175 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "psu.kicad_sch")
    (property "Sheetname" "Power Supply")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/amphenol-cs-fci/68016-202HLF/4273561")
    (property "ki_description" "Generic connector, double row, 02x01, this symbol is compatible with counter-clockwise, top-bottom and odd-even numbering schemes., script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J14" (at -1.615 2.76 180) (layer "B.SilkS"))
    (fp_text value "Conn_02x01" (at 4.385 -4.81 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 -1.27 -360) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "+5VD") (pinfunction "Pin_1") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 114 "+5VP") (pinfunction "Pin_2") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:Spring_Loaded_Pins_2mm" locked (layer "B.Cu")
    (at 127 48 180)
    (descr "1x02, 2.00mm pitch, single row")
    (tags "Spring Loaded Pin Pogo")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/mill-max-manufacturing-corp/0906-0-15-20-76-14-11-0/1147048")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 2.06) (layer "B.SilkS"))
    (fp_text value "Pico USB TP" (at 0.0508 -8.2296) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1 90) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.35 1.35) (drill 0.508) (layers "*.Cu" "*.Mask")
      (net 44 "/Audio/USB_DN") (pinfunction "Pin_1") (pintype "passive") (clearance 0.635))
    (pad "2" thru_hole oval locked (at 0 -2 180) (size 1.35 1.35) (drill 0.508) (layers "*.Cu" "*.Mask")
      (net 102 "/Audio/USB_DP") (pinfunction "Pin_2") (pintype "passive") (clearance 0.635))
    (model "${KIPRJMOD}/3d-models/mill-max-0906-2-15-20-75-14-11-0.step"
      (offset (xyz 0 0 -1.905))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
    (model "${KIPRJMOD}/3d-models/mill-max-0906-2-15-20-75-14-11-0.step"
      (offset (xyz 0 -1.999996 -1.905))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 90 0))
    )
  )
  (footprint "Pedalboard Library:RPi_Pico_SMD_TH" locked (layer "B.Cu")
    (at 103 49 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/61302011121/4846860")
    (attr through_hole)
    (fp_text reference "U1" (at 8.6648 -27.5112) (layer "B.SilkS"))
    (fp_text value "Pico" (at 0 -2.159 270) (layer "B.Fab"))
    (fp_text user "GP16" (at 12.454 -23.274 45) (layer "Cmts.User"))
    (fp_text user "GND" (at -12.346 18.75 45) (layer "Cmts.User"))
    (fp_text user "GND" (at -12.346 -19.35 45) (layer "Cmts.User"))
    (fp_text user "3V3_EN" (at 13.1 18.056 45) (layer "Cmts.User"))
    (fp_text user "GP21" (at 12.454 -8.044 45) (layer "Cmts.User"))
    (fp_text user "GND" (at 12.2 19.906 45) (layer "Cmts.User"))
    (fp_text user "GND" (at 12.2 -5.494 45) (layer "Cmts.User"))
    (fp_text user "GP11" (at -12.746 -11.73 45) (layer "Cmts.User"))
    (fp_text user "GP20" (at 12.454 -10.574 45) (layer "Cmts.User"))
    (fp_text user "GP9" (at -12.346 -4.11 45) (layer "Cmts.User"))
    (fp_text user "GP10" (at -12.6 -9.19 45) (layer "Cmts.User"))
    (fp_text user "GP27" (at 12.454 4.656 45) (layer "Cmts.User"))
    (fp_text user "GP8" (at -12.346 -1.57 45) (layer "Cmts.User"))
    (fp_text user "GP5" (at -12.346 8.59 45) (layer "Cmts.User"))
    (fp_text user "ADC_VREF" (at 13.4 13.356 45) (layer "Cmts.User"))
    (fp_text user "GP15" (at -12.6 -24.43 45) (layer "Cmts.User"))
    (fp_text user "VSYS" (at 12.6 22.446 45) (layer "Cmts.User"))
    (fp_text user "SWDIO" (at 5.6 -26.2 270) (layer "Cmts.User"))
    (fp_text user "GP26" (at 12.454 2.126 45) (layer "Cmts.User"))
    (fp_text user "GND" (at -12.346 6.05 45) (layer "Cmts.User"))
    (fp_text user "VBUS" (at 12.7 25.056 45) (layer "Cmts.User"))
    (fp_text user "GP13" (at -12.6 -16.81 45) (layer "Cmts.User"))
    (fp_text user "GP19" (at 12.454 -13.114 45) (layer "Cmts.User"))
    (fp_text user "GP12" (at -12.746 -14.27 45) (layer "Cmts.User"))
    (fp_text user "GP6" (at -12.346 3.51 45) (layer "Cmts.User"))
    (fp_text user "GP1" (at -12.446 21.3 45) (layer "Cmts.User"))
    (fp_text user "RUN" (at 12.4 -0.414 45) (layer "Cmts.User"))
    (fp_text user "GP18" (at 12.454 -15.654 45) (layer "Cmts.User"))
    (fp_text user "GP3" (at -12.346 13.67 45) (layer "Cmts.User"))
    (fp_text user "GP17" (at 12.454 -20.734 45) (layer "Cmts.User"))
    (fp_text user "GP2" (at -12.446 16.21 45) (layer "Cmts.User"))
    (fp_text user "GND" (at -12.283 -6.078 45) (layer "Cmts.User"))
    (fp_text user "GP22" (at 12.454 -2.954 45) (layer "Cmts.User"))
    (fp_text user "GP0" (at -12.346 23.83 45) (layer "Cmts.User"))
    (fp_text user "3V3" (at 12.3 14.756 45) (layer "Cmts.User"))
    (fp_text user "GP7" (at -12.246 1 45) (layer "Cmts.User"))
    (fp_text user "GP4" (at -12.346 11.13 45) (layer "Cmts.User"))
    (fp_text user "AGND" (at 12.454 7.206 45) (layer "Cmts.User"))
    (fp_text user "GND" (at 12.2 -18.194 45) (layer "Cmts.User"))
    (fp_text user "GP28" (at 12.454 10 45) (layer "Cmts.User"))
    (fp_text user "GP14" (at -12.646 -21.89 45) (layer "Cmts.User"))
    (fp_text user "SWCLK" (at -5.7 -26.2 270) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" thru_hole oval locked (at -8.89 24.13 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 28 "/MIDI/EXT_MIDI_TX") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "2" thru_hole oval locked (at -8.89 21.59 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 27 "/MIDI/EXT_MIDI_RX") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "3" thru_hole rect locked (at -8.89 19.05 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval locked (at -8.89 16.51 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 83 "/MIDI/SW_C") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" thru_hole oval locked (at -8.89 13.97 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 80 "/MIDI/SW_F") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" thru_hole oval locked (at -8.89 11.43 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 79 "/MIDI/SW_E") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" thru_hole oval locked (at -8.89 8.89 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 82 "/MIDI/SW_B") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" thru_hole rect locked (at -8.89 6.35 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval locked (at -8.89 3.81 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 81 "/MIDI/SW_A") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "10" thru_hole oval locked (at -8.89 1.27 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 78 "/MIDI/SW_D") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "11" thru_hole oval locked (at -8.89 -1.27 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 123 "Net-(U1-GPIO8)") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" thru_hole oval locked (at -8.89 -3.81 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 124 "Net-(U1-GPIO9)") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" thru_hole rect locked (at -8.89 -6.35 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" thru_hole oval locked (at -8.89 -8.89 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 33 "unconnected-(U1-GPIO10-Pad14)") (pinfunction "GPIO10") (pintype "bidirectional+no_connect"))
    (pad "15" thru_hole oval locked (at -8.89 -11.43 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 4 "/MIDI/RGB_DATA") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "16" thru_hole oval locked (at -8.89 -13.97 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 34 "unconnected-(U1-GPIO12-Pad16)") (pinfunction "GPIO12") (pintype "bidirectional+no_connect"))
    (pad "17" thru_hole oval locked (at -8.89 -16.51 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 35 "unconnected-(U1-GPIO13-Pad17)") (pinfunction "GPIO13") (pintype "bidirectional+no_connect"))
    (pad "18" thru_hole rect locked (at -8.89 -19.05 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "19" thru_hole oval locked (at -8.89 -21.59 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(U1-GPIO14-Pad19)") (pinfunction "GPIO14") (pintype "bidirectional+no_connect"))
    (pad "20" thru_hole oval locked (at -8.89 -24.13 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(U1-GPIO15-Pad20)") (pinfunction "GPIO15") (pintype "bidirectional+no_connect"))
    (pad "21" thru_hole oval locked (at 8.89 -24.13 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 84 "/MIDI/ROT_VOL_A") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "22" thru_hole oval locked (at 8.89 -21.59 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 85 "/MIDI/ROT_VOL_B") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "23" thru_hole rect locked (at 8.89 -19.05 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "24" thru_hole oval locked (at 8.89 -16.51 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 86 "/MIDI/SW_VOL") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "25" thru_hole oval locked (at 8.89 -13.97 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 87 "/MIDI/ROT_GAIN_A") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "26" thru_hole oval locked (at 8.89 -11.43 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 88 "/MIDI/ROT_GAIN_B") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "27" thru_hole oval locked (at 8.89 -8.89 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 89 "/MIDI/SW_GAIN") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "28" thru_hole rect locked (at 8.89 -6.35 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "29" thru_hole oval locked (at 8.89 -3.81 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(U1-GPIO22-Pad29)") (pinfunction "GPIO22") (pintype "bidirectional+no_connect"))
    (pad "30" thru_hole oval locked (at 8.89 -1.27 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 39 "unconnected-(U1-RUN-Pad30)") (pinfunction "RUN") (pintype "input+no_connect"))
    (pad "31" thru_hole oval locked (at 8.89 1.27 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 40 "unconnected-(U1-GPIO26_ADC0-Pad31)") (pinfunction "GPIO26_ADC0") (pintype "bidirectional+no_connect"))
    (pad "32" thru_hole oval locked (at 8.89 3.81 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(U1-GPIO27_ADC1-Pad32)") (pinfunction "GPIO27_ADC1") (pintype "bidirectional+no_connect"))
    (pad "33" thru_hole rect locked (at 8.89 6.35 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(U1-AGND)") (pinfunction "AGND") (pintype "power_out"))
    (pad "34" thru_hole oval locked (at 8.89 8.89 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(U1-GPIO28_ADC2)") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "35" thru_hole oval locked (at 8.89 11.43 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 19 "Net-(U1-ADC_VREF)") (pinfunction "ADC_VREF") (pintype "output"))
    (pad "36" thru_hole oval locked (at 8.89 13.97 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "3V3") (pintype "power_out"))
    (pad "37" thru_hole oval locked (at 8.89 16.51 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(U1-3V3_EN-Pad37)") (pinfunction "3V3_EN") (pintype "input+no_connect"))
    (pad "38" thru_hole rect locked (at 8.89 19.05 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "39" thru_hole oval locked (at 8.89 21.59 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 120 "/MIDI/VSYS") (pinfunction "VSYS") (pintype "power_in"))
    (pad "40" thru_hole oval locked (at 8.89 24.13 90) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 122 "/MIDI/VBUS_FILTERED") (pinfunction "VBUS") (pintype "power_in"))
    (model "${KIPRJMOD}/3d-models/Pico.wrl"
      (offset (xyz 0 0 2.54))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "B.Cu")
    (at 55.865 82.9626 90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/61300311021/4846824")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at -0.5018 2.7582 180) (layer "B.SilkS"))
    (fp_text value "RGB_LED_EXT" (at 11.465 -1.925) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.7 -2.58) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D10-DOUT)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "+3.3V") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Pedalboard Library:HiFi Berry DAC ADC+" (layer "B.Cu")
    (at 120.25 68.3756 180)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (property "Sheetfile" "audio.kicad_sch")
    (property "Sheetname" "Audio")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/61304021821/16608657")
    (property "ki_description" "expansion header for Raspberry Pi 2 & 3")
    (property "ki_keywords" "raspberrypi gpio")
    (attr through_hole)
    (fp_text reference "J8" (at -3.05 -0.1244) (layer "B.SilkS"))
    (fp_text value "HiFi Berry" (at -3.45 -25.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -24.13 90) (layer "F.Fab"))
    (dimension (type aligned) (layer "Dwgs.User")
      (pts (xy 167.98 63.5056) (xy 171.48 63.5056))
      (height -7)
      (gr_text "3.5 mm" (at 170.98 54.5056) (layer "Dwgs.User"))
      (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
      (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
    )
    (dimension (type aligned) (layer "Dwgs.User")
      (pts (xy 118.98 63.5056) (xy 167.98 63.5056))
      (height -7)
      (gr_text "49 mm" (at 143.48 55.3556) (layer "Dwgs.User"))
      (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
      (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
    )
    (dimension (type aligned) (layer "Dwgs.User")
      (pts (xy 118.98 63.5056) (xy 118.98 121.5056))
      (height 11.5)
      (gr_text "58 mm" (at 106.33 92.5056 90) (layer "Dwgs.User"))
      (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
      (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
    )
    (dimension (type aligned) (layer "Dwgs.User")
      (pts (xy 118.98 92.5056) (xy 118.98 63.5056))
      (height -7.5)
      (gr_text "29 mm" (at 110.33 78.0056 90) (layer "Dwgs.User"))
      (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
      (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
    )
    (dimension (type aligned) (layer "Dwgs.User")
      (pts (xy 118.98 125.0056) (xy 118.98 60.0056))
      (height -16)
      (gr_text "65 mm" (at 101.83 92.5056 90) (layer "Dwgs.User"))
      (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
      (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
    )
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(J7-3V3-Pad1)") (pinfunction "3V3") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 114 "+5VP") (pinfunction "5V") (pintype "power_in"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/Audio/conf_i2c_sda") (pinfunction "SDA/GPIO2") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 116 "Net-(J7-5V-Pad4)") (pinfunction "5V") (pintype "power_in"))
    (pad "5" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "/Audio/conf_i2c_scl") (pinfunction "SCL/GPIO3") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(J7-GCLK0{slash}GPIO4)") (pinfunction "GCLK0/GPIO4") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/Audio/INT_MIDI_TX") (pinfunction "GPIO14/TXD") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "10" thru_hole oval (at 2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/Audio/INT_MIDI_RX") (pinfunction "GPIO15/RXD") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(J7-GPIO17)") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "/Audio/audio_pcm_clk") (pinfunction "GPIO18/PWM0") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "/Audio/audio_in_stereo") (pinfunction "GPIO27") (pintype "bidirectional"))
    (pad "14" thru_hole oval (at 2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "15" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "Net-(J7-GPIO22)") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at 2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "Net-(J7-GPIO23)") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "17" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(J7-3V3-Pad17)") (pinfunction "3V3") (pintype "power_in"))
    (pad "18" thru_hole oval (at 2.54 -20.32 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "Net-(J7-GPIO24)") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "19" thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(J7-MOSI0{slash}GPIO10)") (pinfunction "MOSI0/GPIO10") (pintype "bidirectional"))
    (pad "20" thru_hole oval (at 2.54 -22.86 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "21" thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 50 "Net-(J7-MISO0{slash}GPIO9)") (pinfunction "MISO0/GPIO9") (pintype "bidirectional"))
    (pad "22" thru_hole oval (at 2.54 -25.4 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(J7-GPIO25)") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "23" thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "Net-(J7-SCLK0{slash}GPIO11)") (pinfunction "SCLK0/GPIO11") (pintype "bidirectional"))
    (pad "24" thru_hole oval (at 2.54 -27.94 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "Net-(J7-~{CE0}{slash}GPIO8)") (pinfunction "~{CE0}/GPIO8") (pintype "bidirectional"))
    (pad "25" thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "26" thru_hole oval (at 2.54 -30.48 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "Net-(J7-~{CE1}{slash}GPIO7)") (pinfunction "~{CE1}/GPIO7") (pintype "bidirectional"))
    (pad "27" thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "Net-(J7-ID_SD{slash}GPIO0)") (pinfunction "ID_SD/GPIO0") (pintype "bidirectional"))
    (pad "28" thru_hole oval (at 2.54 -33.02 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "Net-(J7-ID_SC{slash}GPIO1)") (pinfunction "ID_SC/GPIO1") (pintype "bidirectional"))
    (pad "29" thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "Net-(J7-GCLK1{slash}GPIO5)") (pinfunction "GCLK1/GPIO5") (pintype "bidirectional"))
    (pad "30" thru_hole oval (at 2.54 -35.56 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "31" thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "Net-(J7-GCLK2{slash}GPIO6)") (pinfunction "GCLK2/GPIO6") (pintype "bidirectional"))
    (pad "32" thru_hole oval (at 2.54 -38.1 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 59 "Net-(J7-PWM0{slash}GPIO12)") (pinfunction "PWM0/GPIO12") (pintype "bidirectional"))
    (pad "33" thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "Net-(J7-PWM1{slash}GPIO13)") (pinfunction "PWM1/GPIO13") (pintype "bidirectional"))
    (pad "34" thru_hole oval (at 2.54 -40.64 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "/Audio/audio_pcm_fs") (pinfunction "GPIO19/MISO1") (pintype "bidirectional"))
    (pad "36" thru_hole oval (at 2.54 -43.18 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "Net-(J7-GPIO16)") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "37" thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "/Audio/audio_out_stereo") (pinfunction "GPIO26") (pintype "bidirectional"))
    (pad "38" thru_hole oval (at 2.54 -45.72 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/Audio/audio_pcm_din") (pinfunction "GPIO20/MOSI1") (pintype "bidirectional"))
    (pad "39" thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "40" thru_hole oval (at 2.54 -48.26 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "/Audio/audio_pcm_dout") (pinfunction "GPIO21/SCLK1") (pintype "bidirectional"))
    (pad "41" thru_hole rect (at -36.305 -6.47 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 104 "/Audio/in_R-") (pinfunction "in_R-") (pintype "input"))
    (pad "42" thru_hole oval (at -33.765 -6.47 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 106 "/Audio/in_R+") (pinfunction "in_R+") (pintype "input"))
    (pad "43" thru_hole oval (at -36.305 -9.01 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 105 "/Audio/GND_in_R") (pinfunction "in_GND") (pintype "input"))
    (pad "44" thru_hole oval (at -33.765 -9.01 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 108 "/Audio/GND_in_L") (pinfunction "in_GND") (pintype "input"))
    (pad "45" thru_hole oval (at -36.305 -11.55 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 109 "/Audio/in_L+") (pinfunction "in_L+") (pintype "input"))
    (pad "46" thru_hole oval (at -33.765 -11.55 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 107 "/Audio/in_L-") (pinfunction "in_L-") (pintype "input"))
    (pad "47" thru_hole rect (at -32.13 -50.775 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 70 "unconnected-(J8-out_5V-Pad47)") (pinfunction "out_5V") (pintype "power_out+no_connect"))
    (pad "48" thru_hole oval (at -32.13 -53.315 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 74 "Net-(J8-out_R)") (pinfunction "out_R") (pintype "output"))
    (pad "49" thru_hole oval (at -34.67 -50.775 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 110 "/Audio/GND_out") (pinfunction "out_GND") (pintype "input"))
    (pad "50" thru_hole oval (at -34.67 -53.315 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 110 "/Audio/GND_out") (pinfunction "out_GND") (pintype "input"))
    (pad "51" thru_hole oval (at -37.21 -50.775 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 76 "unconnected-(J8-out_5V-Pad51)") (pinfunction "out_5V") (pintype "power_out+no_connect"))
    (pad "52" thru_hole oval (at -37.21 -53.315 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 77 "Net-(J8-out_L)") (pinfunction "out_L") (pintype "output"))
    (model "3d-models/hifiberry-dac-plus-adc-1.2.step"
      (offset (xyz 21.27 35.03 6.9))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Pedalboard Library:Trace_Fuse" (layer "B.Cu")
    (at 96.24 74.69 90)
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "ki_description" "Fuse, small symbol")
    (property "ki_keywords" "fuse")
    (attr smd)
    (fp_text reference "F2" (at 0.05 2.02 270 unlocked) (layer "B.SilkS"))
    (fp_text value "~" (at 0.1 -3.6 270 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1 -5.1 270 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.3 0 90) (size 2.286 1.524) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/Audio/INT_MIDI_RX") (pintype "passive") (thermal_bridge_angle 45))
    (pad "2" smd roundrect (at 1.3 0 90) (size 2.286 1.524) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 123 "Net-(U1-GPIO8)") (pintype "passive") (thermal_bridge_angle 45))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Horizontal" (layer "B.Cu")
    (at 71 52.85 180)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "pico.kicad_sch")
    (property "Sheetname" "MIDI")
    (property "Supplier" "https://www.digikey.ch/de/products/detail/w%C3%BCrth-elektronik/61300621021/4846834")
    (property "ki_description" "Generic connector, double row, 02x03, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J15" (at 5.1632 -7.4496) (layer "B.SilkS"))
    (fp_text value "MIDI IN/OUT" (at 13.93 -2.985 90) (layer "B.Fab"))
    (fp_text user locked "${REFERENCE}" (at 5.31 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 101 "Net-(J15-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 97 "Net-(J15-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 100 "Net-(J15-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 99 "Net-(J15-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 98 "Net-(J15-Pin_6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 118.2 20) (end 189 20)
    (layer "Edge.Cuts"))
  (gr_line (start 20 124) (end 20 61)
    (layer "Edge.Cuts"))
  (gr_line (start 21 125) (end 189 125)
    (layer "Edge.Cuts"))
  (gr_line (start 74 21) (end 74 25)
    (layer "Edge.Cuts"))
  (gr_arc (start 74 21) (mid 74.292893 20.292893) (end 75 20)
    (layer "Edge.Cuts"))
  (gr_arc (start 114.2 21.4) (mid 113.917157 21.282843) (end 113.8 21)
    (layer "Edge.Cuts"))
  (gr_arc (start 21 125) (mid 20.292893 124.707107) (end 20 124)
    (layer "Edge.Cuts"))
  (gr_arc (start 92.2 21.4) (mid 91.917157 21.282843) (end 91.8 21)
    (layer "Edge.Cuts"))
  (gr_line (start 114.2 21.4) (end 117.8 21.4)
    (layer "Edge.Cuts"))
  (gr_line (start 58 59) (end 58 27)
    (layer "Edge.Cuts"))
  (gr_line (start 21 60) (end 57 60)
    (layer "Edge.Cuts"))
  (gr_arc (start 58 27) (mid 58.292893 26.292893) (end 59 26)
    (layer "Edge.Cuts"))
  (gr_line (start 190 21) (end 190 124)
    (layer "Edge.Cuts"))
  (gr_line (start 113.8 20) (end 113.8 21)
    (layer "Edge.Cuts"))
  (gr_line (start 96.2 21) (end 96.2 20)
    (layer "Edge.Cuts"))
  (gr_line (start 96.2 20) (end 113.8 20)
    (layer "Edge.Cuts"))
  (gr_arc (start 189 20) (mid 189.707107 20.292893) (end 190 21)
    (layer "Edge.Cuts"))
  (gr_arc (start 96.2 21) (mid 96.082843 21.282843) (end 95.8 21.4)
    (layer "Edge.Cuts"))
  (gr_line (start 73 26) (end 59 26)
    (layer "Edge.Cuts"))
  (gr_line (start 91.8 20) (end 91.8 21)
    (layer "Edge.Cuts"))
  (gr_arc (start 20 61) (mid 20.292893 60.292893) (end 21 60)
    (layer "Edge.Cuts"))
  (gr_arc (start 74 25) (mid 73.707107 25.707107) (end 73 26)
    (layer "Edge.Cuts"))
  (gr_line (start 92.2 21.4) (end 95.8 21.4)
    (layer "Edge.Cuts"))
  (gr_arc (start 58 59) (mid 57.707107 59.707107) (end 57 60)
    (layer "Edge.Cuts"))
  (gr_line (start 91.8 20) (end 75 20)
    (layer "Edge.Cuts"))
  (gr_arc (start 190 124) (mid 189.707107 124.707107) (end 189 125)
    (layer "Edge.Cuts"))
  (gr_arc (start 118.2 21) (mid 118.082842 21.282844) (end 117.799998 21.400002)
    (layer "Edge.Cuts"))
  (gr_line (start 118.2 21) (end 118.2 20)
    (layer "Edge.Cuts"))
  (gr_text "GND" (at 55.3212 71.4756 -90) (layer "B.SilkS"))
  (gr_text "Data out" (at 52.8828 71.374 -90) (layer "B.SilkS"))
  (gr_text "IN" (at 71.9328 49.7332 90) (layer "B.SilkS"))
  (gr_text "GND" (at 189.23 36.576 90) (layer "B.SilkS"))
  (gr_text "5V PSU" (at 133.46 50.06 90) (layer "B.SilkS"))
  (gr_text "${TITLE}\n${COMPANY}\nBCB: ${REVISION}" (at 85.57 81.1) (layer "B.SilkS"))
  (gr_text "+3.3V \n150mA max" (at 49.0728 71.3232 270) (layer "B.SilkS"))
  (gr_text "MIDI" (at 65.91 51.05) (layer "B.SilkS"))
  (gr_text "in" (at 134.874 45.6692 270) (layer "B.SilkS"))
  (gr_text "LED OUT" (at 49.2252 83.566) (layer "B.SilkS"))
  (gr_text "IN" (at 182.7784 36.7792 90) (layer "B.SilkS"))
  (gr_text "OUT" (at 67.6656 51.8668 -90) (layer "B.SilkS"))
  (gr_text "VREF" (at 176.3268 36.6776 90) (layer "B.SilkS"))
  (gr_text "out" (at 137.4648 45.7708 -90) (layer "B.SilkS"))
  (gr_text "IN L" (at 164.2872 112.522) (layer "F.SilkS"))
  (gr_text "MIDI\nOUT" (at 126.3396 24.7904) (layer "F.SilkS"))
  (gr_text "${TITLE}\n${COMPANY}\nBCB: ${REVISION}" (at 49.9 75.1) (layer "F.SilkS"))
  (gr_text "IN R" (at 164.6428 91.0336) (layer "F.SilkS"))
  (gr_text "EXP" (at 171.2468 55.2196) (layer "F.SilkS"))
  (gr_text "OUT L" (at 39.7764 112.8268) (layer "F.SilkS"))
  (gr_text "OUT R" (at 39.7764 92.3544) (layer "F.SilkS"))
  (gr_text "MIDI\n IN\n" (at 80.8228 24.6888) (layer "F.SilkS"))
  (gr_text "Area for (example)\n- Swithes\n- Alternative I/O" (at 27.2 39.9) (layer "Dwgs.User"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 57 60) (xy 57 20))
    (height -3)
    (gr_text "40 mm" (at 52.85 40 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 133 23) (xy 168 23))
    (height -8.4)
    (gr_text "35.0000 mm" (at 150.5 13.45) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 58 57.5) (xy 20 57.5))
    (height 3.5)
    (gr_text "38 mm" (at 39 52.85) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 168 23) (xy 190 23))
    (height -8.4)
    (gr_text "22 mm" (at 179 13.45) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 59 26) (xy 59 20))
    (height -8)
    (gr_text "6 mm" (at 49.85 23 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 167.980001 121.505601) (xy 189.98 121.505601))
    (height 12.594399)
    (gr_text "22 mm" (at 178.980001 132.95) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 168.66 121.5) (xy 168.66 125))
    (height -24.54)
    (gr_text "3.5 mm" (at 192.05 118.4 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 58 24) (xy 74 24))
    (height -6.5)
    (gr_text "16 mm" (at 66 16.35) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 187 23) (xy 187 20))
    (height 7)
    (gr_text "3 mm" (at 196.130614 22.5 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 80 19.994385) (xy 130 19.994385))
    (height -2.494385)
    (gr_text "50 mm" (at 105 16.35) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 195.42 105.61) (xy 14.58 105.61))
    (height -34.39)
    (gr_text "180.84 mm" (at 105 138.85) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 187 20) (xy 187 125))
    (height -14.2)
    (gr_text "105 mm" (at 200.05 72.5 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 20 125) (xy 190 125))
    (height 12)
    (gr_text "170 mm" (at 105 135.85) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 77 23) (xy 133 23))
    (height -8.5)
    (gr_text "56 mm" (at 105 13.35) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 42 122.4) (xy 20 122.4))
    (height -11.6)
    (gr_text "22 mm" (at 31 132.85) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 115) (net_name "/Power Supply/power_input_gnd") (layer "F.Cu") (name "power-in-gnd") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.4))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 190 32.3)
        (xy 190 20)
        (xy 155.7664 20)
        (xy 152.2204 23.546)
        (xy 152.2204 57.200252)
        (xy 147.881331 57.196291)
        (xy 134.466508 70.345749)
        (xy 134.581699 74)
        (xy 141.860242 74)
        (xy 154.48259 61.856766)
        (xy 162.319789 61.811408)
        (xy 170.1 54.512723)
        (xy 170.1 33.8)
        (xy 190 33.8)
      )
    )
  )
  (zone (net 2) (net_name "+3.3V") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.4))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 58.005615 20)
        (xy 20 20)
        (xy 20.005615 124.994385)
        (xy 190.005615 124.994385)
        (xy 190.005615 19.994385)
        (xy 130 19.994385)
        (xy 130 36)
        (xy 80 36)
        (xy 80 19.994385)
      )
    )
  )
  (zone (net 110) (net_name "/Audio/GND_out") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads (clearance 0.4))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 20 125)
        (xy 19.955 114.54)
        (xy 19.939 72.009)
        (xy 19.5834 72.3646)
        (xy 38.700111 72.3646)
        (xy 39.7764 73.344022)
        (xy 39.7764 106.0704)
        (xy 43.127827 109.421827)
        (xy 88.313785 109.191255)
        (xy 97.522867 118.0592)
        (xy 114.628505 118.0592)
        (xy 116.07 119.38)
        (xy 123.943891 119.424509)
        (xy 131.23 111.84095)
        (xy 158.7 111.814081)
        (xy 162.49 115.6)
        (xy 162.49 125)
      )
    )
  )
  (zone (net 105) (net_name "/Audio/GND_in_R") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.4))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 156.0068 76.0984)
        (xy 149.274311 75.989511)
        (xy 149.188252 71.44284)
        (xy 152.844393 68.002)
        (xy 168.586 68.002)
        (xy 172.9168 72.3328)
        (xy 189.999845 72.3328)
        (xy 189.992 92.615)
        (xy 171.668386 92.615)
        (xy 171.660899 78.946583)
        (xy 167.813537 74.977267)
        (xy 163.957481 75.027711)
        (xy 160.886265 78.2804)
        (xy 156.84365 78.2804)
        (xy 155.922025 77.99314)
      )
    )
  )
  (zone (net 108) (net_name "/Audio/GND_in_L") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads (clearance 0.4))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 155.152834 78.662116)
        (xy 155.152834 76.14291)
        (xy 149.264348 76.122046)
        (xy 149.237034 84.521034)
        (xy 162.9132 98.1972)
        (xy 171.5 98.2226)
        (xy 171.5 113.490854)
        (xy 190.108415 113.5909)
        (xy 190 98.248)
        (xy 189.979361 93.1)
        (xy 171.201422 93.1)
        (xy 171.222453 85.898991)
        (xy 169 85.9214)
        (xy 163.907316 85.9214)
        (xy 160.925118 82.972865)
        (xy 160.951461 78.676411)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.4))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 58 20)
        (xy 20 20)
        (xy 20 125)
        (xy 190 125)
        (xy 190 20.2)
        (xy 189.8 20)
        (xy 130 20)
        (xy 130 36)
        (xy 130 36.00225)
        (xy 80 36)
        (xy 80 20)
      )
    )
  )
)
